Time to live: 64

Flag: 001

Fragment Offset: 22

TCP Segment:

Source Port: 29805 Destination Port: 27710

Sequence Number: 1163157863 Acknowledgment number: 0

TCP Header Length: 0 bytes

Window Size: 0

Flag: other

Urgent Pointer: 0

Option Field: 0

TCP Payload size: 0 bytes

TCP Payload type: other

Data: No payload

Ethernet Frame 150:

Source MAC Address: 00-C0-4F-8D-99-37 Destination MAC Address: 08-00-20-AB-D4-A4 Ether Type field: IPv4

Frame length : 60 Padding: 000000000000

IP Packet:

Source IP Address: /192.168.1.10 Destination IP Address: /192.168.1.22

IP Version: 4 Protocol Type: TCP

IP header length: 20 bytes

Total IP length: 28

Time to live: 64

Flag: 001

Fragment Offset: 7

TCP Segment:

Source Port: 12336 Destination Port: 13600

Sequence Number: 825309749 Acknowledgment number: 0

TCP Header Length: 0 bytes

Window Size: 0

Flag: other

Urgent Pointer: 0

Option Field: 0

TCP Payload size: 0 bytes

TCP Payload type: other

Data: No payload

Ethernet Frame 149:

Source MAC Address: 00-C0-4F-8D-99-37 Destination MAC Address: 08-00-20-AB-D4-A4 Ether Type field: IPv4

Frame length : 60 Padding: 000000000000

IP Packet:

Source IP Address: /192.168.1.10 Destination IP Address: /192.168.1.22

IP Version: 4 Protocol Type: TCP

IP header length: 20 bytes

Total IP length: 28

Time to live: 64

Flag: 001

Fragment Offset: 37

TCP Segment:

Source Port: 28276 Destination Port: 11604

Sequence Number: 2037409082 Acknowledgment number: 0

TCP Header Length: 0 bytes

Window Size: 0

Flag: other

Urgent Pointer: 0

Option Field: 0

TCP Payload size: 0 bytes

TCP Payload type: other

Data: No payload

Ethernet Frame 148:

Source MAC Address: 00-C0-4F-8D-99-37 Destination MAC Address: 08-00-20-AB-D4-A4 Ether Type field: IPv4

Frame length : 60 Padding: 000000000000

IP Packet:

Source IP Address: /192.168.1.10 Destination IP Address: /192.168.1.22

IP Version: 4 Protocol Type: TCP

IP header length: 20 bytes

Total IP length: 28

Time to live: 64

Flag: 001

Fragment Offset: 33

TCP Segment:

Source Port: 29800 Destination Port: 14880

Sequence Number: 909708554 Acknowledgment number: 0

TCP Header Length: 0 bytes

Window Size: 0

Flag: other

Urgent Pointer: 0

Option Field: 0

TCP Payload size: 0 bytes

TCP Payload type: other

Data: No payload

Ethernet Frame 155:

Source MAC Address: 00-C0-4F-8D-99-37 Destination MAC Address: 08-00-20-AB-D4-A4 Ether Type field: IPv4

Frame length : 60 Padding: 000000000000

IP Packet:

Source IP Address: /192.168.1.10 Destination IP Address: /192.168.1.22

IP Version: 4 Protocol Type: TCP

IP header length: 20 bytes

Total IP length: 28

Time to live: 64

Flag: 001

Fragment Offset: 5

TCP Segment:

Source Port: 25914 Destination Port: 8279

Sequence Number: 1701063712 Acknowledgment number: 0

TCP Header Length: 0 bytes

Window Size: 0

Flag: other

Urgent Pointer: 0

Option Field: 0

TCP Payload size: 0 bytes

TCP Payload type: other

Data: No payload

Ethernet Frame 154:

Source MAC Address: 00-C0-4F-8D-99-37 Destination MAC Address: 08-00-20-AB-D4-A4 Ether Type field: IPv4

Frame length : 60 Padding: 485454500000

IP Packet:

Source IP Address: /192.168.1.10 Destination IP Address: /192.168.1.22

IP Version: 4 Protocol Type: TCP

IP header length: 20 bytes

Total IP length: 44

Time to live: 64

Flag: 001

Fragment Offset: 0

TCP Segment:

Source Port: 80 Destination Port: 43999

Sequence Number: 3896578493 Acknowledgment number: 2388860686

TCP Header Length: 20 bytes

Window Size: 17520

Flag: (PSH, ACK)

Urgent Pointer: 0

Option Field: 0

TCP Payload size: 4 bytes

TCP Payload type: other

Data: 00 50 AB DF E8 41 11 BD 8E 63 1F 0E 50 18 44 70 .P...A...c..P.Dp

59 F2 00 00 48 54 54 50 00 00 Y...HTTP..

Ethernet Frame 153:

Source MAC Address: 00-C0-4F-8D-99-37 Destination MAC Address: 08-00-20-AB-D4-A4 Ether Type field: IPv4

Frame length : 60 Padding: 000000000000

IP Packet:

Source IP Address: /192.168.1.10 Destination IP Address: /192.168.1.22

IP Version: 4 Protocol Type: TCP

IP header length: 20 bytes

Total IP length: 28

Time to live: 64

Flag: 001

Fragment Offset: 24

TCP Segment:

Source Port: 13621 Destination Port: 26166

Sequence Number: 1681011254 Acknowledgment number: 0

TCP Header Length: 0 bytes

Window Size: 0

Flag: other

Urgent Pointer: 0

Option Field: 0

TCP Payload size: 0 bytes

TCP Payload type: other

Data: No payload

Ethernet Frame 152:

Source MAC Address: 00-C0-4F-8D-99-37 Destination MAC Address: 08-00-20-AB-D4-A4 Ether Type field: IPv4

Frame length : 60 Padding: 000000000000

IP Packet:

Source IP Address: /192.168.1.10 Destination IP Address: /192.168.1.22

IP Version: 4 Protocol Type: TCP

IP header length: 20 bytes

Total IP length: 28

Time to live: 64

Flag: 001

Fragment Offset: 3

TCP Segment:

Source Port: 12081 Destination Port: 11825

Sequence Number: 540160048 Acknowledgment number: 0

TCP Header Length: 0 bytes

Window Size: 0

Flag: other

Urgent Pointer: 0

Option Field: 0

TCP Payload size: 0 bytes

TCP Payload type: other

Data: No payload

Ethernet Frame 151:

Source MAC Address: 00-C0-4F-8D-99-37 Destination MAC Address: 08-00-20-AB-D4-A4 Ether Type field: IPv4

Frame length : 60 Padding: 000000000000

IP Packet:

Source IP Address: /192.168.1.10 Destination IP Address: /192.168.1.22

IP Version: 4 Protocol Type: TCP

IP header length: 20 bytes

Total IP length: 28

Time to live: 64

Flag: 001

Fragment Offset: 6

TCP Segment:

Source Port: 12601 Destination Port: 8266

Sequence Number: 1634607154 Acknowledgment number: 0

TCP Header Length: 0 bytes

Window Size: 0

Flag: other

Urgent Pointer: 0

Option Field: 0

TCP Payload size: 0 bytes

TCP Payload type: other

Data: No payload

Ethernet Frame 158:

Source MAC Address: 00-C0-4F-8D-99-37 Destination MAC Address: 08-00-20-AB-D4-A4 Ether Type field: IPv4

Frame length : 60 Padding: 000000000000

IP Packet:

Source IP Address: /192.168.1.10 Destination IP Address: /192.168.1.22

IP Version: 4 Protocol Type: TCP

IP header length: 20 bytes

Total IP length: 28

Time to live: 64

Flag: 001

Fragment Offset: 13

TCP Segment:

Source Port: 26469 Destination Port: 29498

Sequence Number: 1936469810 Acknowledgment number: 0

TCP Header Length: 0 bytes

Window Size: 0

Flag: other

Urgent Pointer: 0

Option Field: 0

TCP Payload size: 0 bytes

TCP Payload type: other

Data: No payload

Ethernet Frame 158:

Source MAC Address: 00-C0-4F-8D-99-37 Destination MAC Address: 08-00-20-AB-D4-A4 Ether Type field: IPv4

Frame length : 60 Padding: 000000000000

IP Packet:

Source IP Address: /192.168.1.10 Destination IP Address: /192.168.1.22

IP Version: 4 Protocol Type: TCP

IP header length: 20 bytes

Total IP length: 28

Time to live: 64

Flag: 001

Fragment Offset: 30

TCP Segment:

Source Port: 26469 Destination Port: 29498

Sequence Number: 543324532 Acknowledgment number: 0

TCP Header Length: 0 bytes

Window Size: 0

Flag: other

Urgent Pointer: 0

Option Field: 0

TCP Payload size: 0 bytes

TCP Payload type: other

Data: No payload

Ethernet Frame 157:

Source MAC Address: 00-C0-4F-8D-99-37 Destination MAC Address: 08-00-20-AB-D4-A4 Ether Type field: IPv4

Frame length : 60 Padding: 000000000000

IP Packet:

Source IP Address: /192.168.1.10 Destination IP Address: /192.168.1.22

IP Version: 4 Protocol Type: TCP

IP header length: 20 bytes

Total IP length: 28

Time to live: 64

Flag: 001

Fragment Offset: 18

TCP Segment:

Source Port: 26981 Destination Port: 25658

Sequence Number: 542598500 Acknowledgment number: 0

TCP Header Length: 0 bytes

Window Size: 0

Flag: other

Urgent Pointer: 0

Option Field: 0

TCP Payload size: 0 bytes

TCP Payload type: other

Data: No payload

Ethernet Frame 156:

Source MAC Address: 00-C0-4F-8D-99-37 Destination MAC Address: 08-00-20-AB-D4-A4 Ether Type field: IPv4

Frame length : 60 Padding: 000000000000

IP Packet:

Source IP Address: /192.168.1.10 Destination IP Address: /192.168.1.22

IP Version: 4 Protocol Type: TCP

IP header length: 20 bytes

Total IP length: 28

Time to live: 64

Flag: 001

Fragment Offset: 15

TCP Segment:

Source Port: 25966 Destination Port: 21331

Sequence Number: 1278160942 Acknowledgment number: 0

TCP Header Length: 0 bytes

Window Size: 0

Flag: other

Urgent Pointer: 0

Option Field: 0

TCP Payload size: 0 bytes

TCP Payload type: other

Data: No payload

Ethernet Frame 165:

Source MAC Address: 00-C0-4F-8D-99-37 Destination MAC Address: 08-00-20-AB-D4-A4 Ether Type field: IPv4

Frame length : 60 Padding: 000000000000

IP Packet:

Source IP Address: /192.168.1.10 Destination IP Address: /192.168.1.22

IP Version: 4 Protocol Type: TCP

IP header length: 20 bytes

Total IP length: 28

Time to live: 64

Flag: 001

Fragment Offset: 42

TCP Segment:

Source Port: 17263 Destination Port: 28263

Sequence Number: 1918989427 Acknowledgment number: 0

TCP Header Length: 0 bytes

Window Size: 0

Flag: other

Urgent Pointer: 0

Option Field: 0

TCP Payload size: 0 bytes

TCP Payload type: other

Data: No payload

Ethernet Frame 164:

Source MAC Address: 00-C0-4F-8D-99-37 Destination MAC Address: 08-00-20-AB-D4-A4 Ether Type field: IPv4

Frame length : 60 Padding: 000000000000

IP Packet:

Source IP Address: /192.168.1.10 Destination IP Address: /192.168.1.22

IP Version: 4 Protocol Type: TCP

IP header length: 20 bytes

Total IP length: 28

Time to live: 64

Flag: 001

Fragment Offset: 10

TCP Segment:

Source Port: 14880 Destination Port: 16752

Sequence Number: 1633904741 Acknowledgment number: 0

TCP Header Length: 0 bytes

Window Size: 0

Flag: other

Urgent Pointer: 0

Option Field: 0

TCP Payload size: 0 bytes

TCP Payload type: other

Data: No payload

Ethernet Frame 163:

Source MAC Address: 00-C0-4F-8D-99-37 Destination MAC Address: 08-00-20-AB-D4-A4 Ether Type field: IPv4

Frame length : 60 Padding: 000000000000

IP Packet:

Source IP Address: /192.168.1.10 Destination IP Address: /192.168.1.22

IP Version: 4 Protocol Type: TCP

IP header length: 20 bytes

Total IP length: 28

Time to live: 64

Flag: 001

Fragment Offset: 45

TCP Segment:

Source Port: 30066 Destination Port: 8311

Sequence Number: 1700929648 Acknowledgment number: 0

TCP Header Length: 0 bytes

Window Size: 0

Flag: other

Urgent Pointer: 0

Option Field: 0

TCP Payload size: 0 bytes

TCP Payload type: other

Data: No payload

Ethernet Frame 162:

Source MAC Address: 00-C0-4F-8D-99-37 Destination MAC Address: 08-00-20-AB-D4-A4 Ether Type field: IPv4

Frame length : 60 Padding: 000000000000

IP Packet:

Source IP Address: /192.168.1.10 Destination IP Address: /192.168.1.22

IP Version: 4 Protocol Type: TCP

IP header length: 20 bytes

Total IP length: 28

Time to live: 64

Flag: 001

Fragment Offset: 11

TCP Segment:

Source Port: 30066 Destination Port: 8311

Sequence Number: 775043360 Acknowledgment number: 0

TCP Header Length: 0 bytes

Window Size: 0

Flag: other

Urgent Pointer: 0

Option Field: 0

TCP Payload size: 0 bytes

TCP Payload type: other

Data: No payload

Ethernet Frame 161:

Source MAC Address: 00-C0-4F-8D-99-37 Destination MAC Address: 08-00-20-AB-D4-A4 Ether Type field: IPv4

Frame length : 60 Padding: 000000000000

IP Packet:

Source IP Address: /192.168.1.10 Destination IP Address: /192.168.1.22

IP Version: 4 Protocol Type: TCP

IP header length: 20 bytes

Total IP length: 28

Time to live: 64

Flag: 001

Fragment Offset: 34

TCP Segment:

Source Port: 17263 Destination Port: 11827

Sequence Number: 1701016681 Acknowledgment number: 0

TCP Header Length: 0 bytes

Window Size: 0

Flag: other

Urgent Pointer: 0

Option Field: 0

TCP Payload size: 0 bytes

TCP Payload type: other

Data: No payload

Ethernet Frame 160:

Source MAC Address: 00-C0-4F-8D-99-37 Destination MAC Address: 08-00-20-AB-D4-A4 Ether Type field: IPv4

Frame length : 60 Padding: 000000000000

IP Packet:

Source IP Address: /192.168.1.10 Destination IP Address: /192.168.1.22

IP Version: 4 Protocol Type: TCP

IP header length: 20 bytes

Total IP length: 28

Time to live: 64

Flag: 001

Fragment Offset: 9

TCP Segment:

Source Port: 17263 Destination Port: 28270

Sequence Number: 1920361842 Acknowledgment number: 0

TCP Header Length: 0 bytes

Window Size: 0

Flag: other

Urgent Pointer: 0

Option Field: 0

TCP Payload size: 0 bytes

TCP Payload type: other

Data: No payload

Ethernet Frame 159:

Source MAC Address: 00-C0-4F-8D-99-37 Destination MAC Address: 08-00-20-AB-D4-A4 Ether Type field: IPv4

Frame length : 60 Padding: 000000000000

IP Packet:

Source IP Address: /192.168.1.10 Destination IP Address: /192.168.1.22

IP Version: 4 Protocol Type: TCP

IP header length: 20 bytes

Total IP length: 28

Time to live: 64

Flag: 001

Fragment Offset: 44

TCP Segment:

Source Port: 3338 Destination Port: 21349

Sequence Number: 1852055663 Acknowledgment number: 0

TCP Header Length: 0 bytes

Window Size: 0

Flag: other

Urgent Pointer: 0

Option Field: 0

TCP Payload size: 0 bytes

TCP Payload type: other

Data: No payload

Ethernet Frame 168:

Source MAC Address: 00-C0-4F-8D-99-37 Destination MAC Address: 08-00-20-AB-D4-A4 Ether Type field: IPv4

Frame length : 60 Padding: 000000000000

IP Packet:

Source IP Address: /192.168.1.10 Destination IP Address: /192.168.1.22

IP Version: 4 Protocol Type: TCP

IP header length: 20 bytes

Total IP length: 28

Time to live: 64

Flag: 001

Fragment Offset: 46

TCP Segment:

Source Port: 24935 Destination Port: 25889

Sequence Number: 1009738351 Acknowledgment number: 0

TCP Header Length: 0 bytes

Window Size: 0

Flag: other

Urgent Pointer: 0

Option Field: 0

TCP Payload size: 0 bytes

TCP Payload type: other

Data: No payload

Ethernet Frame 166:

Source MAC Address: 00-C0-4F-8D-99-37 Destination MAC Address: 08-00-20-AB-D4-A4 Ether Type field: IPv4

Frame length : 60 Padding: 000000000000

IP Packet:

Source IP Address: /192.168.1.10 Destination IP Address: /192.168.1.22

IP Version: 4 Protocol Type: TCP

IP header length: 20 bytes

Total IP length: 28

Time to live: 64

Flag: 001

Fragment Offset: 14

TCP Segment:

Source Port: 24935 Destination Port: 25889

Sequence Number: 908087152 Acknowledgment number: 0

TCP Header Length: 0 bytes

Window Size: 0

Flag: other

Urgent Pointer: 0

Option Field: 0

TCP Payload size: 0 bytes

TCP Payload type: other

Data: No payload

Ethernet Frame 169:

Source MAC Address: 00-C0-4F-8D-99-37 Destination MAC Address: 08-00-20-AB-D4-A4 Ether Type field: IPv4

Frame length : 60 Padding: 000000000000

IP Packet:

Source IP Address: /192.168.1.10 Destination IP Address: /192.168.1.22

IP Version: 4 Protocol Type: TCP

IP header length: 20 bytes

Total IP length: 28

Time to live: 64

Flag: 001

Fragment Offset: 25

TCP Segment:

Source Port: 13880 Destination Port: 25142

Sequence Number: 945972279 Acknowledgment number: 0

TCP Header Length: 0 bytes

Window Size: 0

Flag: other

Urgent Pointer: 0

Option Field: 0

TCP Payload size: 0 bytes

TCP Payload type: other

Data: No payload

Ethernet Frame 167:

Source MAC Address: 00-C0-4F-8D-99-37 Destination MAC Address: 08-00-20-AB-D4-A4 Ether Type field: IPv4

Frame length : 60 Padding: 000000000000

IP Packet:

Source IP Address: /192.168.1.10 Destination IP Address: /192.168.1.22

IP Version: 4 Protocol Type: TCP

IP header length: 20 bytes

Total IP length: 28

Time to live: 64

Flag: 001

Fragment Offset: 21

TCP Segment:

Source Port: 24935 Destination Port: 25889

Sequence Number: 875831367 Acknowledgment number: 0

TCP Header Length: 0 bytes

Window Size: 0

Flag: other

Urgent Pointer: 0

Option Field: 0

TCP Payload size: 0 bytes

TCP Payload type: other

Data: No payload

Ethernet Frame 171:

Source MAC Address: 00-C0-4F-8D-99-37 Destination MAC Address: 08-00-20-AB-D4-A4 Ether Type field: IPv4

Frame length : 60 Padding: 000000000000

IP Packet:

Source IP Address: /192.168.1.10 Destination IP Address: /192.168.1.22

IP Version: 4 Protocol Type: TCP

IP header length: 20 bytes

Total IP length: 28

Time to live: 64

Flag: 001

Fragment Offset: 12

TCP Segment:

Source Port: 10325 Destination Port: 28265

Sequence Number: 2015961197 Acknowledgment number: 0

TCP Header Length: 0 bytes

Window Size: 0

Flag: other

Urgent Pointer: 0

Option Field: 0

TCP Payload size: 0 bytes

TCP Payload type: other

Data: No payload

Ethernet Frame 173:

Source MAC Address: 00-C0-4F-8D-99-37 Destination MAC Address: 08-00-20-AB-D4-A4 Ether Type field: IPv4

Frame length : 60 Padding: 000000000000

IP Packet:

Source IP Address: /192.168.1.10 Destination IP Address: /192.168.1.22

IP Version: 4 Protocol Type: TCP

IP header length: 20 bytes

Total IP length: 28

Time to live: 64

Flag: 001

Fragment Offset: 36

TCP Segment:

Source Port: 25869 Destination Port: 2627

Sequence Number: 1869509733 Acknowledgment number: 0

TCP Header Length: 0 bytes

Window Size: 0

Flag: other

Urgent Pointer: 0

Option Field: 0

TCP Payload size: 0 bytes

TCP Payload type: other

Data: No payload

Ethernet Frame 170:

Source MAC Address: 00-C0-4F-8D-99-37 Destination MAC Address: 08-00-20-AB-D4-A4 Ether Type field: IPv4

Frame length : 60 Padding: 000000000000

IP Packet:

Source IP Address: /192.168.1.10 Destination IP Address: /192.168.1.22

IP Version: 4 Protocol Type: TCP

IP header length: 20 bytes

Total IP length: 28

Time to live: 64

Flag: 001

Fragment Offset: 23

TCP Segment:

Source Port: 26212 Destination Port: 12345

Sequence Number: 808794420 Acknowledgment number: 0

TCP Header Length: 0 bytes

Window Size: 0

Flag: other

Urgent Pointer: 0

Option Field: 0

TCP Payload size: 0 bytes

TCP Payload type: other

Data: No payload

Ethernet Frame 172:

Source MAC Address: 00-C0-4F-8D-99-37 Destination MAC Address: 08-00-20-AB-D4-A4 Ether Type field: IPv4

Frame length : 60 Padding: 000000000000

IP Packet:

Source IP Address: /192.168.1.10 Destination IP Address: /192.168.1.22

IP Version: 4 Protocol Type: TCP

IP header length: 20 bytes

Total IP length: 28

Time to live: 64

Flag: 001

Fragment Offset: 27

TCP Segment:

Source Port: 26212 Destination Port: 2627

Sequence Number: 926442806 Acknowledgment number: 0

TCP Header Length: 0 bytes

Window Size: 0

Flag: other

Urgent Pointer: 0

Option Field: 0

TCP Payload size: 0 bytes

TCP Payload type: other

Data: No payload

Ethernet Frame 177:

Source MAC Address: 00-C0-4F-8D-99-37 Destination MAC Address: 08-00-20-AB-D4-A4 Ether Type field: IPv4

Frame length : 60 Padding: 000000000000

IP Packet:

Source IP Address: /192.168.1.10 Destination IP Address: /192.168.1.22

IP Version: 4 Protocol Type: TCP

IP header length: 20 bytes

Total IP length: 28

Time to live: 64

Flag: 001

Fragment Offset: 43

TCP Segment:

Source Port: 11296 Destination Port: 31087

Sequence Number: 1965520485 Acknowledgment number: 0

TCP Header Length: 0 bytes

Window Size: 0

Flag: other

Urgent Pointer: 0

Option Field: 0

TCP Payload size: 0 bytes

TCP Payload type: other

Data: No payload

Ethernet Frame 175:

Source MAC Address: 00-C0-4F-8D-99-37 Destination MAC Address: 08-00-20-AB-D4-A4 Ether Type field: IPv4

Frame length : 60 Padding: 000000000000

IP Packet:

Source IP Address: /192.168.1.10 Destination IP Address: /192.168.1.22

IP Version: 4 Protocol Type: TCP

IP header length: 20 bytes

Total IP length: 28

Time to live: 64

Flag: 001

Fragment Offset: 4

TCP Segment:

Source Port: 8271 Destination Port: 19213

Sequence Number: 172253556 Acknowledgment number: 0

TCP Header Length: 0 bytes

Window Size: 0

Flag: other

Urgent Pointer: 0

Option Field: 0

TCP Payload size: 0 bytes

TCP Payload type: other

Data: No payload

Ethernet Frame 176:

Source MAC Address: 00-C0-4F-8D-99-37 Destination MAC Address: 08-00-20-AB-D4-A4 Ether Type field: IPv4

Frame length : 60 Padding: 000000000000

IP Packet:

Source IP Address: /192.168.1.10 Destination IP Address: /192.168.1.22

IP Version: 4 Protocol Type: TCP

IP header length: 20 bytes

Total IP length: 23

Time to live: 64

Flag: 000

Fragment Offset: 48

TCP Segment:

Source Port: 27710 Destination Port: 2560

Sequence Number: 0 Acknowledgment number: 0

TCP Header Length: 0 bytes

Window Size: 0

Flag: other

Urgent Pointer: 0

Option Field: 0

TCP Payload size: 0 bytes

TCP Payload type: other

Data: No payload

Ethernet Frame 174:

Source MAC Address: 00-C0-4F-8D-99-37 Destination MAC Address: 08-00-20-AB-D4-A4 Ether Type field: IPv4

Frame length : 60 Padding: 000000000000

IP Packet:

Source IP Address: /192.168.1.10 Destination IP Address: /192.168.1.22

IP Version: 4 Protocol Type: TCP

IP header length: 20 bytes

Total IP length: 28

Time to live: 64

Flag: 001

Fragment Offset: 16

TCP Segment:

Source Port: 14638 Destination Port: 14179

Sequence Number: 218778721 Acknowledgment number: 0

TCP Header Length: 0 bytes

Window Size: 0

Flag: other

Urgent Pointer: 0

Option Field: 0

TCP Payload size: 0 bytes

TCP Payload type: other

Data: No payload

Ethernet Frame 178:

Source MAC Address: 00-C0-4F-8D-99-37 Destination MAC Address: 08-00-20-AB-D4-A4 Ether Type field: IPv4

Frame length : 60 Padding: 000000000000

IP Packet:

Source IP Address: /192.168.1.10 Destination IP Address: /192.168.1.22

IP Version: 4 Protocol Type: TCP

IP header length: 20 bytes

Total IP length: 28

Time to live: 64

Flag: 001

Fragment Offset: 32

TCP Segment:

Source Port: 25966 Destination Port: 29741

Sequence Number: 1281715815 Acknowledgment number: 0

TCP Header Length: 0 bytes

Window Size: 0

Flag: other

Urgent Pointer: 0

Option Field: 0

TCP Payload size: 0 bytes

TCP Payload type: other

Data: No payload

Ethernet Frame 179:

Source MAC Address: 00-C0-4F-8D-99-37 Destination MAC Address: 08-00-20-AB-D4-A4 Ether Type field: IPv4

Frame length : 60 Padding: 000000000000

IP Packet:

Source IP Address: /192.168.1.10 Destination IP Address: /192.168.1.22

IP Version: 4 Protocol Type: TCP

IP header length: 20 bytes

Total IP length: 28

Time to live: 64

Flag: 001

Fragment Offset: 19

TCP Segment:

Source Port: 11296 Destination Port: 12855

Sequence Number: 542073716 Acknowledgment number: 0

TCP Header Length: 0 bytes

Window Size: 0

Flag: other

Urgent Pointer: 0

Option Field: 0

TCP Payload size: 0 bytes

TCP Payload type: other

Data: No payload

Ethernet Frame 180:

Source MAC Address: 00-C0-4F-8D-99-37 Destination MAC Address: 08-00-20-AB-D4-A4 Ether Type field: IPv4

Frame length : 60 Padding: 000000000000

IP Packet:

Source IP Address: /192.168.1.10 Destination IP Address: /192.168.1.22

IP Version: 4 Protocol Type: TCP

IP header length: 20 bytes

Total IP length: 28

Time to live: 64

Flag: 001

Fragment Offset: 28

TCP Segment:

Source Port: 25400 Destination Port: 15976

Sequence Number: 218775907 Acknowledgment number: 0

TCP Header Length: 0 bytes

Window Size: 0

Flag: other

Urgent Pointer: 0

Option Field: 0

TCP Payload size: 0 bytes

TCP Payload type: other

Data: No payload

Ethernet Frame 180:

Source MAC Address: 00-C0-4F-8D-99-37 Destination MAC Address: 08-00-20-AB-D4-A4 Ether Type field: IPv4

Frame length : 60 Padding: 000000000000

IP Packet:

Source IP Address: /192.168.1.10 Destination IP Address: /192.168.1.22

IP Version: 4 Protocol Type: TCP

IP header length: 20 bytes

Total IP length: 28

Time to live: 64

Flag: 001

Fragment Offset: 41

TCP Segment:

Source Port: 25400 Destination Port: 15976

Sequence Number: 1702439968 Acknowledgment number: 0

TCP Header Length: 0 bytes

Window Size: 0

Flag: other

Urgent Pointer: 0

Option Field: 0

TCP Payload size: 0 bytes

TCP Payload type: other

Data: No payload

Ethernet Frame 184:

Source MAC Address: 00-C0-4F-8D-99-37 Destination MAC Address: 08-00-20-AB-D4-A4 Ether Type field: IPv4

Frame length : 60 Padding: 000000000000

IP Packet:

Source IP Address: /192.168.1.10 Destination IP Address: /192.168.1.22

IP Version: 4 Protocol Type: TCP

IP header length: 20 bytes

Total IP length: 28

Time to live: 64

Flag: 001

Fragment Offset: 29

TCP Segment:

Source Port: 25445 Destination Port: 28788

Sequence Number: 760373614 Acknowledgment number: 0

TCP Header Length: 0 bytes

Window Size: 0

Flag: other

Urgent Pointer: 0

Option Field: 0

TCP Payload size: 0 bytes

TCP Payload type: other

Data: No payload

Ethernet Frame 183:

Source MAC Address: 00-C0-4F-8D-99-37 Destination MAC Address: 08-00-20-AB-D4-A4 Ether Type field: IPv4

Frame length : 60 Padding: 000000000000

IP Packet:

Source IP Address: /192.168.1.10 Destination IP Address: /192.168.1.22

IP Version: 4 Protocol Type: TCP

IP header length: 20 bytes

Total IP length: 28

Time to live: 64

Flag: 001

Fragment Offset: 35

TCP Segment:

Source Port: 13107 Destination Port: 13624

Sequence Number: 1668050803 Acknowledgment number: 0

TCP Header Length: 0 bytes

Window Size: 0

Flag: other

Urgent Pointer: 0

Option Field: 0

TCP Payload size: 0 bytes

TCP Payload type: other

Data: No payload

Ethernet Frame 182:

Source MAC Address: 00-C0-4F-8D-99-37 Destination MAC Address: 08-00-20-AB-D4-A4 Ether Type field: IPv4

Frame length : 60 Padding: 000000000000

IP Packet:

Source IP Address: /192.168.1.10 Destination IP Address: /192.168.1.22

IP Version: 4 Protocol Type: TCP

IP header length: 20 bytes

Total IP length: 28

Time to live: 64

Flag: 001

Fragment Offset: 26

TCP Segment:

Source Port: 13107 Destination Port: 13624

Sequence Number: 962998629 Acknowledgment number: 0

TCP Header Length: 0 bytes

Window Size: 0

Flag: other

Urgent Pointer: 0

Option Field: 0

TCP Payload size: 0 bytes

TCP Payload type: other

Data: No payload

Ethernet Frame 181:

Source MAC Address: 00-C0-4F-8D-99-37 Destination MAC Address: 08-00-20-AB-D4-A4 Ether Type field: IPv4

Frame length : 60 Padding: 000000000000

IP Packet:

Source IP Address: /192.168.1.10 Destination IP Address: /192.168.1.22

IP Version: 4 Protocol Type: TCP

IP header length: 20 bytes

Total IP length: 28

Time to live: 64

Flag: 001

Fragment Offset: 8

TCP Segment:

Source Port: 13107 Destination Port: 13624

Sequence Number: 541543764 Acknowledgment number: 0

TCP Header Length: 0 bytes

Window Size: 0

Flag: other

Urgent Pointer: 0

Option Field: 0

TCP Payload size: 0 bytes

TCP Payload type: other

Data: No payload

Ethernet Frame 185:

Source MAC Address: 00-C0-4F-8D-99-37 Destination MAC Address: 08-00-20-AB-D4-A4 Ether Type field: IPv4

Frame length : 60 Padding: 000000000000

IP Packet:

Source IP Address: /192.168.1.10 Destination IP Address: /192.168.1.22

IP Version: 4 Protocol Type: TCP

IP header length: 20 bytes

Total IP length: 40

Time to live: 64

Flag: 010

Fragment Offset: 0

TCP Segment:

Source Port: 80 Destination Port: 43999

Sequence Number: 3896578860 Acknowledgment number: 2388860686

TCP Header Length: 20 bytes

Window Size: 17520

Flag: (FIN, ACK)

Urgent Pointer: 0

Option Field: 0

TCP Payload size: 0 bytes

TCP Payload type: other

Data: No payload

Ethernet Frame 186:

Source MAC Address: 00-C0-4F-8D-99-37 Destination MAC Address: 08-00-20-AB-D4-A4 Ether Type field: IPv4

Frame length : 60 Padding: 000000000000

IP Packet:

Source IP Address: /192.168.1.10 Destination IP Address: /192.168.1.22

IP Version: 4 Protocol Type: TCP

IP header length: 20 bytes

Total IP length: 40

Time to live: 64

Flag: 010

Fragment Offset: 0

TCP Segment:

Source Port: 80 Destination Port: 43999

Sequence Number: 3896578861 Acknowledgment number: 2388860687

TCP Header Length: 20 bytes

Window Size: 17520

Flag: ACK

Urgent Pointer: 0

Option Field: 0

TCP Payload size: 0 bytes

TCP Payload type: other

Data: No payload

Ethernet Frame 187:

Source MAC Address: 08-00-20-AB-D4-A4 Destination MAC Address: 00-C0-4F-8D-99-37 Ether Type field: IPv4

Frame length : 60 Padding: 000000000000

IP Packet:

Source IP Address: /192.168.1.22 Destination IP Address: /192.168.1.10

IP Version: 4 Protocol Type: TCP

IP header length: 20 bytes

Total IP length: 40

Time to live: 64

Flag: 010

Fragment Offset: 0

TCP Segment:

Source Port: 43999 Destination Port: 80

Sequence Number: 2388860686 Acknowledgment number: 3896578860

TCP Header Length: 20 bytes

Window Size: 49273

Flag: ACK

Urgent Pointer: 0

Option Field: 0

TCP Payload size: 0 bytes

TCP Payload type: other

Data: No payload

Ethernet Frame 188:

Source MAC Address: 08-00-20-AB-D4-A4 Destination MAC Address: 00-C0-4F-8D-99-37 Ether Type field: IPv4

Frame length : 60 Padding: 000000000000

IP Packet:

Source IP Address: /192.168.1.22 Destination IP Address: /192.168.1.10

IP Version: 4 Protocol Type: TCP

IP header length: 20 bytes

Total IP length: 40

Time to live: 64

Flag: 010

Fragment Offset: 0

TCP Segment:

Source Port: 43999 Destination Port: 80

Sequence Number: 2388860686 Acknowledgment number: 3896578861

TCP Header Length: 20 bytes

Window Size: 49273

Flag: ACK

Urgent Pointer: 0

Option Field: 0

TCP Payload size: 0 bytes

TCP Payload type: other

Data: No payload

Ethernet Frame 189:

Source MAC Address: 08-00-20-AB-D4-A4 Destination MAC Address: 00-C0-4F-8D-99-37 Ether Type field: IPv4

Frame length : 60 Padding: 000000000000

IP Packet:

Source IP Address: /192.168.1.22 Destination IP Address: /192.168.1.10

IP Version: 4 Protocol Type: TCP

IP header length: 20 bytes

Total IP length: 40

Time to live: 64

Flag: 010

Fragment Offset: 0

TCP Segment:

Source Port: 43999 Destination Port: 80

Sequence Number: 2388860686 Acknowledgment number: 3896578861

TCP Header Length: 20 bytes

Window Size: 49273

Flag: (FIN, ACK)

Urgent Pointer: 0

Option Field: 0

TCP Payload size: 0 bytes

TCP Payload type: other

Data: No payload

Ethernet Frame 190:

Source MAC Address: 00-60-97-B9-58-7D Destination MAC Address: 00-C0-4F-49-D8-25 Ether Type field: IPv4

Frame length : 74 Padding:

IP Packet:

Source IP Address: /192.168.1.62 Destination IP Address: /192.168.1.42

IP Version: 4 Protocol Type: TCP

IP header length: 20 bytes

Total IP length: 60

Time to live: 64

Flag: 000

Fragment Offset: 0

TCP Segment:

Source Port: 4938 Destination Port: 21

Sequence Number: 708153373 Acknowledgment number: 0

TCP Header Length: 40 bytes

Window Size: 5840

Flag: SYN

Urgent Pointer: 0

Option Field: 20

TCP Payload size: 0 bytes

TCP Payload type: FTP

Data: No payload

Ethernet Frame 191:

Source MAC Address: 00-60-97-B9-58-7D Destination MAC Address: 00-C0-4F-49-D8-25 Ether Type field: IPv4

Frame length : 66 Padding:

IP Packet:

Source IP Address: /192.168.1.62 Destination IP Address: /192.168.1.42

IP Version: 4 Protocol Type: TCP

IP header length: 20 bytes

Total IP length: 52

Time to live: 64

Flag: 000

Fragment Offset: 0

TCP Segment:

Source Port: 4938 Destination Port: 21

Sequence Number: 708153374 Acknowledgment number: 4221341147

TCP Header Length: 32 bytes

Window Size: 5840

Flag: ACK

Urgent Pointer: 0

Option Field: 12

TCP Payload size: 0 bytes

TCP Payload type: FTP

Data: No payload

Ethernet Frame 192:

Source MAC Address: 00-C0-4F-49-D8-25 Destination MAC Address: 00-60-97-B9-58-7D Ether Type field: IPv4

Frame length : 74 Padding:

IP Packet:

Source IP Address: /192.168.1.42 Destination IP Address: /192.168.1.62

IP Version: 4 Protocol Type: TCP

IP header length: 20 bytes

Total IP length: 60

Time to live: 64

Flag: 000

Fragment Offset: 0

TCP Segment:

Source Port: 21 Destination Port: 4938

Sequence Number: 4221341146 Acknowledgment number: 708153374

TCP Header Length: 40 bytes

Window Size: 5792

Flag: (SYN, ACK)

Urgent Pointer: 0

Option Field: 20

TCP Payload size: 0 bytes

TCP Payload type: FTP

Data: No payload

Ethernet Frame 193:

Source MAC Address: 00-C0-4F-49-D8-25 Destination MAC Address: 00-60-97-B9-58-7D Ether Type field: IPv4

Frame length : 60 Padding: 000000000000

IP Packet:

Source IP Address: /192.168.1.42 Destination IP Address: /192.168.1.62

IP Version: 4 Protocol Type: TCP

IP header length: 20 bytes

Total IP length: 28

Time to live: 64

Flag: 001

Fragment Offset: 21

TCP Segment:

Source Port: 8272 Destination Port: 21838

Sequence Number: 1230194757 Acknowledgment number: 0

TCP Header Length: 0 bytes

Window Size: 0

Flag: other

Urgent Pointer: 0

Option Field: 0

TCP Payload size: 0 bytes

TCP Payload type: other

Data: No payload

Ethernet Frame 194:

Source MAC Address: 00-60-97-B9-58-7D Destination MAC Address: 00-C0-4F-49-D8-25 Ether Type field: IPv4

Frame length : 66 Padding:

IP Packet:

Source IP Address: /192.168.1.62 Destination IP Address: /192.168.1.42

IP Version: 4 Protocol Type: TCP

IP header length: 20 bytes

Total IP length: 52

Time to live: 64

Flag: 000

Fragment Offset: 0

TCP Segment:

Source Port: 20037 Destination Port: 8265

Sequence Number: 708153374 Acknowledgment number: 4221341308

TCP Header Length: 32 bytes

Window Size: 5840

Flag: ACK

Urgent Pointer: 0

Option Field: 12

TCP Payload size: 0 bytes

TCP Payload type: FTP

Data: No payload

Ethernet Frame 195:

Source MAC Address: 00-C0-4F-49-D8-25 Destination MAC Address: 00-60-97-B9-58-7D Ether Type field: IPv4

Frame length : 60 Padding: 000000000000

IP Packet:

Source IP Address: /192.168.1.42 Destination IP Address: /192.168.1.62

IP Version: 4 Protocol Type: TCP

IP header length: 20 bytes

Total IP length: 28

Time to live: 64

Flag: 001

Fragment Offset: 5

TCP Segment:

Source Port: 20037 Destination Port: 8265

Sequence Number: 1394622796 Acknowledgment number: 0

TCP Header Length: 0 bytes

Window Size: 0

Flag: other

Urgent Pointer: 0

Option Field: 0

TCP Payload size: 0 bytes

TCP Payload type: other

Data: No payload

Ethernet Frame 197:

Source MAC Address: 00-C0-4F-49-D8-25 Destination MAC Address: 00-60-97-B9-58-7D Ether Type field: IPv4

Frame length : 60 Padding: 000000000000

IP Packet:

Source IP Address: /192.168.1.42 Destination IP Address: /192.168.1.62

IP Version: 4 Protocol Type: TCP

IP header length: 20 bytes

Total IP length: 28

Time to live: 64

Flag: 001

Fragment Offset: 20

TCP Segment:

Source Port: 8264 Destination Port: 16722

Sequence Number: 1397247065 Acknowledgment number: 0

TCP Header Length: 0 bytes

Window Size: 0

Flag: other

Urgent Pointer: 0

Option Field: 0

TCP Payload size: 0 bytes

TCP Payload type: other

Data: No payload

Ethernet Frame 198:

Source MAC Address: 00-C0-4F-49-D8-25 Destination MAC Address: 00-60-97-B9-58-7D Ether Type field: IPv4

Frame length : 60 Padding: 000000000000

IP Packet:

Source IP Address: /192.168.1.42 Destination IP Address: /192.168.1.62

IP Version: 4 Protocol Type: TCP

IP header length: 20 bytes

Total IP length: 28

Time to live: 64

Flag: 001

Fragment Offset: 15

TCP Segment:

Source Port: 19535 Destination Port: 18002

Sequence Number: 1330454600 Acknowledgment number: 0

TCP Header Length: 0 bytes

Window Size: 0

Flag: other

Urgent Pointer: 0

Option Field: 0

TCP Payload size: 0 bytes

TCP Payload type: other

Data: No payload

Ethernet Frame 199:

Source MAC Address: 00-C0-4F-49-D8-25 Destination MAC Address: 00-60-97-B9-58-7D Ether Type field: IPv4

Frame length : 60 Padding: 000000000000

IP Packet:

Source IP Address: /192.168.1.42 Destination IP Address: /192.168.1.62

IP Version: 4 Protocol Type: TCP

IP header length: 20 bytes

Total IP length: 28

Time to live: 64

Flag: 001

Fragment Offset: 6

TCP Segment:

Source Port: 19535 Destination Port: 18002

Sequence Number: 1142969423 Acknowledgment number: 0

TCP Header Length: 0 bytes

Window Size: 0

Flag: other

Urgent Pointer: 0

Option Field: 0

TCP Payload size: 0 bytes

TCP Payload type: other

Data: No payload

Ethernet Frame 196:

Source MAC Address: 00-C0-4F-49-D8-25 Destination MAC Address: 00-60-97-B9-58-7D Ether Type field: IPv4

Frame length : 60 Padding: 000000000000

IP Packet:

Source IP Address: /192.168.1.42 Destination IP Address: /192.168.1.62

IP Version: 4 Protocol Type: TCP

IP header length: 20 bytes

Total IP length: 28

Time to live: 64

Flag: 001

Fragment Offset: 12

TCP Segment:

Source Port: 19535 Destination Port: 18002

Sequence Number: 1162092610 Acknowledgment number: 0

TCP Header Length: 0 bytes

Window Size: 0

Flag: other

Urgent Pointer: 0

Option Field: 0

TCP Payload size: 0 bytes

TCP Payload type: other

Data: No payload

Ethernet Frame 200:

Source MAC Address: 00-C0-4F-49-D8-25 Destination MAC Address: 00-60-97-B9-58-7D Ether Type field: IPv4

Frame length : 60 Padding: 000000000000

IP Packet:

Source IP Address: /192.168.1.42 Destination IP Address: /192.168.1.62

IP Version: 4 Protocol Type: TCP

IP header length: 20 bytes

Total IP length: 28

Time to live: 64

Flag: 001

Fragment Offset: 14

TCP Segment:

Source Port: 21313 Destination Port: 20036

Sequence Number: 541347655 Acknowledgment number: 0

TCP Header Length: 0 bytes

Window Size: 0

Flag: other

Urgent Pointer: 0

Option Field: 0

TCP Payload size: 0 bytes

TCP Payload type: other

Data: No payload

Ethernet Frame 201:

Source MAC Address: 00-C0-4F-49-D8-25 Destination MAC Address: 00-60-97-B9-58-7D Ether Type field: IPv4

Frame length : 60 Padding: 000000000000

IP Packet:

Source IP Address: /192.168.1.42 Destination IP Address: /192.168.1.62

IP Version: 4 Protocol Type: TCP

IP header length: 20 bytes

Total IP length: 28

Time to live: 64

Flag: 001

Fragment Offset: 22

TCP Segment:

Source Port: 17440 Destination Port: 16985

Sequence Number: 542327113 Acknowledgment number: 0

TCP Header Length: 0 bytes

Window Size: 0

Flag: other

Urgent Pointer: 0

Option Field: 0

TCP Payload size: 0 bytes

TCP Payload type: other

Data: No payload

Ethernet Frame 202:

Source MAC Address: 00-C0-4F-49-D8-25 Destination MAC Address: 00-60-97-B9-58-7D Ether Type field: IPv4

Frame length : 60 Padding: 000000000000

IP Packet:

Source IP Address: /192.168.1.42 Destination IP Address: /192.168.1.62

IP Version: 4 Protocol Type: TCP

IP header length: 20 bytes

Total IP length: 28

Time to live: 64

Flag: 001

Fragment Offset: 4

TCP Segment:

Source Port: 8277 Destination Port: 21317

Sequence Number: 1313808463 Acknowledgment number: 0

TCP Header Length: 0 bytes

Window Size: 0

Flag: other

Urgent Pointer: 0

Option Field: 0

TCP Payload size: 0 bytes

TCP Payload type: other

Data: No payload

Ethernet Frame 202:

Source MAC Address: 00-C0-4F-49-D8-25 Destination MAC Address: 00-60-97-B9-58-7D Ether Type field: IPv4

Frame length : 60 Padding: 000000000000

IP Packet:

Source IP Address: /192.168.1.42 Destination IP Address: /192.168.1.62

IP Version: 4 Protocol Type: TCP

IP header length: 20 bytes

Total IP length: 28

Time to live: 64

Flag: 001

Fragment Offset: 7

TCP Segment:

Source Port: 8277 Destination Port: 21317

Sequence Number: 542394441 Acknowledgment number: 0

TCP Header Length: 0 bytes

Window Size: 0

Flag: other

Urgent Pointer: 0

Option Field: 0

TCP Payload size: 0 bytes

TCP Payload type: other

Data: No payload

Ethernet Frame 204:

Source MAC Address: 00-C0-4F-49-D8-25 Destination MAC Address: 00-60-97-B9-58-7D Ether Type field: IPv4

Frame length : 60 Padding: 000000000000

IP Packet:

Source IP Address: /192.168.1.42 Destination IP Address: /192.168.1.62

IP Version: 4 Protocol Type: TCP

IP header length: 20 bytes

Total IP length: 28

Time to live: 64

Flag: 001

Fragment Offset: 17

TCP Segment:

Source Port: 21844 Destination Port: 18511

Sequence Number: 1380538949 Acknowledgment number: 0

TCP Header Length: 0 bytes

Window Size: 0

Flag: other

Urgent Pointer: 0

Option Field: 0

TCP Payload size: 0 bytes

TCP Payload type: other

Data: No payload

Ethernet Frame 203:

Source MAC Address: 00-C0-4F-49-D8-25 Destination MAC Address: 00-60-97-B9-58-7D Ether Type field: IPv4

Frame length : 60 Padding: 000000000000

IP Packet:

Source IP Address: /192.168.1.42 Destination IP Address: /192.168.1.62

IP Version: 4 Protocol Type: TCP

IP header length: 20 bytes

Total IP length: 28

Time to live: 64

Flag: 001

Fragment Offset: 11

TCP Segment:

Source Port: 21844 Destination Port: 18511

Sequence Number: 541937486 Acknowledgment number: 0

TCP Header Length: 0 bytes

Window Size: 0

Flag: other

Urgent Pointer: 0

Option Field: 0

TCP Payload size: 0 bytes

TCP Payload type: other

Data: No payload

Ethernet Frame 209:

Source MAC Address: 00-C0-4F-49-D8-25 Destination MAC Address: 00-60-97-B9-58-7D Ether Type field: IPv4

Frame length : 60 Padding: 000000000000

IP Packet:

Source IP Address: /192.168.1.42 Destination IP Address: /192.168.1.62

IP Version: 4 Protocol Type: TCP

IP header length: 20 bytes

Total IP length: 28

Time to live: 64

Flag: 001

Fragment Offset: 10

TCP Segment:

Source Port: 2560 Destination Port: 0

Sequence Number: 542591308 Acknowledgment number: 0

TCP Header Length: 0 bytes

Window Size: 0

Flag: other

Urgent Pointer: 0

Option Field: 0

TCP Payload size: 0 bytes

TCP Payload type: other

Data: No payload

Ethernet Frame 212:

Source MAC Address: 00-C0-4F-49-D8-25 Destination MAC Address: 00-60-97-B9-58-7D Ether Type field: IPv4

Frame length : 66 Padding:

IP Packet:

Source IP Address: /192.168.1.42 Destination IP Address: /192.168.1.62

IP Version: 4 Protocol Type: TCP

IP header length: 20 bytes

Total IP length: 52

Time to live: 64

Flag: 001

Fragment Offset: 0

TCP Segment:

Source Port: 21 Destination Port: 4938

Sequence Number: 4221341147 Acknowledgment number: 708153374

TCP Header Length: 32 bytes

Window Size: 5792

Flag: (PSH, ACK)

Urgent Pointer: 0

Option Field: 12

TCP Payload size: 0 bytes

TCP Payload type: FTP

Data: No payload

Ethernet Frame 210:

Source MAC Address: 00-C0-4F-49-D8-25 Destination MAC Address: 00-60-97-B9-58-7D Ether Type field: IPv4

Frame length : 60 Padding: 000000000000

IP Packet:

Source IP Address: /192.168.1.42 Destination IP Address: /192.168.1.62

IP Version: 4 Protocol Type: TCP

IP header length: 20 bytes

Total IP length: 21

Time to live: 64

Flag: 000

Fragment Offset: 24

TCP Segment:

Source Port: 2560 Destination Port: 0

Sequence Number: 0 Acknowledgment number: 0

TCP Header Length: 0 bytes

Window Size: 0

Flag: other

Urgent Pointer: 0

Option Field: 0

TCP Payload size: 0 bytes

TCP Payload type: other

Data: No payload

Ethernet Frame 208:

Source MAC Address: 00-C0-4F-49-D8-25 Destination MAC Address: 00-60-97-B9-58-7D Ether Type field: IPv4

Frame length : 60 Padding: 000000000000

IP Packet:

Source IP Address: /192.168.1.42 Destination IP Address: /192.168.1.62

IP Version: 4 Protocol Type: TCP

IP header length: 20 bytes

Total IP length: 28

Time to live: 64

Flag: 001

Fragment Offset: 23

TCP Segment:

Source Port: 2560 Destination Port: 0

Sequence Number: 1196633613 Acknowledgment number: 0

TCP Header Length: 0 bytes

Window Size: 0

Flag: other

Urgent Pointer: 0

Option Field: 0

TCP Payload size: 0 bytes

TCP Payload type: other

Data: No payload

Ethernet Frame 205:

Source MAC Address: 00-C0-4F-49-D8-25 Destination MAC Address: 00-60-97-B9-58-7D Ether Type field: IPv4

Frame length : 60 Padding: 000000000000

IP Packet:

Source IP Address: /192.168.1.42 Destination IP Address: /192.168.1.62

IP Version: 4 Protocol Type: TCP

IP header length: 20 bytes

Total IP length: 28

Time to live: 64

Flag: 001

Fragment Offset: 8

TCP Segment:

Source Port: 8279 Destination Port: 18764

Sequence Number: 1381385554 Acknowledgment number: 0

TCP Header Length: 0 bytes

Window Size: 0

Flag: other

Urgent Pointer: 0

Option Field: 0

TCP Payload size: 0 bytes

TCP Payload type: other

Data: No payload

Ethernet Frame 207:

Source MAC Address: 00-C0-4F-49-D8-25 Destination MAC Address: 00-60-97-B9-58-7D Ether Type field: IPv4

Frame length : 60 Padding: 000000000000

IP Packet:

Source IP Address: /192.168.1.42 Destination IP Address: /192.168.1.62

IP Version: 4 Protocol Type: TCP

IP header length: 20 bytes

Total IP length: 28

Time to live: 64

Flag: 001

Fragment Offset: 19

TCP Segment:

Source Port: 8279 Destination Port: 18764

Sequence Number: 1277182533 Acknowledgment number: 0

TCP Header Length: 0 bytes

Window Size: 0

Flag: other

Urgent Pointer: 0

Option Field: 0

TCP Payload size: 0 bytes

TCP Payload type: other

Data: No payload

Ethernet Frame 206:

Source MAC Address: 00-C0-4F-49-D8-25 Destination MAC Address: 00-60-97-B9-58-7D Ether Type field: IPv4

Frame length : 60 Padding: 000000000000

IP Packet:

Source IP Address: /192.168.1.42 Destination IP Address: /192.168.1.62

IP Version: 4 Protocol Type: TCP

IP header length: 20 bytes

Total IP length: 28

Time to live: 64

Flag: 001

Fragment Offset: 13

TCP Segment:

Source Port: 8279 Destination Port: 18764

Sequence Number: 1414025045 Acknowledgment number: 0

TCP Header Length: 0 bytes

Window Size: 0

Flag: other

Urgent Pointer: 0

Option Field: 0

TCP Payload size: 0 bytes

TCP Payload type: other

Data: No payload

Ethernet Frame 213:

Source MAC Address: 00-C0-4F-49-D8-25 Destination MAC Address: 00-60-97-B9-58-7D Ether Type field: IPv4

Frame length : 60 Padding: 000000000000

IP Packet:

Source IP Address: /192.168.1.42 Destination IP Address: /192.168.1.62

IP Version: 4 Protocol Type: TCP

IP header length: 20 bytes

Total IP length: 28

Time to live: 64

Flag: 001

Fragment Offset: 16

TCP Segment:

Source Port: 17440 Destination Port: 16707

Sequence Number: 542461505 Acknowledgment number: 0

TCP Header Length: 0 bytes

Window Size: 0

Flag: other

Urgent Pointer: 0

Option Field: 0

TCP Payload size: 0 bytes

TCP Payload type: other

Data: No payload

Ethernet Frame 213:

Source MAC Address: 00-C0-4F-49-D8-25 Destination MAC Address: 00-60-97-B9-58-7D Ether Type field: IPv4

Frame length : 60 Padding: 000000000000

IP Packet:

Source IP Address: /192.168.1.42 Destination IP Address: /192.168.1.62

IP Version: 4 Protocol Type: TCP

IP header length: 20 bytes

Total IP length: 28

Time to live: 64

Flag: 001

Fragment Offset: 18

TCP Segment:

Source Port: 17440 Destination Port: 16707

Sequence Number: 1128616787 Acknowledgment number: 0

TCP Header Length: 0 bytes

Window Size: 0

Flag: other

Urgent Pointer: 0

Option Field: 0

TCP Payload size: 0 bytes

TCP Payload type: other

Data: No payload

Ethernet Frame 211:

Source MAC Address: 00-C0-4F-49-D8-25 Destination MAC Address: 00-60-97-B9-58-7D Ether Type field: IPv4

Frame length : 60 Padding: 000000000000

IP Packet:

Source IP Address: /192.168.1.42 Destination IP Address: /192.168.1.62

IP Version: 4 Protocol Type: TCP

IP header length: 20 bytes

Total IP length: 28

Time to live: 64

Flag: 001

Fragment Offset: 9

TCP Segment:

Source Port: 21 Destination Port: 4938

Sequence Number: 1414092361 Acknowledgment number: 0

TCP Header Length: 0 bytes

Window Size: 0

Flag: other

Urgent Pointer: 0

Option Field: 0

TCP Payload size: 0 bytes

TCP Payload type: other

Data: No payload

C:\Users\Prakash Thapa\Desktop\Spring 2018\NetworkSecurity\Assignments\Project1>javac \*.java

C:\Users\Prakash Thapa\Desktop\Spring 2018\NetworkSecurity\Assignments\Project1>java FrameParserDriver

Running Network Packet Parser.X

Device name in Java [0]=\Device\NPF\_{1B15DC9B-2D1A-4498-BA9B-456F60B6B41B}

Device name in Java [1]=\Device\NPF\_{EEA0A0D8-B476-40D1-81FC-99D89E2B64BF}

Device name in Java [2]=\Device\NPF\_{FF749EB5-8E5D-4358-AD08-B2192754EA2A}

Device name in Java [3]=\Device\NPF\_{56C306B8-36CB-4DB7-ABC5-F9864C29E32D}

Device name in Java [4]=\Device\NPF\_{3E34684D-ABAD-4C92-ACD9-69FF86F1FEA0}

Device name in Java [5]=\Device\NPF\_{C01ECCC1-DE4A-4C00-AB5E-FC0CF2359BC3}

Enter the adapter number:

5

Adapter [5] is open: \Device\NPF\_{C01ECCC1-DE4A-4C00-AB5E-FC0CF2359BC3}

Ethernet Frame 0:

Source MAC Address: 00-C0-4F-8D-93-F2 Destination MAC Address: 00-C0-4F-8D-99-31 Ether Type field: IPv4

Frame length : 60 Padding: 0000

IP Packet:

Source IP Address: /192.168.1.66 Destination IP Address: /192.168.1.14

IP Version: 4 Protocol Type: UDP

IP header length: 20 bytes

Total IP length: 28

Time to live: 64

Flag: 001

Fragment Offset: 3

UDP Datagram.

Source Port: 26990 Destination Port: 25860

UDP Length: 29555

UDP Data Length: 29547

UDP Data: 00 00 00 00 00 00 00 00 00 00 00 00 00 00 00 00 ................

00 00 ..

Ethernet Frame 3:

Source MAC Address: 00-C0-4F-8D-93-F2 Destination MAC Address: 00-C0-4F-8D-99-31 Ether Type field: IPv4

Frame length : 60 Padding: 0000

IP Packet:

Source IP Address: /192.168.1.66 Destination IP Address: /192.168.1.14

IP Version: 4 Protocol Type: UDP

IP header length: 20 bytes

Total IP length: 28

Time to live: 64

Flag: 001

Fragment Offset: 2

UDP Datagram.

Source Port: 0 Destination Port: 0

UDP Length: 1641

UDP Data Length: 1633

UDP Data: 00 00 00 00 00 00 00 00 00 00 00 00 00 00 00 00 ................

00 00 ..

Ethernet Frame 2:

Source MAC Address: 00-C0-4F-8D-93-F2 Destination MAC Address: 00-C0-4F-8D-99-31 Ether Type field: IPv4

Frame length : 60 Padding: 0000

IP Packet:

Source IP Address: /192.168.1.66 Destination IP Address: /192.168.1.14

IP Version: 4 Protocol Type: UDP

IP header length: 20 bytes

Total IP length: 28

Time to live: 64

Flag: 001

Fragment Offset: 0

UDP Datagram.

Source Port: 34808 Destination Port: 53

UDP Length: 48

UDP Data Length: 40

UDP Data: 00 00 00 00 00 00 00 00 00 00 00 00 00 00 00 00 ................

00 00 ..

Ethernet Frame 4:

Source MAC Address: 00-C0-4F-8D-93-F2 Destination MAC Address: 00-C0-4F-8D-99-31 Ether Type field: IPv4

Frame length : 60 Padding: 0000

IP Packet:

Source IP Address: /192.168.1.66 Destination IP Address: /192.168.1.14

IP Version: 4 Protocol Type: UDP

IP header length: 20 bytes

Total IP length: 28

Time to live: 64

Flag: 001

Fragment Offset: 1

UDP Datagram.

Source Port: 58893 Destination Port: 256

UDP Length: 1

UDP Data Length: -7

UDP Data: 00 00 00 00 00 00 00 00 00 00 00 00 00 00 00 00 ................

00 00 ..

Ethernet Frame 1:

Source MAC Address: 00-C0-4F-8D-93-F2 Destination MAC Address: 00-C0-4F-8D-99-31 Ether Type field: IPv4

Frame length : 60 Padding: 0000

IP Packet:

Source IP Address: /192.168.1.66 Destination IP Address: /192.168.1.14

IP Version: 4 Protocol Type: UDP

IP header length: 20 bytes

Total IP length: 28

Time to live: 64

Flag: 000

Fragment Offset: 5

UDP Datagram.

Source Port: 25956 Destination Port: 29952

UDP Length: 1

UDP Data Length: -7

UDP Data: 00 00 00 00 00 00 00 00 00 00 00 00 00 00 00 00 ................

00 00 ..

Ethernet Frame 0:

Source MAC Address: 00-C0-4F-8D-93-F2 Destination MAC Address: 00-C0-4F-8D-99-31 Ether Type field: IPv4

Frame length : 60 Padding: 0000

IP Packet:

Source IP Address: /192.168.1.66 Destination IP Address: /192.168.1.14

IP Version: 4 Protocol Type: UDP

IP header length: 20 bytes

Total IP length: 28

Time to live: 64

Flag: 001

Fragment Offset: 4

UDP Datagram.

Source Port: 1653 Destination Port: 29813

UDP Length: 27763

UDP Data Length: 27755

UDP Data: 00 00 00 00 00 00 00 00 00 00 00 00 00 00 00 00 ................

00 00 ..

Ethernet Frame 5:

Source MAC Address: 00-C0-4F-8D-99-31 Destination MAC Address: 00-C0-4F-8D-93-F2 Ether Type field: IPv4

Frame length : 60 Padding: 0000

IP Packet:

Source IP Address: /192.168.1.14 Destination IP Address: /192.168.1.66

IP Version: 4 Protocol Type: UDP

IP header length: 20 bytes

Total IP length: 28

Time to live: 64

Flag: 001

Fragment Offset: 5

UDP Datagram.

Source Port: 25956 Destination Port: 29952

UDP Length: 1

UDP Data Length: -7

UDP Data: 00 00 00 00 00 00 00 00 00 00 00 00 00 00 00 00 ................

00 00 ..

Ethernet Frame 8:

Source MAC Address: 00-C0-4F-8D-99-31 Destination MAC Address: 00-C0-4F-8D-93-F2 Ether Type field: IPv4

Frame length : 60 Padding: 0000

IP Packet:

Source IP Address: /192.168.1.14 Destination IP Address: /192.168.1.66

IP Version: 4 Protocol Type: UDP

IP header length: 20 bytes

Total IP length: 28

Time to live: 64

Flag: 001

Fragment Offset: 7

UDP Datagram.

Source Port: 20864 Destination Port: 4

UDP Length: 49320

UDP Data Length: 49312

UDP Data: 00 00 00 00 00 00 00 00 00 00 00 00 00 00 00 00 ................

00 00 ..

Ethernet Frame 7:

Source MAC Address: 00-C0-4F-8D-99-31 Destination MAC Address: 00-C0-4F-8D-93-F2 Ether Type field: IPv4

Frame length : 60 Padding: 0000

IP Packet:

Source IP Address: /192.168.1.14 Destination IP Address: /192.168.1.66

IP Version: 4 Protocol Type: UDP

IP header length: 20 bytes

Total IP length: 28

Time to live: 64

Flag: 001

Fragment Offset: 2

UDP Datagram.

Source Port: 1 Destination Port: 1

UDP Length: 1641

UDP Data Length: 1633

UDP Data: 00 00 00 00 00 00 00 00 00 00 00 00 00 00 00 00 ................

00 00 ..

Ethernet Frame 6:

Source MAC Address: 00-C0-4F-8D-99-31 Destination MAC Address: 00-C0-4F-8D-93-F2 Ether Type field: IPv4

Frame length : 60 Padding: 0000

IP Packet:

Source IP Address: /192.168.1.14 Destination IP Address: /192.168.1.66

IP Version: 4 Protocol Type: UDP

IP header length: 20 bytes

Total IP length: 28

Time to live: 64

Flag: 001

Fragment Offset: 4

UDP Datagram.

Source Port: 1653 Destination Port: 29813

UDP Length: 27763

UDP Data Length: 27755

UDP Data: 00 00 00 00 00 00 00 00 00 00 00 00 00 00 00 00 ................

00 00 ..

Ethernet Frame 17:

Source MAC Address: 00-C0-4F-8D-99-31 Destination MAC Address: 00-C0-4F-8D-93-F2 Ether Type field: IPv4

Frame length : 60 Padding: 0000

IP Packet:

Source IP Address: /192.168.1.14 Destination IP Address: /192.168.1.66

IP Version: 4 Protocol Type: UDP

IP header length: 20 bytes

Total IP length: 24

Time to live: 64

Flag: 000

Fragment Offset: 12

UDP Datagram.

Source Port: 49320 Destination Port: 270

UDP Length: 0

UDP Data Length: -8

UDP Data: 00 00 00 00 00 00 00 00 00 00 00 00 00 00 00 00 ................

00 00 ..

Ethernet Frame 16:

Source MAC Address: 00-C0-4F-8D-99-31 Destination MAC Address: 00-C0-4F-8D-93-F2 Ether Type field: IPv4

Frame length : 60 Padding: 0000

IP Packet:

Source IP Address: /192.168.1.14 Destination IP Address: /192.168.1.66

IP Version: 4 Protocol Type: UDP

IP header length: 20 bytes

Total IP length: 28

Time to live: 64

Flag: 001

Fragment Offset: 6

UDP Datagram.

Source Port: 49164 Destination Port: 1

UDP Length: 1

UDP Data Length: -7

UDP Data: 00 00 00 00 00 00 00 00 00 00 00 00 00 00 00 00 ................

00 00 ..

Ethernet Frame 14:

Source MAC Address: 00-C0-4F-8D-99-31 Destination MAC Address: 00-C0-4F-8D-93-F2 Ether Type field: IPv4

Frame length : 60 Padding: 0000

IP Packet:

Source IP Address: /192.168.1.14 Destination IP Address: /192.168.1.66

IP Version: 4 Protocol Type: UDP

IP header length: 20 bytes

Total IP length: 28

Time to live: 64

Flag: 001

Fragment Offset: 9

UDP Datagram.

Source Port: 20864 Destination Port: 8

UDP Length: 1378

UDP Data Length: 1370

UDP Data: 00 00 00 00 00 00 00 00 00 00 00 00 00 00 00 00 ................

00 00 ..

Ethernet Frame 15:

Source MAC Address: 00-C0-4F-8D-99-31 Destination MAC Address: 00-C0-4F-8D-93-F2 Ether Type field: IPv4

Frame length : 60 Padding: 0000

IP Packet:

Source IP Address: /192.168.1.14 Destination IP Address: /192.168.1.66

IP Version: 4 Protocol Type: UDP

IP header length: 20 bytes

Total IP length: 28

Time to live: 64

Flag: 001

Fragment Offset: 11

UDP Datagram.

Source Port: 1 Destination Port: 1

UDP Length: 20864

UDP Data Length: 20856

UDP Data: 00 00 00 00 00 00 00 00 00 00 00 00 00 00 00 00 ................

00 00 ..

Ethernet Frame 13:

Source MAC Address: 00-C0-4F-8D-99-31 Destination MAC Address: 00-C0-4F-8D-93-F2 Ether Type field: IPv4

Frame length : 60 Padding: 0000

IP Packet:

Source IP Address: /192.168.1.14 Destination IP Address: /192.168.1.66

IP Version: 4 Protocol Type: UDP

IP header length: 20 bytes

Total IP length: 28

Time to live: 64

Flag: 001

Fragment Offset: 8

UDP Datagram.

Source Port: 49171 Destination Port: 2

UDP Length: 1

UDP Data Length: -7

UDP Data: 00 00 00 00 00 00 00 00 00 00 00 00 00 00 00 00 ................

00 00 ..

Ethernet Frame 12:

Source MAC Address: 00-C0-4F-8D-99-31 Destination MAC Address: 00-C0-4F-8D-93-F2 Ether Type field: IPv4

Frame length : 60 Padding: 0000

IP Packet:

Source IP Address: /192.168.1.14 Destination IP Address: /192.168.1.66

IP Version: 4 Protocol Type: UDP

IP header length: 20 bytes

Total IP length: 28

Time to live: 64

Flag: 001

Fragment Offset: 3

UDP Datagram.

Source Port: 26990 Destination Port: 25860

UDP Length: 29555

UDP Data Length: 29547

UDP Data: 00 00 00 00 00 00 00 00 00 00 00 00 00 00 00 00 ................

00 00 ..

Ethernet Frame 11:

Source MAC Address: 00-C0-4F-8D-99-31 Destination MAC Address: 00-C0-4F-8D-93-F2 Ether Type field: IPv4

Frame length : 60 Padding: 0000

IP Packet:

Source IP Address: /192.168.1.14 Destination IP Address: /192.168.1.66

IP Version: 4 Protocol Type: UDP

IP header length: 20 bytes

Total IP length: 28

Time to live: 64

Flag: 001

Fragment Offset: 10

UDP Datagram.

Source Port: 28526 Destination Port: 49171

UDP Length: 49220

UDP Data Length: 49212

UDP Data: 00 00 00 00 00 00 00 00 00 00 00 00 00 00 00 00 ................

00 00 ..

Ethernet Frame 10:

Source MAC Address: 00-C0-4F-8D-99-31 Destination MAC Address: 00-C0-4F-8D-93-F2 Ether Type field: IPv4

Frame length : 60 Padding: 0000

IP Packet:

Source IP Address: /192.168.1.14 Destination IP Address: /192.168.1.66

IP Version: 4 Protocol Type: UDP

IP header length: 20 bytes

Total IP length: 28

Time to live: 64

Flag: 001

Fragment Offset: 0

UDP Datagram.

Source Port: 53 Destination Port: 34808

UDP Length: 100

UDP Data Length: 92

UDP Data: 00 00 00 00 00 00 00 00 00 00 00 00 00 00 00 00 ................

00 00 ..

Ethernet Frame 9:

Source MAC Address: 00-C0-4F-8D-99-31 Destination MAC Address: 00-C0-4F-8D-93-F2 Ether Type field: IPv4

Frame length : 60 Padding: 0000

IP Packet:

Source IP Address: /192.168.1.14 Destination IP Address: /192.168.1.66

IP Version: 4 Protocol Type: UDP

IP header length: 20 bytes

Total IP length: 28

Time to live: 64

Flag: 001

Fragment Offset: 1

UDP Datagram.

Source Port: 58893 Destination Port: 34176

UDP Length: 1

UDP Data Length: -7

UDP Data: 00 00 00 00 00 00 00 00 00 00 00 00 00 00 00 00 ................

00 00 ..

Ethernet Frame 18:

Source MAC Address: 08-00-20-AB-D4-A4 Destination MAC Address: 00-C0-4F-58-D9-94 Ether Type field: IPv4

Frame length : 60 Padding: 0000

IP Packet:

Source IP Address: /192.168.1.22 Destination IP Address: /192.168.1.46

IP Version: 4 Protocol Type: UDP

IP header length: 20 bytes

Total IP length: 28

Time to live: 255

Flag: 001

Fragment Offset: 0

UDP Datagram.

Source Port: 52578 Destination Port: 53

UDP Length: 57

UDP Data Length: 49

UDP Data: 00 00 00 00 00 00 00 00 00 00 00 00 00 00 00 00 ................

00 00 ..

Ethernet Frame 19:

Source MAC Address: 00-C0-4F-58-D9-94 Destination MAC Address: 08-00-20-AB-D4-A4 Ether Type field: IPv4

Frame length : 60 Padding: 0000

IP Packet:

Source IP Address: /192.168.1.46 Destination IP Address: /192.168.1.22

IP Version: 4 Protocol Type: UDP

IP header length: 20 bytes

Total IP length: 28

Time to live: 128

Flag: 001

Fragment Offset: 2

UDP Datagram.

Source Port: 0 Destination Port: 0

UDP Length: 2152

UDP Data Length: 2144

UDP Data: 00 00 00 00 00 00 00 00 00 00 00 00 00 00 00 00 ................

00 00 ..

Ethernet Frame 20:

Source MAC Address: 00-C0-4F-58-D9-94 Destination MAC Address: 08-00-20-AB-D4-A4 Ether Type field: IPv4

Frame length : 60 Padding: 0000

IP Packet:

Source IP Address: /192.168.1.46 Destination IP Address: /192.168.1.22

IP Version: 4 Protocol Type: UDP

IP header length: 20 bytes

Total IP length: 28

Time to live: 128

Flag: 001

Fragment Offset: 8

UDP Datagram.

Source Port: 14 Destination Port: 4096

UDP Length: 1216

UDP Data Length: 1208

UDP Data: 00 00 00 00 00 00 00 00 00 00 00 00 00 00 00 00 ................

00 00 ..

Ethernet Frame 22:

Source MAC Address: 00-C0-4F-58-D9-94 Destination MAC Address: 08-00-20-AB-D4-A4 Ether Type field: IPv4

Frame length : 60 Padding: 0000

IP Packet:

Source IP Address: /192.168.1.46 Destination IP Address: /192.168.1.22

IP Version: 4 Protocol Type: UDP

IP header length: 20 bytes

Total IP length: 21

Time to live: 128

Flag: 000

Fragment Offset: 9

UDP Datagram.

Source Port: 2560 Destination Port: 0

UDP Length: 0

UDP Data Length: -8

UDP Data: 00 00 00 00 00 00 00 00 00 00 00 00 00 00 00 00 ................

00 00 ..

Ethernet Frame 21:

Source MAC Address: 00-C0-4F-58-D9-94 Destination MAC Address: 08-00-20-AB-D4-A4 Ether Type field: IPv4

Frame length : 60 Padding: 0000

IP Packet:

Source IP Address: /192.168.1.46 Destination IP Address: /192.168.1.22

IP Version: 4 Protocol Type: UDP

IP header length: 20 bytes

Total IP length: 28

Time to live: 128

Flag: 001

Fragment Offset: 1

UDP Datagram.

Source Port: 57410 Destination Port: 34176

UDP Length: 1

UDP Data Length: -7

UDP Data: 00 00 00 00 00 00 00 00 00 00 00 00 00 00 00 00 ................

00 00 ..

Ethernet Frame 23:

Source MAC Address: 00-C0-4F-58-D9-94 Destination MAC Address: 08-00-20-AB-D4-A4 Ether Type field: IPv4

Frame length : 60 Padding: 0000

IP Packet:

Source IP Address: /192.168.1.46 Destination IP Address: /192.168.1.22

IP Version: 4 Protocol Type: UDP

IP header length: 20 bytes

Total IP length: 28

Time to live: 128

Flag: 001

Fragment Offset: 0

UDP Datagram.

Source Port: 53 Destination Port: 52578

UDP Length: 73

UDP Data Length: 65

UDP Data: 00 00 00 00 00 00 00 00 00 00 00 00 00 00 00 00 ................

00 00 ..

Ethernet Frame 24:

Source MAC Address: 00-C0-4F-58-D9-94 Destination MAC Address: 08-00-20-AB-D4-A4 Ether Type field: IPv4

Frame length : 60 Padding: 0000

IP Packet:

Source IP Address: /192.168.1.46 Destination IP Address: /192.168.1.22

IP Version: 4 Protocol Type: UDP

IP header length: 20 bytes

Total IP length: 28

Time to live: 128

Flag: 001

Fragment Offset: 3

UDP Datagram.

Source Port: 29295 Destination Port: 26469

UDP Length: 28166

UDP Data Length: 28158

UDP Data: 00 00 00 00 00 00 00 00 00 00 00 00 00 00 00 00 ................

00 00 ..

Ethernet Frame 27:

Source MAC Address: 00-C0-4F-58-D9-94 Destination MAC Address: 08-00-20-AB-D4-A4 Ether Type field: IPv4

Frame length : 60 Padding: 0000

IP Packet:

Source IP Address: /192.168.1.46 Destination IP Address: /192.168.1.22

IP Version: 4 Protocol Type: UDP

IP header length: 20 bytes

Total IP length: 28

Time to live: 128

Flag: 001

Fragment Offset: 7

UDP Datagram.

Source Port: 448 Destination Port: 3072

UDP Length: 256

UDP Data Length: 248

UDP Data: 00 00 00 00 00 00 00 00 00 00 00 00 00 00 00 00 ................

00 00 ..

Ethernet Frame 26:

Source MAC Address: 00-C0-4F-58-D9-94 Destination MAC Address: 08-00-20-AB-D4-A4 Ether Type field: IPv4

Frame length : 60 Padding: 0000

IP Packet:

Source IP Address: /192.168.1.46 Destination IP Address: /192.168.1.22

IP Version: 4 Protocol Type: UDP

IP header length: 20 bytes

Total IP length: 28

Time to live: 128

Flag: 001

Fragment Offset: 5

UDP Datagram.

Source Port: 25350 Destination Port: 30068

UDP Length: 30060

UDP Data Length: 30052

UDP Data: 00 00 00 00 00 00 00 00 00 00 00 00 00 00 00 00 ................

00 00 ..

Ethernet Frame 25:

Source MAC Address: 00-C0-4F-58-D9-94 Destination MAC Address: 08-00-20-AB-D4-A4 Ether Type field: IPv4

Frame length : 60 Padding: 0000

IP Packet:

Source IP Address: /192.168.1.46 Destination IP Address: /192.168.1.22

IP Version: 4 Protocol Type: UDP

IP header length: 20 bytes

Total IP length: 28

Time to live: 128

Flag: 001

Fragment Offset: 6

UDP Datagram.

Source Port: 869 Destination Port: 25717

UDP Length: 0

UDP Data Length: -8

UDP Data: 00 00 00 00 00 00 00 00 00 00 00 00 00 00 00 00 ................

00 00 ..

Ethernet Frame 28:

Source MAC Address: 00-C0-4F-58-D9-94 Destination MAC Address: 08-00-20-AB-D4-A4 Ether Type field: IPv4

Frame length : 60 Padding: 0000

IP Packet:

Source IP Address: /192.168.1.46 Destination IP Address: /192.168.1.22

IP Version: 4 Protocol Type: UDP

IP header length: 20 bytes

Total IP length: 28

Time to live: 128

Flag: 001

Fragment Offset: 4

UDP Datagram.

Source Port: 28533 Destination Port: 28721

UDP Length: 1139

UDP Data Length: 1131

UDP Data: 00 00 00 00 00 00 00 00 00 00 00 00 00 00 00 00 ................

00 00 ..

Ethernet Frame 29:

Source MAC Address: 08-00-20-AB-D4-A4 Destination MAC Address: 00-C0-4F-58-D9-94 Ether Type field: IPv4

Frame length : 60 Padding: 0000

IP Packet:

Source IP Address: /192.168.1.22 Destination IP Address: /192.168.1.46

IP Version: 4 Protocol Type: UDP

IP header length: 20 bytes

Total IP length: 28

Time to live: 255

Flag: 001

Fragment Offset: 6

UDP Datagram.

Source Port: 869 Destination Port: 25717

UDP Length: 0

UDP Data Length: -8

UDP Data: 00 00 00 00 00 00 00 00 00 00 00 00 00 00 00 00 ................

00 00 ..

Ethernet Frame 30:

Source MAC Address: 08-00-20-AB-D4-A4 Destination MAC Address: 00-C0-4F-58-D9-94 Ether Type field: IPv4

Frame length : 60 Padding: 0000

IP Packet:

Source IP Address: /192.168.1.22 Destination IP Address: /192.168.1.46

IP Version: 4 Protocol Type: UDP

IP header length: 20 bytes

Total IP length: 28

Time to live: 255

Flag: 001

Fragment Offset: 5

UDP Datagram.

Source Port: 25350 Destination Port: 30068

UDP Length: 30060

UDP Data Length: 30052

UDP Data: 00 00 00 00 00 00 00 00 00 00 00 00 00 00 00 00 ................

00 00 ..

Ethernet Frame 31:

Source MAC Address: 08-00-20-AB-D4-A4 Destination MAC Address: 00-C0-4F-58-D9-94 Ether Type field: IPv4

Frame length : 60 Padding: 0000

IP Packet:

Source IP Address: /192.168.1.22 Destination IP Address: /192.168.1.46

IP Version: 4 Protocol Type: UDP

IP header length: 20 bytes

Total IP length: 28

Time to live: 255

Flag: 001

Fragment Offset: 2

UDP Datagram.

Source Port: 0 Destination Port: 0

UDP Length: 2152

UDP Data Length: 2144

UDP Data: 00 00 00 00 00 00 00 00 00 00 00 00 00 00 00 00 ................

00 00 ..

Ethernet Frame 33:

Source MAC Address: 08-00-20-AB-D4-A4 Destination MAC Address: 00-C0-4F-58-D9-94 Ether Type field: IPv4

Frame length : 60 Padding: 0000

IP Packet:

Source IP Address: /192.168.1.22 Destination IP Address: /192.168.1.46

IP Version: 4 Protocol Type: UDP

IP header length: 20 bytes

Total IP length: 21

Time to live: 255

Flag: 000

Fragment Offset: 7

UDP Datagram.

Source Port: 256 Destination Port: 0

UDP Length: 0

UDP Data Length: -8

UDP Data: 00 00 00 00 00 00 00 00 00 00 00 00 00 00 00 00 ................

00 00 ..

Ethernet Frame 32:

Source MAC Address: 08-00-20-AB-D4-A4 Destination MAC Address: 00-C0-4F-58-D9-94 Ether Type field: IPv4

Frame length : 60 Padding: 0000

IP Packet:

Source IP Address: /192.168.1.22 Destination IP Address: /192.168.1.46

IP Version: 4 Protocol Type: UDP

IP header length: 20 bytes

Total IP length: 28

Time to live: 255

Flag: 001

Fragment Offset: 3

UDP Datagram.

Source Port: 29295 Destination Port: 26469

UDP Length: 28166

UDP Data Length: 28158

UDP Data: 00 00 00 00 00 00 00 00 00 00 00 00 00 00 00 00 ................

00 00 ..

Ethernet Frame 34:

Source MAC Address: 08-00-20-AB-D4-A4 Destination MAC Address: 00-C0-4F-58-D9-94 Ether Type field: IPv4

Frame length : 60 Padding: 0000

IP Packet:

Source IP Address: /192.168.1.22 Destination IP Address: /192.168.1.46

IP Version: 4 Protocol Type: UDP

IP header length: 20 bytes

Total IP length: 28

Time to live: 255

Flag: 001

Fragment Offset: 4

UDP Datagram.

Source Port: 28533 Destination Port: 28721

UDP Length: 1139

UDP Data Length: 1131

UDP Data: 00 00 00 00 00 00 00 00 00 00 00 00 00 00 00 00 ................

00 00 ..

Ethernet Frame 35:

Source MAC Address: 08-00-20-AB-D4-A4 Destination MAC Address: 00-C0-4F-58-D9-94 Ether Type field: IPv4

Frame length : 60 Padding: 0000

IP Packet:

Source IP Address: /192.168.1.22 Destination IP Address: /192.168.1.46

IP Version: 4 Protocol Type: UDP

IP header length: 20 bytes

Total IP length: 28

Time to live: 255

Flag: 001

Fragment Offset: 1

UDP Datagram.

Source Port: 57410 Destination Port: 256

UDP Length: 1

UDP Data Length: -7

UDP Data: 00 00 00 00 00 00 00 00 00 00 00 00 00 00 00 00 ................

00 00 ..

Ethernet Frame 36:

Source MAC Address: 00-04-76-3B-0C-E7 Destination MAC Address: 00-E0-81-25-C0-8B Ether Type field: IPv4

Frame length : 60 Padding:

IP Packet:

Source IP Address: /192.168.1.32 Destination IP Address: /192.168.1.75

IP Version: 4 Protocol Type: ICMP

IP header length: 20 bytes

Total IP length: 28

Time to live: 64

Flag: 001

Fragment Offset: 4

Type: 8

Request or Reply: Request

Code: 8

Ethernet Frame 38:

Source MAC Address: 00-04-76-3B-0C-E7 Destination MAC Address: 00-E0-81-25-C0-8B Ether Type field: IPv4

Frame length : 60 Padding:

IP Packet:

Source IP Address: /192.168.1.32 Destination IP Address: /192.168.1.75

IP Version: 4 Protocol Type: ICMP

IP header length: 20 bytes

Total IP length: 28

Time to live: 64

Flag: 001

Fragment Offset: 5

Type: 0

Request or Reply: Reply

Code: 0

Ethernet Frame 36:

Source MAC Address: 00-04-76-3B-0C-E7 Destination MAC Address: 00-E0-81-25-C0-8B Ether Type field: IPv4

Frame length : 60 Padding:

IP Packet:

Source IP Address: /192.168.1.32 Destination IP Address: /192.168.1.75

IP Version: 4 Protocol Type: ICMP

IP header length: 20 bytes

Total IP length: 28

Time to live: 64

Flag: 001

Fragment Offset: 6

Type: 8

Request or Reply: Request

Code: 8

Ethernet Frame 37:

Source MAC Address: 00-04-76-3B-0C-E7 Destination MAC Address: 00-E0-81-25-C0-8B Ether Type field: IPv4

Frame length : 60 Padding:

IP Packet:

Source IP Address: /192.168.1.32 Destination IP Address: /192.168.1.75

IP Version: 4 Protocol Type: ICMP

IP header length: 20 bytes

Total IP length: 28

Time to live: 64

Flag: 001

Fragment Offset: 2

Type: 8

Request or Reply: Request

Code: 8

Ethernet Frame 39:

Source MAC Address: 00-E0-81-25-C0-8B Destination MAC Address: 00-04-76-3B-0C-E7 Ether Type field: IPv4

Frame length : 98 Padding:

IP Packet:

Source IP Address: /192.168.1.75 Destination IP Address: /192.168.1.32

IP Version: 4 Protocol Type: ICMP

IP header length: 20 bytes

Total IP length: 84

Time to live: 128

Flag: 000

Fragment Offset: 0

Type: 0

Request or Reply: Reply

Code: 0

Ethernet Frame 40:

Source MAC Address: 00-04-76-3B-0C-E7 Destination MAC Address: 00-E0-81-25-C0-8B Ether Type field: IPv4

Frame length : 60 Padding:

IP Packet:

Source IP Address: /192.168.1.32 Destination IP Address: /192.168.1.75

IP Version: 4 Protocol Type: ICMP

IP header length: 20 bytes

Total IP length: 28

Time to live: 64

Flag: 001

Fragment Offset: 3

Type: 0

Request or Reply: Reply

Code: 0

Ethernet Frame 39:

Source MAC Address: 00-04-76-3B-0C-E7 Destination MAC Address: 00-E0-81-25-C0-8B Ether Type field: IPv4

Frame length : 60 Padding:

IP Packet:

Source IP Address: /192.168.1.32 Destination IP Address: /192.168.1.75

IP Version: 4 Protocol Type: ICMP

IP header length: 20 bytes

Total IP length: 28

Time to live: 64

Flag: 001

Fragment Offset: 1

Type: E

Request or Reply:

Code: E

Ethernet Frame 41:

Source MAC Address: 00-04-76-3B-0C-E7 Destination MAC Address: 00-E0-81-25-C0-8B Ether Type field: IPv4

Frame length : 60 Padding:

IP Packet:

Source IP Address: /192.168.1.32 Destination IP Address: /192.168.1.75

IP Version: 4 Protocol Type: ICMP

IP header length: 20 bytes

Total IP length: 28

Time to live: 64

Flag: 000

Fragment Offset: 7

Type: 0

Request or Reply: Reply

Code: 0

Ethernet Frame 45:

Source MAC Address: 00-04-76-3B-0C-E7 Destination MAC Address: 00-E0-81-25-C0-8B Ether Type field: IPv4

Frame length : 60 Padding:

IP Packet:

Source IP Address: /192.168.1.32 Destination IP Address: /192.168.1.75

IP Version: 4 Protocol Type: ICMP

IP header length: 20 bytes

Total IP length: 28

Time to live: 64

Flag: 001

Fragment Offset: 4

Type: 8

Request or Reply: Request

Code: 8

Ethernet Frame 44:

Source MAC Address: 00-04-76-3B-0C-E7 Destination MAC Address: 00-E0-81-25-C0-8B Ether Type field: IPv4

Frame length : 60 Padding:

IP Packet:

Source IP Address: /192.168.1.32 Destination IP Address: /192.168.1.75

IP Version: 4 Protocol Type: ICMP

IP header length: 20 bytes

Total IP length: 28

Time to live: 64

Flag: 001

Fragment Offset: 3

Type: 0

Request or Reply: Reply

Code: 0

Ethernet Frame 43:

Source MAC Address: 00-04-76-3B-0C-E7 Destination MAC Address: 00-E0-81-25-C0-8B Ether Type field: IPv4

Frame length : 60 Padding:

IP Packet:

Source IP Address: /192.168.1.32 Destination IP Address: /192.168.1.75

IP Version: 4 Protocol Type: ICMP

IP header length: 20 bytes

Total IP length: 28

Time to live: 64

Flag: 001

Fragment Offset: 6

Type: 8

Request or Reply: Request

Code: 8

Ethernet Frame 42:

Source MAC Address: 00-04-76-3B-0C-E7 Destination MAC Address: 00-E0-81-25-C0-8B Ether Type field: IPv4

Frame length : 60 Padding:

IP Packet:

Source IP Address: /192.168.1.32 Destination IP Address: /192.168.1.75

IP Version: 4 Protocol Type: ICMP

IP header length: 20 bytes

Total IP length: 28

Time to live: 64

Flag: 001

Fragment Offset: 0

Type: 8

Request or Reply: Request

Code: 8

Ethernet Frame 50:

Source MAC Address: 00-04-76-3B-0C-E7 Destination MAC Address: 00-E0-81-25-C0-8B Ether Type field: IPv4

Frame length : 60 Padding:

IP Packet:

Source IP Address: /192.168.1.32 Destination IP Address: /192.168.1.75

IP Version: 4 Protocol Type: ICMP

IP header length: 20 bytes

Total IP length: 28

Time to live: 64

Flag: 001

Fragment Offset: 0

Type: 8

Request or Reply: Request

Code: 8

Ethernet Frame 49:

Source MAC Address: 00-04-76-3B-0C-E7 Destination MAC Address: 00-E0-81-25-C0-8B Ether Type field: IPv4

Frame length : 60 Padding:

IP Packet:

Source IP Address: /192.168.1.32 Destination IP Address: /192.168.1.75

IP Version: 4 Protocol Type: ICMP

IP header length: 20 bytes

Total IP length: 28

Time to live: 64

Flag: 001

Fragment Offset: 1

Type: F

Request or Reply:

Code: F

Ethernet Frame 48:

Source MAC Address: 00-04-76-3B-0C-E7 Destination MAC Address: 00-E0-81-25-C0-8B Ether Type field: IPv4

Frame length : 60 Padding:

IP Packet:

Source IP Address: /192.168.1.32 Destination IP Address: /192.168.1.75

IP Version: 4 Protocol Type: ICMP

IP header length: 20 bytes

Total IP length: 28

Time to live: 64

Flag: 000

Fragment Offset: 7

Type: 0

Request or Reply: Reply

Code: 0

Ethernet Frame 47:

Source MAC Address: 00-04-76-3B-0C-E7 Destination MAC Address: 00-E0-81-25-C0-8B Ether Type field: IPv4

Frame length : 60 Padding:

IP Packet:

Source IP Address: /192.168.1.32 Destination IP Address: /192.168.1.75

IP Version: 4 Protocol Type: ICMP

IP header length: 20 bytes

Total IP length: 28

Time to live: 64

Flag: 001

Fragment Offset: 2

Type: 8

Request or Reply: Request

Code: 8

Ethernet Frame 46:

Source MAC Address: 00-04-76-3B-0C-E7 Destination MAC Address: 00-E0-81-25-C0-8B Ether Type field: IPv4

Frame length : 60 Padding:

IP Packet:

Source IP Address: /192.168.1.32 Destination IP Address: /192.168.1.75

IP Version: 4 Protocol Type: ICMP

IP header length: 20 bytes

Total IP length: 28

Time to live: 64

Flag: 001

Fragment Offset: 5

Type: 0

Request or Reply: Reply

Code: 0

Ethernet Frame 54:

Source MAC Address: 00-04-76-3B-0C-E7 Destination MAC Address: 00-E0-81-25-C0-8B Ether Type field: IPv4

Frame length : 60 Padding:

IP Packet:

Source IP Address: /192.168.1.32 Destination IP Address: /192.168.1.75

IP Version: 4 Protocol Type: ICMP

IP header length: 20 bytes

Total IP length: 28

Time to live: 64

Flag: 001

Fragment Offset: 6

Type: 8

Request or Reply: Request

Code: 8

Ethernet Frame 54:

Source MAC Address: 00-04-76-3B-0C-E7 Destination MAC Address: 00-E0-81-25-C0-8B Ether Type field: IPv4

Frame length : 60 Padding:

IP Packet:

Source IP Address: /192.168.1.32 Destination IP Address: /192.168.1.75

IP Version: 4 Protocol Type: ICMP

IP header length: 20 bytes

Total IP length: 28

Time to live: 64

Flag: 001

Fragment Offset: 1

Type: 0

Request or Reply: Reply

Code: 0

Ethernet Frame 53:

Source MAC Address: 00-E0-81-25-C0-8B Destination MAC Address: 00-04-76-3B-0C-E7 Ether Type field: IPv4

Frame length : 98 Padding:

IP Packet:

Source IP Address: /192.168.1.75 Destination IP Address: /192.168.1.32

IP Version: 4 Protocol Type: ICMP

IP header length: 20 bytes

Total IP length: 84

Time to live: 128

Flag: 000

Fragment Offset: 0

Type: 0

Request or Reply: Reply

Code: 0

Ethernet Frame 52:

Source MAC Address: 00-04-76-3B-0C-E7 Destination MAC Address: 00-E0-81-25-C0-8B Ether Type field: IPv4

Frame length : 60 Padding:

IP Packet:

Source IP Address: /192.168.1.32 Destination IP Address: /192.168.1.75

IP Version: 4 Protocol Type: ICMP

IP header length: 20 bytes

Total IP length: 28

Time to live: 64

Flag: 001

Fragment Offset: 4

Type: 8

Request or Reply: Request

Code: 8

Ethernet Frame 51:

Source MAC Address: 00-04-76-3B-0C-E7 Destination MAC Address: 00-E0-81-25-C0-8B Ether Type field: IPv4

Frame length : 60 Padding:

IP Packet:

Source IP Address: /192.168.1.32 Destination IP Address: /192.168.1.75

IP Version: 4 Protocol Type: ICMP

IP header length: 20 bytes

Total IP length: 28

Time to live: 64

Flag: 001

Fragment Offset: 0

Type: 8

Request or Reply: Request

Code: 8

Ethernet Frame 57:

Source MAC Address: 00-04-76-3B-0C-E7 Destination MAC Address: 00-E0-81-25-C0-8B Ether Type field: IPv4

Frame length : 60 Padding:

IP Packet:

Source IP Address: /192.168.1.32 Destination IP Address: /192.168.1.75

IP Version: 4 Protocol Type: ICMP

IP header length: 20 bytes

Total IP length: 28

Time to live: 64

Flag: 001

Fragment Offset: 3

Type: 0

Request or Reply: Reply

Code: 0

Ethernet Frame 58:

Source MAC Address: 00-04-76-3B-0C-E7 Destination MAC Address: 00-E0-81-25-C0-8B Ether Type field: IPv4

Frame length : 60 Padding:

IP Packet:

Source IP Address: /192.168.1.32 Destination IP Address: /192.168.1.75

IP Version: 4 Protocol Type: ICMP

IP header length: 20 bytes

Total IP length: 28

Time to live: 64

Flag: 001

Fragment Offset: 5

Type: 0

Request or Reply: Reply

Code: 0

Ethernet Frame 56:

Source MAC Address: 00-04-76-3B-0C-E7 Destination MAC Address: 00-E0-81-25-C0-8B Ether Type field: IPv4

Frame length : 60 Padding:

IP Packet:

Source IP Address: /192.168.1.32 Destination IP Address: /192.168.1.75

IP Version: 4 Protocol Type: ICMP

IP header length: 20 bytes

Total IP length: 28

Time to live: 64

Flag: 000

Fragment Offset: 7

Type: 0

Request or Reply: Reply

Code: 0

Ethernet Frame 55:

Source MAC Address: 00-04-76-3B-0C-E7 Destination MAC Address: 00-E0-81-25-C0-8B Ether Type field: IPv4

Frame length : 60 Padding:

IP Packet:

Source IP Address: /192.168.1.32 Destination IP Address: /192.168.1.75

IP Version: 4 Protocol Type: ICMP

IP header length: 20 bytes

Total IP length: 28

Time to live: 64

Flag: 001

Fragment Offset: 2

Type: 8

Request or Reply: Request

Code: 8

Ethernet Frame 59:

Source MAC Address: 00-04-76-3B-0C-E7 Destination MAC Address: 00-E0-81-25-C0-8B Ether Type field: IPv4

Frame length : 60 Padding:

IP Packet:

Source IP Address: /192.168.1.32 Destination IP Address: /192.168.1.75

IP Version: 4 Protocol Type: ICMP

IP header length: 20 bytes

Total IP length: 28

Time to live: 64

Flag: 001

Fragment Offset: 5

Type: 0

Request or Reply: Reply

Code: 0

Ethernet Frame 60:

Source MAC Address: 00-E0-81-25-C0-8B Destination MAC Address: 00-04-76-3B-0C-E7 Ether Type field: IPv4

Frame length : 98 Padding:

IP Packet:

Source IP Address: /192.168.1.75 Destination IP Address: /192.168.1.32

IP Version: 4 Protocol Type: ICMP

IP header length: 20 bytes

Total IP length: 84

Time to live: 128

Flag: 000

Fragment Offset: 0

Type: 0

Request or Reply: Reply

Code: 0

Ethernet Frame 61:

Source MAC Address: 00-04-76-3B-0C-E7 Destination MAC Address: 00-E0-81-25-C0-8B Ether Type field: IPv4

Frame length : 60 Padding:

IP Packet:

Source IP Address: /192.168.1.32 Destination IP Address: /192.168.1.75

IP Version: 4 Protocol Type: ICMP

IP header length: 20 bytes

Total IP length: 28

Time to live: 64

Flag: 001

Fragment Offset: 0

Type: 8

Request or Reply: Request

Code: 8

Ethernet Frame 63:

Source MAC Address: 00-04-76-3B-0C-E7 Destination MAC Address: 00-E0-81-25-C0-8B Ether Type field: IPv4

Frame length : 60 Padding:

IP Packet:

Source IP Address: /192.168.1.32 Destination IP Address: /192.168.1.75

IP Version: 4 Protocol Type: ICMP

IP header length: 20 bytes

Total IP length: 28

Time to live: 64

Flag: 001

Fragment Offset: 2

Type: 8

Request or Reply: Request

Code: 8

Ethernet Frame 62:

Source MAC Address: 00-04-76-3B-0C-E7 Destination MAC Address: 00-E0-81-25-C0-8B Ether Type field: IPv4

Frame length : 60 Padding:

IP Packet:

Source IP Address: /192.168.1.32 Destination IP Address: /192.168.1.75

IP Version: 4 Protocol Type: ICMP

IP header length: 20 bytes

Total IP length: 28

Time to live: 64

Flag: 001

Fragment Offset: 1

Type: 1

Request or Reply:

Code: 1

Ethernet Frame 64:

Source MAC Address: 00-04-76-3B-0C-E7 Destination MAC Address: 00-E0-81-25-C0-8B Ether Type field: IPv4

Frame length : 60 Padding:

IP Packet:

Source IP Address: /192.168.1.32 Destination IP Address: /192.168.1.75

IP Version: 4 Protocol Type: ICMP

IP header length: 20 bytes

Total IP length: 28

Time to live: 64

Flag: 001

Fragment Offset: 6

Type: 8

Request or Reply: Request

Code: 8

Ethernet Frame 69:

Source MAC Address: 00-04-76-3B-0C-E7 Destination MAC Address: 00-E0-81-25-C0-8B Ether Type field: IPv4

Frame length : 60 Padding:

IP Packet:

Source IP Address: /192.168.1.32 Destination IP Address: /192.168.1.75

IP Version: 4 Protocol Type: ICMP

IP header length: 20 bytes

Total IP length: 28

Time to live: 64

Flag: 001

Fragment Offset: 3

Type: 0

Request or Reply: Reply

Code: 0

Ethernet Frame 68:

Source MAC Address: 00-04-76-3B-0C-E7 Destination MAC Address: 00-E0-81-25-C0-8B Ether Type field: IPv4

Frame length : 60 Padding:

IP Packet:

Source IP Address: /192.168.1.32 Destination IP Address: /192.168.1.75

IP Version: 4 Protocol Type: ICMP

IP header length: 20 bytes

Total IP length: 28

Time to live: 64

Flag: 001

Fragment Offset: 5

Type: 0

Request or Reply: Reply

Code: 0

Ethernet Frame 67:

Source MAC Address: 00-04-76-3B-0C-E7 Destination MAC Address: 00-E0-81-25-C0-8B Ether Type field: IPv4

Frame length : 60 Padding:

IP Packet:

Source IP Address: /192.168.1.32 Destination IP Address: /192.168.1.75

IP Version: 4 Protocol Type: ICMP

IP header length: 20 bytes

Total IP length: 28

Time to live: 64

Flag: 001

Fragment Offset: 1

Type: 2

Request or Reply:

Code: 2

Ethernet Frame 66:

Source MAC Address: 00-E0-81-25-C0-8B Destination MAC Address: 00-04-76-3B-0C-E7 Ether Type field: IPv4

Frame length : 98 Padding:

IP Packet:

Source IP Address: /192.168.1.75 Destination IP Address: /192.168.1.32

IP Version: 4 Protocol Type: ICMP

IP header length: 20 bytes

Total IP length: 84

Time to live: 128

Flag: 000

Fragment Offset: 0

Type: 0

Request or Reply: Reply

Code: 0

Ethernet Frame 65:

Source MAC Address: 00-04-76-3B-0C-E7 Destination MAC Address: 00-E0-81-25-C0-8B Ether Type field: IPv4

Frame length : 60 Padding:

IP Packet:

Source IP Address: /192.168.1.32 Destination IP Address: /192.168.1.75

IP Version: 4 Protocol Type: ICMP

IP header length: 20 bytes

Total IP length: 28

Time to live: 64

Flag: 001

Fragment Offset: 3

Type: 0

Request or Reply: Reply

Code: 0

Ethernet Frame 70:

Source MAC Address: 00-04-76-3B-0C-E7 Destination MAC Address: 00-E0-81-25-C0-8B Ether Type field: IPv4

Frame length : 60 Padding:

IP Packet:

Source IP Address: /192.168.1.32 Destination IP Address: /192.168.1.75

IP Version: 4 Protocol Type: ICMP

IP header length: 20 bytes

Total IP length: 28

Time to live: 64

Flag: 001

Fragment Offset: 4

Type: 8

Request or Reply: Request

Code: 8

Ethernet Frame 71:

Source MAC Address: 00-04-76-3B-0C-E7 Destination MAC Address: 00-E0-81-25-C0-8B Ether Type field: IPv4

Frame length : 60 Padding:

IP Packet:

Source IP Address: /192.168.1.32 Destination IP Address: /192.168.1.75

IP Version: 4 Protocol Type: ICMP

IP header length: 20 bytes

Total IP length: 28

Time to live: 64

Flag: 000

Fragment Offset: 7

Type: 0

Request or Reply: Reply

Code: 0

Ethernet Frame 73:

Source MAC Address: 00-04-76-3B-0C-E7 Destination MAC Address: 00-E0-81-25-C0-8B Ether Type field: IPv4

Frame length : 60 Padding:

IP Packet:

Source IP Address: /192.168.1.32 Destination IP Address: /192.168.1.75

IP Version: 4 Protocol Type: ICMP

IP header length: 20 bytes

Total IP length: 28

Time to live: 64

Flag: 001

Fragment Offset: 0

Type: 8

Request or Reply: Request

Code: 8

Ethernet Frame 74:

Source MAC Address: 00-04-76-3B-0C-E7 Destination MAC Address: 00-E0-81-25-C0-8B Ether Type field: IPv4

Frame length : 60 Padding:

IP Packet:

Source IP Address: /192.168.1.32 Destination IP Address: /192.168.1.75

IP Version: 4 Protocol Type: ICMP

IP header length: 20 bytes

Total IP length: 28

Time to live: 64

Flag: 000

Fragment Offset: 7

Type: 0

Request or Reply: Reply

Code: 0

Ethernet Frame 75:

Source MAC Address: 00-04-76-3B-0C-E7 Destination MAC Address: 00-E0-81-25-C0-8B Ether Type field: IPv4

Frame length : 60 Padding:

IP Packet:

Source IP Address: /192.168.1.32 Destination IP Address: /192.168.1.75

IP Version: 4 Protocol Type: ICMP

IP header length: 20 bytes

Total IP length: 28

Time to live: 64

Flag: 001

Fragment Offset: 6

Type: 8

Request or Reply: Request

Code: 8

Ethernet Frame 72:

Source MAC Address: 00-04-76-3B-0C-E7 Destination MAC Address: 00-E0-81-25-C0-8B Ether Type field: IPv4

Frame length : 60 Padding:

IP Packet:

Source IP Address: /192.168.1.32 Destination IP Address: /192.168.1.75

IP Version: 4 Protocol Type: ICMP

IP header length: 20 bytes

Total IP length: 28

Time to live: 64

Flag: 001

Fragment Offset: 4

Type: 8

Request or Reply: Request

Code: 8

Ethernet Frame 73:

Source MAC Address: 00-04-76-3B-0C-E7 Destination MAC Address: 00-E0-81-25-C0-8B Ether Type field: IPv4

Frame length : 60 Padding:

IP Packet:

Source IP Address: /192.168.1.32 Destination IP Address: /192.168.1.75

IP Version: 4 Protocol Type: ICMP

IP header length: 20 bytes

Total IP length: 28

Time to live: 64

Flag: 001

Fragment Offset: 2

Type: 8

Request or Reply: Request

Code: 8

Ethernet Frame 76:

Source MAC Address: 00-04-76-3B-0C-E7 Destination MAC Address: 00-E0-81-25-C0-8B Ether Type field: IPv4

Frame length : 60 Padding:

IP Packet:

Source IP Address: /192.168.1.32 Destination IP Address: /192.168.1.75

IP Version: 4 Protocol Type: ICMP

IP header length: 20 bytes

Total IP length: 28

Time to live: 64

Flag: 001

Fragment Offset: 5

Type: 0

Request or Reply: Reply

Code: 0

Ethernet Frame 78:

Source MAC Address: 00-04-76-3B-0C-E7 Destination MAC Address: 00-E0-81-25-C0-8B Ether Type field: IPv4

Frame length : 60 Padding:

IP Packet:

Source IP Address: /192.168.1.32 Destination IP Address: /192.168.1.75

IP Version: 4 Protocol Type: ICMP

IP header length: 20 bytes

Total IP length: 28

Time to live: 64

Flag: 001

Fragment Offset: 2

Type: 8

Request or Reply: Request

Code: 8

Ethernet Frame 77:

Source MAC Address: 00-04-76-3B-0C-E7 Destination MAC Address: 00-E0-81-25-C0-8B Ether Type field: IPv4

Frame length : 60 Padding:

IP Packet:

Source IP Address: /192.168.1.32 Destination IP Address: /192.168.1.75

IP Version: 4 Protocol Type: ICMP

IP header length: 20 bytes

Total IP length: 28

Time to live: 64

Flag: 001

Fragment Offset: 3

Type: 0

Request or Reply: Reply

Code: 0

Ethernet Frame 79:

Source MAC Address: 00-E0-81-25-C0-8B Destination MAC Address: 00-04-76-3B-0C-E7 Ether Type field: IPv4

Frame length : 98 Padding:

IP Packet:

Source IP Address: /192.168.1.75 Destination IP Address: /192.168.1.32

IP Version: 4 Protocol Type: ICMP

IP header length: 20 bytes

Total IP length: 84

Time to live: 128

Flag: 000

Fragment Offset: 0

Type: 0

Request or Reply: Reply

Code: 0

Ethernet Frame 80:

Source MAC Address: 00-04-76-3B-0C-E7 Destination MAC Address: 00-E0-81-25-C0-8B Ether Type field: IPv4

Frame length : 60 Padding:

IP Packet:

Source IP Address: /192.168.1.32 Destination IP Address: /192.168.1.75

IP Version: 4 Protocol Type: ICMP

IP header length: 20 bytes

Total IP length: 28

Time to live: 64

Flag: 000

Fragment Offset: 7

Type: 0

Request or Reply: Reply

Code: 0

Ethernet Frame 86:

Source MAC Address: 00-04-76-3B-0C-E7 Destination MAC Address: 00-E0-81-25-C0-8B Ether Type field: IPv4

Frame length : 60 Padding:

IP Packet:

Source IP Address: /192.168.1.32 Destination IP Address: /192.168.1.75

IP Version: 4 Protocol Type: ICMP

IP header length: 20 bytes

Total IP length: 28

Time to live: 64

Flag: 001

Fragment Offset: 4

Type: 8

Request or Reply: Request

Code: 8

Ethernet Frame 85:

Source MAC Address: 00-04-76-3B-0C-E7 Destination MAC Address: 00-E0-81-25-C0-8B Ether Type field: IPv4

Frame length : 60 Padding:

IP Packet:

Source IP Address: /192.168.1.32 Destination IP Address: /192.168.1.75

IP Version: 4 Protocol Type: ICMP

IP header length: 20 bytes

Total IP length: 28

Time to live: 64

Flag: 001

Fragment Offset: 0

Type: 8

Request or Reply: Request

Code: 8

Ethernet Frame 84:

Source MAC Address: 00-04-76-3B-0C-E7 Destination MAC Address: 00-E0-81-25-C0-8B Ether Type field: IPv4

Frame length : 60 Padding:

IP Packet:

Source IP Address: /192.168.1.32 Destination IP Address: /192.168.1.75

IP Version: 4 Protocol Type: ICMP

IP header length: 20 bytes

Total IP length: 28

Time to live: 64

Flag: 001

Fragment Offset: 1

Type: 3

Request or Reply:

Code: 3

Ethernet Frame 83:

Source MAC Address: 00-E0-81-25-C0-8B Destination MAC Address: 00-04-76-3B-0C-E7 Ether Type field: IPv4

Frame length : 98 Padding:

IP Packet:

Source IP Address: /192.168.1.75 Destination IP Address: /192.168.1.32

IP Version: 4 Protocol Type: ICMP

IP header length: 20 bytes

Total IP length: 84

Time to live: 128

Flag: 000

Fragment Offset: 0

Type: 0

Request or Reply: Reply

Code: 0

Ethernet Frame 81:

Source MAC Address: 00-04-76-3B-0C-E7 Destination MAC Address: 00-E0-81-25-C0-8B Ether Type field: IPv4

Frame length : 60 Padding:

IP Packet:

Source IP Address: /192.168.1.32 Destination IP Address: /192.168.1.75

IP Version: 4 Protocol Type: ICMP

IP header length: 20 bytes

Total IP length: 28

Time to live: 64

Flag: 001

Fragment Offset: 0

Type: 8

Request or Reply: Request

Code: 8

Ethernet Frame 82:

Source MAC Address: 00-04-76-3B-0C-E7 Destination MAC Address: 00-E0-81-25-C0-8B Ether Type field: IPv4

Frame length : 60 Padding:

IP Packet:

Source IP Address: /192.168.1.32 Destination IP Address: /192.168.1.75

IP Version: 4 Protocol Type: ICMP

IP header length: 20 bytes

Total IP length: 28

Time to live: 64

Flag: 001

Fragment Offset: 4

Type: 8

Request or Reply: Request

Code: 8

Ethernet Frame 88:

Source MAC Address: 00-04-76-3B-0C-E7 Destination MAC Address: 00-E0-81-25-C0-8B Ether Type field: IPv4

Frame length : 60 Padding:

IP Packet:

Source IP Address: /192.168.1.32 Destination IP Address: /192.168.1.75

IP Version: 4 Protocol Type: ICMP

IP header length: 20 bytes

Total IP length: 28

Time to live: 64

Flag: 001

Fragment Offset: 6

Type: 8

Request or Reply: Request

Code: 8

Ethernet Frame 87:

Source MAC Address: 00-04-76-3B-0C-E7 Destination MAC Address: 00-E0-81-25-C0-8B Ether Type field: IPv4

Frame length : 60 Padding:

IP Packet:

Source IP Address: /192.168.1.32 Destination IP Address: /192.168.1.75

IP Version: 4 Protocol Type: ICMP

IP header length: 20 bytes

Total IP length: 28

Time to live: 64

Flag: 001

Fragment Offset: 6

Type: 8

Request or Reply: Request

Code: 8

Ethernet Frame 90:

Source MAC Address: 00-04-76-3B-0C-E7 Destination MAC Address: 00-E0-81-25-C0-8B Ether Type field: IPv4

Frame length : 60 Padding:

IP Packet:

Source IP Address: /192.168.1.32 Destination IP Address: /192.168.1.75

IP Version: 4 Protocol Type: ICMP

IP header length: 20 bytes

Total IP length: 28

Time to live: 64

Flag: 000

Fragment Offset: 7

Type: 0

Request or Reply: Reply

Code: 0

Ethernet Frame 91:

Source MAC Address: 00-04-76-3B-0C-E7 Destination MAC Address: 00-E0-81-25-C0-8B Ether Type field: IPv4

Frame length : 60 Padding:

IP Packet:

Source IP Address: /192.168.1.32 Destination IP Address: /192.168.1.75

IP Version: 4 Protocol Type: ICMP

IP header length: 20 bytes

Total IP length: 28

Time to live: 64

Flag: 001

Fragment Offset: 1

Type: 4

Request or Reply:

Code: 4

Ethernet Frame 89:

Source MAC Address: 00-04-76-3B-0C-E7 Destination MAC Address: 00-E0-81-25-C0-8B Ether Type field: IPv4

Frame length : 60 Padding:

IP Packet:

Source IP Address: /192.168.1.32 Destination IP Address: /192.168.1.75

IP Version: 4 Protocol Type: ICMP

IP header length: 20 bytes

Total IP length: 28

Time to live: 64

Flag: 001

Fragment Offset: 3

Type: 0

Request or Reply: Reply

Code: 0

Ethernet Frame 90:

Source MAC Address: 00-04-76-3B-0C-E7 Destination MAC Address: 00-E0-81-25-C0-8B Ether Type field: IPv4

Frame length : 60 Padding:

IP Packet:

Source IP Address: /192.168.1.32 Destination IP Address: /192.168.1.75

IP Version: 4 Protocol Type: ICMP

IP header length: 20 bytes

Total IP length: 28

Time to live: 64

Flag: 001

Fragment Offset: 5

Type: 0

Request or Reply: Reply

Code: 0

Ethernet Frame 92:

Source MAC Address: 00-04-76-3B-0C-E7 Destination MAC Address: 00-E0-81-25-C0-8B Ether Type field: IPv4

Frame length : 60 Padding:

IP Packet:

Source IP Address: /192.168.1.32 Destination IP Address: /192.168.1.75

IP Version: 4 Protocol Type: ICMP

IP header length: 20 bytes

Total IP length: 28

Time to live: 64

Flag: 001

Fragment Offset: 2

Type: 8

Request or Reply: Request

Code: 8

Ethernet Frame 93:

Source MAC Address: 00-04-76-3B-0C-E7 Destination MAC Address: 00-E0-81-25-C0-8B Ether Type field: IPv4

Frame length : 60 Padding:

IP Packet:

Source IP Address: /192.168.1.32 Destination IP Address: /192.168.1.75

IP Version: 4 Protocol Type: ICMP

IP header length: 20 bytes

Total IP length: 28

Time to live: 64

Flag: 001

Fragment Offset: 1

Type: 5

Request or Reply:

Code: 5

Ethernet Frame 95:

Source MAC Address: 00-04-76-3B-0C-E7 Destination MAC Address: 00-E0-81-25-C0-8B Ether Type field: IPv4

Frame length : 60 Padding:

IP Packet:

Source IP Address: /192.168.1.32 Destination IP Address: /192.168.1.75

IP Version: 4 Protocol Type: ICMP

IP header length: 20 bytes

Total IP length: 28

Time to live: 64

Flag: 001

Fragment Offset: 0

Type: 8

Request or Reply: Request

Code: 8

Ethernet Frame 94:

Source MAC Address: 00-04-76-3B-0C-E7 Destination MAC Address: 00-E0-81-25-C0-8B Ether Type field: IPv4

Frame length : 60 Padding:

IP Packet:

Source IP Address: /192.168.1.32 Destination IP Address: /192.168.1.75

IP Version: 4 Protocol Type: ICMP

IP header length: 20 bytes

Total IP length: 28

Time to live: 64

Flag: 001

Fragment Offset: 4

Type: 8

Request or Reply: Request

Code: 8

Ethernet Frame 96:

Source MAC Address: 00-E0-81-25-C0-8B Destination MAC Address: 00-04-76-3B-0C-E7 Ether Type field: IPv4

Frame length : 98 Padding:

IP Packet:

Source IP Address: /192.168.1.75 Destination IP Address: /192.168.1.32

IP Version: 4 Protocol Type: ICMP

IP header length: 20 bytes

Total IP length: 84

Time to live: 128

Flag: 000

Fragment Offset: 0

Type: 0

Request or Reply: Reply

Code: 0

Ethernet Frame 97:

Source MAC Address: 00-04-76-3B-0C-E7 Destination MAC Address: 00-E0-81-25-C0-8B Ether Type field: IPv4

Frame length : 60 Padding:

IP Packet:

Source IP Address: /192.168.1.32 Destination IP Address: /192.168.1.75

IP Version: 4 Protocol Type: ICMP

IP header length: 20 bytes

Total IP length: 28

Time to live: 64

Flag: 001

Fragment Offset: 3

Type: 0

Request or Reply: Reply

Code: 0

Ethernet Frame 100:

Source MAC Address: 00-04-76-3B-0C-E7 Destination MAC Address: 00-E0-81-25-C0-8B Ether Type field: IPv4

Frame length : 60 Padding:

IP Packet:

Source IP Address: /192.168.1.32 Destination IP Address: /192.168.1.75

IP Version: 4 Protocol Type: ICMP

IP header length: 20 bytes

Total IP length: 28

Time to live: 64

Flag: 000

Fragment Offset: 7

Type: 0

Request or Reply: Reply

Code: 0

Ethernet Frame 99:

Source MAC Address: 00-E0-81-25-C0-8B Destination MAC Address: 00-04-76-3B-0C-E7 Ether Type field: IPv4

Frame length : 98 Padding:

IP Packet:

Source IP Address: /192.168.1.75 Destination IP Address: /192.168.1.32

IP Version: 4 Protocol Type: ICMP

IP header length: 20 bytes

Total IP length: 84

Time to live: 128

Flag: 000

Fragment Offset: 0

Type: 0

Request or Reply: Reply

Code: 0

Ethernet Frame 103:

Source MAC Address: 00-04-76-3B-0C-E7 Destination MAC Address: 00-E0-81-25-C0-8B Ether Type field: IPv4

Frame length : 60 Padding:

IP Packet:

Source IP Address: /192.168.1.32 Destination IP Address: /192.168.1.75

IP Version: 4 Protocol Type: ICMP

IP header length: 20 bytes

Total IP length: 28

Time to live: 64

Flag: 001

Fragment Offset: 5

Type: 0

Request or Reply: Reply

Code: 0

Ethernet Frame 102:

Source MAC Address: 00-04-76-3B-0C-E7 Destination MAC Address: 00-E0-81-25-C0-8B Ether Type field: IPv4

Frame length : 60 Padding:

IP Packet:

Source IP Address: /192.168.1.32 Destination IP Address: /192.168.1.75

IP Version: 4 Protocol Type: ICMP

IP header length: 20 bytes

Total IP length: 28

Time to live: 64

Flag: 001

Fragment Offset: 6

Type: 8

Request or Reply: Request

Code: 8

Ethernet Frame 101:

Source MAC Address: 00-04-76-3B-0C-E7 Destination MAC Address: 00-E0-81-25-C0-8B Ether Type field: IPv4

Frame length : 60 Padding:

IP Packet:

Source IP Address: /192.168.1.32 Destination IP Address: /192.168.1.75

IP Version: 4 Protocol Type: ICMP

IP header length: 20 bytes

Total IP length: 28

Time to live: 64

Flag: 001

Fragment Offset: 4

Type: 8

Request or Reply: Request

Code: 8

Ethernet Frame 98:

Source MAC Address: 00-04-76-3B-0C-E7 Destination MAC Address: 00-E0-81-25-C0-8B Ether Type field: IPv4

Frame length : 60 Padding:

IP Packet:

Source IP Address: /192.168.1.32 Destination IP Address: /192.168.1.75

IP Version: 4 Protocol Type: ICMP

IP header length: 20 bytes

Total IP length: 28

Time to live: 64

Flag: 001

Fragment Offset: 2

Type: 8

Request or Reply: Request

Code: 8

Ethernet Frame 104:

Source MAC Address: 00-04-76-3B-0C-E7 Destination MAC Address: 00-E0-81-25-C0-8B Ether Type field: IPv4

Frame length : 60 Padding:

IP Packet:

Source IP Address: /192.168.1.32 Destination IP Address: /192.168.1.75

IP Version: 4 Protocol Type: ICMP

IP header length: 20 bytes

Total IP length: 28

Time to live: 64

Flag: 000

Fragment Offset: 7

Type: 0

Request or Reply: Reply

Code: 0

Ethernet Frame 106:

Source MAC Address: 00-04-76-3B-0C-E7 Destination MAC Address: 00-E0-81-25-C0-8B Ether Type field: IPv4

Frame length : 60 Padding:

IP Packet:

Source IP Address: /192.168.1.32 Destination IP Address: /192.168.1.75

IP Version: 4 Protocol Type: ICMP

IP header length: 20 bytes

Total IP length: 28

Time to live: 64

Flag: 001

Fragment Offset: 2

Type: 8

Request or Reply: Request

Code: 8

Ethernet Frame 105:

Source MAC Address: 00-04-76-3B-0C-E7 Destination MAC Address: 00-E0-81-25-C0-8B Ether Type field: IPv4

Frame length : 60 Padding:

IP Packet:

Source IP Address: /192.168.1.32 Destination IP Address: /192.168.1.75

IP Version: 4 Protocol Type: ICMP

IP header length: 20 bytes

Total IP length: 28

Time to live: 64

Flag: 001

Fragment Offset: 5

Type: 0

Request or Reply: Reply

Code: 0

Ethernet Frame 107:

Source MAC Address: 00-04-76-3B-0C-E7 Destination MAC Address: 00-E0-81-25-C0-8B Ether Type field: IPv4

Frame length : 60 Padding:

IP Packet:

Source IP Address: /192.168.1.32 Destination IP Address: /192.168.1.75

IP Version: 4 Protocol Type: ICMP

IP header length: 20 bytes

Total IP length: 28

Time to live: 64

Flag: 001

Fragment Offset: 1

Type: 6

Request or Reply:

Code: 6

Ethernet Frame 109:

Source MAC Address: 00-04-76-3B-0C-E7 Destination MAC Address: 00-E0-81-25-C0-8B Ether Type field: IPv4

Frame length : 60 Padding:

IP Packet:

Source IP Address: /192.168.1.32 Destination IP Address: /192.168.1.75

IP Version: 4 Protocol Type: ICMP

IP header length: 20 bytes

Total IP length: 28

Time to live: 64

Flag: 001

Fragment Offset: 0

Type: 8

Request or Reply: Request

Code: 8

Ethernet Frame 110:

Source MAC Address: 00-E0-81-25-C0-8B Destination MAC Address: 00-04-76-3B-0C-E7 Ether Type field: IPv4

Frame length : 98 Padding:

IP Packet:

Source IP Address: /192.168.1.75 Destination IP Address: /192.168.1.32

IP Version: 4 Protocol Type: ICMP

IP header length: 20 bytes

Total IP length: 84

Time to live: 128

Flag: 000

Fragment Offset: 0

Type: 0

Request or Reply: Reply

Code: 0

Ethernet Frame 108:

Source MAC Address: 00-04-76-3B-0C-E7 Destination MAC Address: 00-E0-81-25-C0-8B Ether Type field: IPv4

Frame length : 60 Padding:

IP Packet:

Source IP Address: /192.168.1.32 Destination IP Address: /192.168.1.75

IP Version: 4 Protocol Type: ICMP

IP header length: 20 bytes

Total IP length: 28

Time to live: 64

Flag: 001

Fragment Offset: 6

Type: 8

Request or Reply: Request

Code: 8

Ethernet Frame 112:

Source MAC Address: 00-04-76-3B-0C-E7 Destination MAC Address: 00-E0-81-25-C0-8B Ether Type field: IPv4

Frame length : 60 Padding:

IP Packet:

Source IP Address: /192.168.1.32 Destination IP Address: /192.168.1.75

IP Version: 4 Protocol Type: ICMP

IP header length: 20 bytes

Total IP length: 28

Time to live: 64

Flag: 001

Fragment Offset: 2

Type: 8

Request or Reply: Request

Code: 8

Ethernet Frame 111:

Source MAC Address: 00-04-76-3B-0C-E7 Destination MAC Address: 00-E0-81-25-C0-8B Ether Type field: IPv4

Frame length : 60 Padding:

IP Packet:

Source IP Address: /192.168.1.32 Destination IP Address: /192.168.1.75

IP Version: 4 Protocol Type: ICMP

IP header length: 20 bytes

Total IP length: 28

Time to live: 64

Flag: 001

Fragment Offset: 3

Type: 0

Request or Reply: Reply

Code: 0

Ethernet Frame 113:

Source MAC Address: 00-04-76-3B-0C-E7 Destination MAC Address: 00-E0-81-25-C0-8B Ether Type field: IPv4

Frame length : 60 Padding:

IP Packet:

Source IP Address: /192.168.1.32 Destination IP Address: /192.168.1.75

IP Version: 4 Protocol Type: ICMP

IP header length: 20 bytes

Total IP length: 28

Time to live: 64

Flag: 001

Fragment Offset: 4

Type: 8

Request or Reply: Request

Code: 8

Ethernet Frame 115:

Source MAC Address: 00-04-76-3B-0C-E7 Destination MAC Address: 00-E0-81-25-C0-8B Ether Type field: IPv4

Frame length : 60 Padding:

IP Packet:

Source IP Address: /192.168.1.32 Destination IP Address: /192.168.1.75

IP Version: 4 Protocol Type: ICMP

IP header length: 20 bytes

Total IP length: 28

Time to live: 64

Flag: 001

Fragment Offset: 1

Type: 7

Request or Reply:

Code: 7

Ethernet Frame 114:

Source MAC Address: 00-04-76-3B-0C-E7 Destination MAC Address: 00-E0-81-25-C0-8B Ether Type field: IPv4

Frame length : 60 Padding:

IP Packet:

Source IP Address: /192.168.1.32 Destination IP Address: /192.168.1.75

IP Version: 4 Protocol Type: ICMP

IP header length: 20 bytes

Total IP length: 28

Time to live: 64

Flag: 001

Fragment Offset: 0

Type: 8

Request or Reply: Request

Code: 8

Ethernet Frame 116:

Source MAC Address: 00-04-76-3B-0C-E7 Destination MAC Address: 00-E0-81-25-C0-8B Ether Type field: IPv4

Frame length : 60 Padding:

IP Packet:

Source IP Address: /192.168.1.32 Destination IP Address: /192.168.1.75

IP Version: 4 Protocol Type: ICMP

IP header length: 20 bytes

Total IP length: 28

Time to live: 64

Flag: 001

Fragment Offset: 6

Type: 8

Request or Reply: Request

Code: 8

Ethernet Frame 119:

Source MAC Address: 00-04-76-3B-0C-E7 Destination MAC Address: 00-E0-81-25-C0-8B Ether Type field: IPv4

Frame length : 60 Padding:

IP Packet:

Source IP Address: /192.168.1.32 Destination IP Address: /192.168.1.75

IP Version: 4 Protocol Type: ICMP

IP header length: 20 bytes

Total IP length: 28

Time to live: 64

Flag: 001

Fragment Offset: 5

Type: 0

Request or Reply: Reply

Code: 0

Ethernet Frame 118:

Source MAC Address: 00-04-76-3B-0C-E7 Destination MAC Address: 00-E0-81-25-C0-8B Ether Type field: IPv4

Frame length : 60 Padding:

IP Packet:

Source IP Address: /192.168.1.32 Destination IP Address: /192.168.1.75

IP Version: 4 Protocol Type: ICMP

IP header length: 20 bytes

Total IP length: 28

Time to live: 64

Flag: 000

Fragment Offset: 7

Type: 0

Request or Reply: Reply

Code: 0

Ethernet Frame 117:

Source MAC Address: 00-E0-81-25-C0-8B Destination MAC Address: 00-04-76-3B-0C-E7 Ether Type field: IPv4

Frame length : 98 Padding:

IP Packet:

Source IP Address: /192.168.1.75 Destination IP Address: /192.168.1.32

IP Version: 4 Protocol Type: ICMP

IP header length: 20 bytes

Total IP length: 84

Time to live: 128

Flag: 000

Fragment Offset: 0

Type: 0

Request or Reply: Reply

Code: 0

Ethernet Frame 120:

Source MAC Address: 00-04-76-3B-0C-E7 Destination MAC Address: 00-E0-81-25-C0-8B Ether Type field: IPv4

Frame length : 60 Padding:

IP Packet:

Source IP Address: /192.168.1.32 Destination IP Address: /192.168.1.75

IP Version: 4 Protocol Type: ICMP

IP header length: 20 bytes

Total IP length: 28

Time to live: 64

Flag: 001

Fragment Offset: 3

Type: 0

Request or Reply: Reply

Code: 0

Ethernet Frame 121:

Source MAC Address: 00-C0-4F-58-D9-94 Destination MAC Address: 00-C0-4F-8D-93-CC Ether Type field: ARP

Frame length : 60 Padding:

Packet Type: ARP

Hardware Type: Ethernet 1

Protocol Type: IPv4

Hardware size: 6

Protocol size: 4

Opcode : Reply (2)

Sender MAC Address: 00-C0-4F-58-D9-94

Sender IP Address: /192.168.1.203

Target MAC Address: 00-C0-4F-8D-93-CC

Target IP Address: /192.168.1.200

Ethernet Frame 122:

Source MAC Address: 00-C0-4F-8D-93-CC Destination MAC Address: FF-FF-FF-FF-FF-FF Ether Type field: ARP

Frame length : 60 Padding:

Packet Type: ARP

Hardware Type: Ethernet 1

Protocol Type: IPv4

Hardware size: 6

Protocol size: 4

Opcode : Request (1)

Sender MAC Address: 00-C0-4F-8D-93-CC

Sender IP Address: /192.168.1.203

Target MAC Address: 00-00-00-00-00-00

Target IP Address: /192.168.1.200

Ethernet Frame 123:

Source MAC Address: 00-C0-4F-8D-93-F2 Destination MAC Address: 00-C0-4F-8D-99-31 Ether Type field: IPv4

Frame length : 82 Padding:

IP Packet:

Source IP Address: /192.168.1.66 Destination IP Address: /192.168.1.14

IP Version: 4 Protocol Type: UDP

IP header length: 20 bytes

Total IP length: 68

Time to live: 64

Flag: 010

Fragment Offset: 0

UDP Datagram.

Source Port: 34808 Destination Port: 53

UDP Length: 48

UDP Data Length: 40

UDP Data: E6 0D 01 00 00 01 00 00 00 00 00 00 06 69 6F 64 .............iod

69 6E 65 04 73 73 61 63 06 75 74 75 6C 73 61 03 ine.ssac.utulsa.

65 64 75 00 00 01 00 01 edu.....

Ethernet Frame 124:

Source MAC Address: 00-C0-4F-8D-99-31 Destination MAC Address: 00-C0-4F-8D-93-F2 Ether Type field: IPv4

Frame length : 134 Padding:

IP Packet:

Source IP Address: /192.168.1.14 Destination IP Address: /192.168.1.66

IP Version: 4 Protocol Type: UDP

IP header length: 20 bytes

Total IP length: 120

Time to live: 64

Flag: 010

Fragment Offset: 0

UDP Datagram.

Source Port: 53 Destination Port: 34808

UDP Length: 100

UDP Data Length: 92

UDP Data: E6 0D 85 80 00 01 00 01 00 01 00 01 06 69 6F 64 .............iod

69 6E 65 04 73 73 61 63 06 75 74 75 6C 73 61 03 ine.ssac.utulsa.

65 64 75 00 00 01 00 01 C0 0C 00 01 00 01 00 01 edu.............

51 80 00 04 C0 A8 01 3E C0 13 00 02 00 01 00 01 Q......>........

51 80 00 08 05 62 6F 72 6F 6E C0 13 C0 44 00 01 Q....boron...D..

00 01 00 01 51 80 00 04 C0 A8 01 0E ....Q.......

Ethernet Frame 125:

Source MAC Address: 08-00-20-AB-D4-A4 Destination MAC Address: 00-C0-4F-58-D9-94 Ether Type field: IPv4

Frame length : 91 Padding:

IP Packet:

Source IP Address: /192.168.1.22 Destination IP Address: /192.168.1.46

IP Version: 4 Protocol Type: UDP

IP header length: 20 bytes

Total IP length: 77

Time to live: 255

Flag: 010

Fragment Offset: 0

UDP Datagram.

Source Port: 52578 Destination Port: 53

UDP Length: 57

UDP Data Length: 49

UDP Data: E0 42 01 00 00 01 00 00 00 00 00 00 08 68 79 64 .B...........hyd

72 6F 67 65 6E 06 67 72 6F 75 70 31 04 73 73 61 rogen.group1.ssa

63 06 75 74 75 6C 73 61 03 65 64 75 00 00 01 00 c.utulsa.edu....

01 .

Ethernet Frame 126:

Source MAC Address: 00-C0-4F-58-D9-94 Destination MAC Address: 08-00-20-AB-D4-A4 Ether Type field: IPv4

Frame length : 107 Padding:

IP Packet:

Source IP Address: /192.168.1.46 Destination IP Address: /192.168.1.22

IP Version: 4 Protocol Type: UDP

IP header length: 20 bytes

Total IP length: 93

Time to live: 128

Flag: 000

Fragment Offset: 0

UDP Datagram.

Source Port: 53 Destination Port: 52578

UDP Length: 73

UDP Data Length: 65

UDP Data: E0 42 85 80 00 01 00 01 00 00 00 00 08 68 79 64 .B...........hyd

72 6F 67 65 6E 06 67 72 6F 75 70 31 04 73 73 61 rogen.group1.ssa

63 06 75 74 75 6C 73 61 03 65 64 75 00 00 01 00 c.utulsa.edu....

01 C0 0C 00 01 00 01 00 00 0E 10 00 04 C0 A8 01 ................

0A .

Ethernet Frame 128:

Source MAC Address: 00-60-97-B9-58-7D Destination MAC Address: 00-C0-4F-49-D8-25 Ether Type field: IPv4

Frame length : 66 Padding:

IP Packet:

Source IP Address: /192.168.1.62 Destination IP Address: /192.168.1.42

IP Version: 4 Protocol Type: TCP

IP header length: 20 bytes

Total IP length: 52

Time to live: 64

Flag: 010

Fragment Offset: 0

TCP Segment:

Source Port: 4938 Destination Port: 21

Sequence Number: 708153374 Acknowledgment number: 4221341147

TCP Header Length: 32 bytes

Window Size: 5840

Flag: ACK

Urgent Pointer: 0

Option Field: 12

TCP Payload size: 0 bytes

TCP Payload type: FTP

Data: No payload

Ethernet Frame 130:

Source MAC Address: 00-C0-4F-49-D8-25 Destination MAC Address: 00-60-97-B9-58-7D Ether Type field: IPv4

Frame length : 227 Padding:

IP Packet:

Source IP Address: /192.168.1.42 Destination IP Address: /192.168.1.62

IP Version: 4 Protocol Type: TCP

IP header length: 20 bytes

Total IP length: 213

Time to live: 64

Flag: 010

Fragment Offset: 0

TCP Segment:

Source Port: 4938 Destination Port: 21

Sequence Number: 4221341147 Acknowledgment number: 708153374

TCP Header Length: 32 bytes

Window Size: 5792

Flag: (PSH, ACK)

Urgent Pointer: 0

Option Field: 12

TCP Payload size: 161 bytes

TCP Payload type: FTP

Data: 32 32 30 20 4E 4F 20 4F 4E 45 20 49 53 20 41 4C 220 NO ONE IS AL

4C 4F 57 45 44 20 54 4F 20 55 53 45 20 54 48 49 LOWED TO USE THI

53 20 53 45 52 56 45 52 2E 20 41 43 54 49 56 49 S SERVER. ACTIVI

54 49 45 53 20 57 49 4C 4C 20 42 45 20 4D 4F 4E TIES WILL BE MON

49 54 4F 52 45 44 20 42 59 20 41 20 54 48 4F 55 ITORED BY A THOU

53 41 4E 44 20 44 4F 47 53 20 46 52 4F 4D 20 48 SAND DOGS FROM H

45 4C 4C 2E 20 55 4E 41 55 54 48 4F 52 49 5A 45 ELL. UNAUTHORIZE

44 20 41 43 43 45 53 53 20 57 49 4C 4C 20 42 45 D ACCESS WILL BE

20 48 41 52 53 48 4C 59 20 50 55 4E 49 53 48 45 HARSHLY PUNISHE

44 20 42 59 20 53 41 49 44 20 44 4F 47 53 2E 0D D BY SAID DOGS..

0A .

Ethernet Frame 129:

Source MAC Address: 00-60-97-B9-58-7D Destination MAC Address: 00-C0-4F-49-D8-25 Ether Type field: IPv4

Frame length : 66 Padding:

IP Packet:

Source IP Address: /192.168.1.62 Destination IP Address: /192.168.1.42

IP Version: 4 Protocol Type: TCP

IP header length: 20 bytes

Total IP length: 52

Time to live: 64

Flag: 010

Fragment Offset: 0

TCP Segment:

Source Port: 4938 Destination Port: 21

Sequence Number: 708153374 Acknowledgment number: 4221341308

TCP Header Length: 32 bytes

Window Size: 5840

Flag: ACK

Urgent Pointer: 0

Option Field: 12

TCP Payload size: 0 bytes

TCP Payload type: FTP

Data: No payload

Ethernet Frame 127:

Source MAC Address: 00-60-97-B9-58-7D Destination MAC Address: 00-C0-4F-49-D8-25 Ether Type field: IPv4

Frame length : 74 Padding:

IP Packet:

Source IP Address: /192.168.1.62 Destination IP Address: /192.168.1.42

IP Version: 4 Protocol Type: TCP

IP header length: 20 bytes

Total IP length: 60

Time to live: 64

Flag: 010

Fragment Offset: 0

TCP Segment:

Source Port: 4938 Destination Port: 21

Sequence Number: 708153373 Acknowledgment number: 0

TCP Header Length: 40 bytes

Window Size: 5840

Flag: SYN

Urgent Pointer: 0

Option Field: 20

TCP Payload size: 0 bytes

TCP Payload type: FTP

Data: No payload

Ethernet Frame 127:

Source MAC Address: 00-C0-4F-49-D8-25 Destination MAC Address: 00-60-97-B9-58-7D Ether Type field: IPv4

Frame length : 74 Padding:

IP Packet:

Source IP Address: /192.168.1.42 Destination IP Address: /192.168.1.62

IP Version: 4 Protocol Type: TCP

IP header length: 20 bytes

Total IP length: 60

Time to live: 64

Flag: 010

Fragment Offset: 0

TCP Segment:

Source Port: 4938 Destination Port: 21

Sequence Number: 4221341146 Acknowledgment number: 708153374

TCP Header Length: 40 bytes

Window Size: 5792

Flag: (SYN, ACK)

Urgent Pointer: 0

Option Field: 20

TCP Payload size: 0 bytes

TCP Payload type: FTP

Data: No payload

Ethernet Frame 133:

Source MAC Address: 00-C0-4F-49-D8-25 Destination MAC Address: 00-60-97-B9-58-7D Ether Type field: IPv4

Frame length : 104 Padding:

IP Packet:

Source IP Address: /192.168.1.42 Destination IP Address: /192.168.1.62

IP Version: 4 Protocol Type: TCP

IP header length: 20 bytes

Total IP length: 90

Time to live: 64

Flag: 010

Fragment Offset: 0

TCP Segment:

Source Port: 21 Destination Port: 4938

Sequence Number: 4221341308 Acknowledgment number: 708153384

TCP Header Length: 32 bytes

Window Size: 5792

Flag: (PSH, ACK)

Urgent Pointer: 0

Option Field: 12

TCP Payload size: 38 bytes

TCP Payload type: FTP

Data: 35 33 30 20 50 6C 65 61 73 65 20 6C 6F 67 69 6E 530 Please login

20 77 69 74 68 20 55 53 45 52 20 61 6E 64 20 50 with USER and P

41 53 53 2E 0D 0A ASS...

Ethernet Frame 131:

Source MAC Address: 00-60-97-B9-58-7D Destination MAC Address: 00-C0-4F-49-D8-25 Ether Type field: IPv4

Frame length : 76 Padding:

IP Packet:

Source IP Address: /192.168.1.62 Destination IP Address: /192.168.1.42

IP Version: 4 Protocol Type: TCP

IP header length: 20 bytes

Total IP length: 62

Time to live: 64

Flag: 010

Fragment Offset: 0

TCP Segment:

Source Port: 21 Destination Port: 4938

Sequence Number: 708153374 Acknowledgment number: 4221341308

TCP Header Length: 32 bytes

Window Size: 5840

Flag: (PSH, ACK)

Urgent Pointer: 0

Option Field: 12

TCP Payload size: 10 bytes

TCP Payload type: FTP

Data: 41 55 54 48 20 53 53 4C 0D 0A AUTH SSL..

Ethernet Frame 132:

Source MAC Address: 00-C0-4F-49-D8-25 Destination MAC Address: 00-60-97-B9-58-7D Ether Type field: IPv4

Frame length : 66 Padding:

IP Packet:

Source IP Address: /192.168.1.42 Destination IP Address: /192.168.1.62

IP Version: 4 Protocol Type: TCP

IP header length: 20 bytes

Total IP length: 52

Time to live: 64

Flag: 010

Fragment Offset: 0

TCP Segment:

Source Port: 21 Destination Port: 4938

Sequence Number: 4221341308 Acknowledgment number: 708153384

TCP Header Length: 32 bytes

Window Size: 5792

Flag: ACK

Urgent Pointer: 0

Option Field: 12

TCP Payload size: 0 bytes

TCP Payload type: FTP

Data: No payload

Ethernet Frame 134:

Source MAC Address: 00-60-97-B9-58-7D Destination MAC Address: 00-C0-4F-49-D8-25 Ether Type field: IPv4

Frame length : 80 Padding:

IP Packet:

Source IP Address: /192.168.1.62 Destination IP Address: /192.168.1.42

IP Version: 4 Protocol Type: TCP

IP header length: 20 bytes

Total IP length: 66

Time to live: 64

Flag: 010

Fragment Offset: 0

TCP Segment:

Source Port: 21 Destination Port: 4938

Sequence Number: 708153384 Acknowledgment number: 4221341346

TCP Header Length: 32 bytes

Window Size: 5840

Flag: (PSH, ACK)

Urgent Pointer: 0

Option Field: 12

TCP Payload size: 14 bytes

TCP Payload type: other

Data: 55 53 45 52 20 67 72 6F 75 70 31 34 0D 0A USER group14..

Ethernet Frame 136:

Source MAC Address: 00-C0-4F-49-D8-25 Destination MAC Address: 00-60-97-B9-58-7D Ether Type field: IPv4

Frame length : 100 Padding:

IP Packet:

Source IP Address: /192.168.1.42 Destination IP Address: /192.168.1.62

IP Version: 4 Protocol Type: TCP

IP header length: 20 bytes

Total IP length: 86

Time to live: 64

Flag: 010

Fragment Offset: 0

TCP Segment:

Source Port: 21 Destination Port: 4938

Sequence Number: 4221341346 Acknowledgment number: 708153398

TCP Header Length: 32 bytes

Window Size: 5792

Flag: (PSH, ACK)

Urgent Pointer: 0

Option Field: 12

TCP Payload size: 34 bytes

TCP Payload type: FTP

Data: 33 33 31 20 50 6C 65 61 73 65 20 73 70 65 63 69 331 Please speci

66 79 20 74 68 65 20 70 61 73 73 77 6F 72 64 2E fy the password.

0D 0A ..

Ethernet Frame 135:

Source MAC Address: 00-60-97-B9-58-7D Destination MAC Address: 00-C0-4F-49-D8-25 Ether Type field: IPv4

Frame length : 85 Padding:

IP Packet:

Source IP Address: /192.168.1.62 Destination IP Address: /192.168.1.42

IP Version: 4 Protocol Type: TCP

IP header length: 20 bytes

Total IP length: 71

Time to live: 64

Flag: 010

Fragment Offset: 0

TCP Segment:

Source Port: 21 Destination Port: 4938

Sequence Number: 708153398 Acknowledgment number: 4221341380

TCP Header Length: 32 bytes

Window Size: 5840

Flag: (PSH, ACK)

Urgent Pointer: 0

Option Field: 12

TCP Payload size: 19 bytes

TCP Payload type: other

Data: 50 41 53 53 20 31 39 32 2E 31 36 38 2E 31 2E 36 PASS 192.168.1.6

32 0D 0A 2..

Ethernet Frame 137:

Source MAC Address: 00-60-97-B9-58-7D Destination MAC Address: 00-C0-4F-49-D8-25 Ether Type field: IPv4

Frame length : 74 Padding:

IP Packet:

Source IP Address: /192.168.1.62 Destination IP Address: /192.168.1.42

IP Version: 4 Protocol Type: TCP

IP header length: 20 bytes

Total IP length: 60

Time to live: 64

Flag: 010

Fragment Offset: 0

TCP Segment:

Source Port: 4938 Destination Port: 4938

Sequence Number: 708153417 Acknowledgment number: 4221341413

TCP Header Length: 32 bytes

Window Size: 5840

Flag: (PSH, ACK)

Urgent Pointer: 0

Option Field: 12

TCP Payload size: 8 bytes

TCP Payload type: other

Data: 54 59 50 45 20 41 0D 0A TYPE A..

Ethernet Frame 140:

Source MAC Address: 00-60-97-B9-58-7D Destination MAC Address: 00-C0-4F-49-D8-25 Ether Type field: IPv4

Frame length : 91 Padding:

IP Packet:

Source IP Address: /192.168.1.62 Destination IP Address: /192.168.1.42

IP Version: 4 Protocol Type: TCP

IP header length: 20 bytes

Total IP length: 77

Time to live: 64

Flag: 010

Fragment Offset: 0

TCP Segment:

Source Port: 4938 Destination Port: 4938

Sequence Number: 708153425 Acknowledgment number: 4221341443

TCP Header Length: 32 bytes

Window Size: 5840

Flag: (PSH, ACK)

Urgent Pointer: 0

Option Field: 12

TCP Payload size: 25 bytes

TCP Payload type: other

Data: 50 4F 52 54 20 31 39 32 2C 31 36 38 2C 31 2C 36 PORT 192,168,1,6

32 2C 31 39 2C 37 36 0D 0A 2,19,76..

Ethernet Frame 139:

Source MAC Address: 00-C0-4F-49-D8-25 Destination MAC Address: 00-60-97-B9-58-7D Ether Type field: IPv4

Frame length : 117 Padding:

IP Packet:

Source IP Address: /192.168.1.42 Destination IP Address: /192.168.1.62

IP Version: 4 Protocol Type: TCP

IP header length: 20 bytes

Total IP length: 103

Time to live: 64

Flag: 010

Fragment Offset: 0

TCP Segment:

Source Port: 4938 Destination Port: 4938

Sequence Number: 4221341443 Acknowledgment number: 708153450

TCP Header Length: 32 bytes

Window Size: 5792

Flag: (PSH, ACK)

Urgent Pointer: 0

Option Field: 12

TCP Payload size: 51 bytes

TCP Payload type: FTP

Data: 32 30 30 20 50 4F 52 54 20 63 6F 6D 6D 61 6E 64 200 PORT command

20 73 75 63 63 65 73 73 66 75 6C 2E 20 43 6F 6E successful. Con

73 69 64 65 72 20 75 73 69 6E 67 20 50 41 53 56 sider using PASV

2E 0D 0A ...

Ethernet Frame 138:

Source MAC Address: 00-C0-4F-49-D8-25 Destination MAC Address: 00-60-97-B9-58-7D Ether Type field: IPv4

Frame length : 96 Padding:

IP Packet:

Source IP Address: /192.168.1.42 Destination IP Address: /192.168.1.62

IP Version: 4 Protocol Type: TCP

IP header length: 20 bytes

Total IP length: 82

Time to live: 64

Flag: 010

Fragment Offset: 0

TCP Segment:

Source Port: 4938 Destination Port: 4938

Sequence Number: 4221341413 Acknowledgment number: 708153425

TCP Header Length: 32 bytes

Window Size: 5792

Flag: (PSH, ACK)

Urgent Pointer: 0

Option Field: 12

TCP Payload size: 30 bytes

TCP Payload type: FTP

Data: 32 30 30 20 53 77 69 74 63 68 69 6E 67 20 74 6F 200 Switching to

20 41 53 43 49 49 20 6D 6F 64 65 2E 0D 0A ASCII mode...

Ethernet Frame 149:

Source MAC Address: 00-C0-4F-49-D8-25 Destination MAC Address: 00-60-97-B9-58-7D Ether Type field: IPv4

Frame length : 66 Padding:

IP Packet:

Source IP Address: /192.168.1.42 Destination IP Address: /192.168.1.62

IP Version: 4 Protocol Type: TCP

IP header length: 20 bytes

Total IP length: 52

Time to live: 64

Flag: 010

Fragment Offset: 0

TCP Segment:

Source Port: 20 Destination Port: 4940

Sequence Number: 4221101711 Acknowledgment number: 709020036

TCP Header Length: 32 bytes

Window Size: 5840

Flag: ACK

Urgent Pointer: 0

Option Field: 12

TCP Payload size: 0 bytes

TCP Payload type: other

Data: No payload

Ethernet Frame 148:

Source MAC Address: 00-C0-4F-49-D8-25 Destination MAC Address: 00-60-97-B9-58-7D Ether Type field: IPv4

Frame length : 88 Padding:

IP Packet:

Source IP Address: /192.168.1.42 Destination IP Address: /192.168.1.62

IP Version: 4 Protocol Type: TCP

IP header length: 20 bytes

Total IP length: 74

Time to live: 64

Flag: 010

Fragment Offset: 0

TCP Segment:

Source Port: 20 Destination Port: 4940

Sequence Number: 4221341494 Acknowledgment number: 708153472

TCP Header Length: 32 bytes

Window Size: 5792

Flag: (PSH, ACK)

Urgent Pointer: 0

Option Field: 12

TCP Payload size: 22 bytes

TCP Payload type: FTP

Data: 31 35 30 20 4F 6B 20 74 6F 20 73 65 6E 64 20 64 150 Ok to send d

61 74 61 2E 0D 0A ata...

Ethernet Frame 147:

Source MAC Address: 00-C0-4F-49-D8-25 Destination MAC Address: 00-60-97-B9-58-7D Ether Type field: IPv4

Frame length : 66 Padding:

IP Packet:

Source IP Address: /192.168.1.42 Destination IP Address: /192.168.1.62

IP Version: 4 Protocol Type: TCP

IP header length: 20 bytes

Total IP length: 52

Time to live: 64

Flag: 010

Fragment Offset: 0

TCP Segment:

Source Port: 20 Destination Port: 4940

Sequence Number: 4221101711 Acknowledgment number: 709020621

TCP Header Length: 32 bytes

Window Size: 6435

Flag: ACK

Urgent Pointer: 0

Option Field: 12

TCP Payload size: 0 bytes

TCP Payload type: other

Data: No payload

Ethernet Frame 146:

Source MAC Address: 00-C0-4F-49-D8-25 Destination MAC Address: 00-60-97-B9-58-7D Ether Type field: IPv4

Frame length : 88 Padding:

IP Packet:

Source IP Address: /192.168.1.42 Destination IP Address: /192.168.1.62

IP Version: 4 Protocol Type: TCP

IP header length: 20 bytes

Total IP length: 74

Time to live: 64

Flag: 010

Fragment Offset: 0

TCP Segment:

Source Port: 20 Destination Port: 4940

Sequence Number: 4221341516 Acknowledgment number: 708153472

TCP Header Length: 32 bytes

Window Size: 5792

Flag: (PSH, ACK)

Urgent Pointer: 0

Option Field: 12

TCP Payload size: 22 bytes

TCP Payload type: FTP

Data: 32 32 36 20 46 69 6C 65 20 72 65 63 65 69 76 65 226 File receive

20 4F 4B 2E 0D 0A OK...

Ethernet Frame 145:

Source MAC Address: 00-60-97-B9-58-7D Destination MAC Address: 00-C0-4F-49-D8-25 Ether Type field: IPv4

Frame length : 88 Padding:

IP Packet:

Source IP Address: /192.168.1.62 Destination IP Address: /192.168.1.42

IP Version: 4 Protocol Type: TCP

IP header length: 20 bytes

Total IP length: 74

Time to live: 64

Flag: 010

Fragment Offset: 0

TCP Segment:

Source Port: 20 Destination Port: 4940

Sequence Number: 708153450 Acknowledgment number: 4221341494

TCP Header Length: 32 bytes

Window Size: 5840

Flag: (PSH, ACK)

Urgent Pointer: 0

Option Field: 12

TCP Payload size: 22 bytes

TCP Payload type: FTP

Data: 53 54 4F 52 20 46 54 50 2D 47 52 4F 55 50 31 34 STOR FTP-GROUP14

2E 4E 46 4F 0D 0A .NFO..

Ethernet Frame 144:

Source MAC Address: 00-60-97-B9-58-7D Destination MAC Address: 00-C0-4F-49-D8-25 Ether Type field: IPv4

Frame length : 66 Padding:

IP Packet:

Source IP Address: /192.168.1.62 Destination IP Address: /192.168.1.42

IP Version: 4 Protocol Type: TCP

IP header length: 20 bytes

Total IP length: 52

Time to live: 64

Flag: 010

Fragment Offset: 0

TCP Segment:

Source Port: 4940 Destination Port: 4938

Sequence Number: 709020621 Acknowledgment number: 4221101711

TCP Header Length: 32 bytes

Window Size: 5792

Flag: (FIN, ACK)

Urgent Pointer: 0

Option Field: 12

TCP Payload size: 0 bytes

TCP Payload type: other

Data: No payload

Ethernet Frame 143:

Source MAC Address: 00-60-97-B9-58-7D Destination MAC Address: 00-C0-4F-49-D8-25 Ether Type field: IPv4

Frame length : 74 Padding:

IP Packet:

Source IP Address: /192.168.1.62 Destination IP Address: /192.168.1.42

IP Version: 4 Protocol Type: TCP

IP header length: 20 bytes

Total IP length: 60

Time to live: 64

Flag: 010

Fragment Offset: 0

TCP Segment:

Source Port: 4940 Destination Port: 20

Sequence Number: 709020035 Acknowledgment number: 4221101711

TCP Header Length: 40 bytes

Window Size: 5792

Flag: (SYN, ACK)

Urgent Pointer: 0

Option Field: 20

TCP Payload size: 0 bytes

TCP Payload type: other

Data: No payload

Ethernet Frame 142:

Source MAC Address: 00-C0-4F-49-D8-25 Destination MAC Address: 00-60-97-B9-58-7D Ether Type field: IPv4

Frame length : 74 Padding:

IP Packet:

Source IP Address: /192.168.1.42 Destination IP Address: /192.168.1.62

IP Version: 4 Protocol Type: TCP

IP header length: 20 bytes

Total IP length: 60

Time to live: 64

Flag: 010

Fragment Offset: 0

TCP Segment:

Source Port: 20 Destination Port: 4940

Sequence Number: 4221101710 Acknowledgment number: 0

TCP Header Length: 40 bytes

Window Size: 5840

Flag: SYN

Urgent Pointer: 0

Option Field: 20

TCP Payload size: 0 bytes

TCP Payload type: other

Data: No payload

Ethernet Frame 141:

Source MAC Address: 00-C0-4F-49-D8-25 Destination MAC Address: 00-60-97-B9-58-7D Ether Type field: IPv4

Frame length : 99 Padding:

IP Packet:

Source IP Address: /192.168.1.42 Destination IP Address: /192.168.1.62

IP Version: 4 Protocol Type: TCP

IP header length: 20 bytes

Total IP length: 85

Time to live: 64

Flag: 010

Fragment Offset: 0

TCP Segment:

Source Port: 21 Destination Port: 4938

Sequence Number: 4221341380 Acknowledgment number: 708153417

TCP Header Length: 32 bytes

Window Size: 5792

Flag: (PSH, ACK)

Urgent Pointer: 0

Option Field: 12

TCP Payload size: 33 bytes

TCP Payload type: FTP

Data: 32 33 30 20 4C 6F 67 69 6E 20 73 75 63 63 65 73 230 Login succes

73 66 75 6C 2E 20 48 61 76 65 20 66 75 6E 2E 0D sful. Have fun..

0A .

Ethernet Frame 156:

Source MAC Address: 00-60-97-B9-58-7D Destination MAC Address: 00-C0-4F-49-D8-25 Ether Type field: IPv4

Frame length : 66 Padding:

IP Packet:

Source IP Address: /192.168.1.62 Destination IP Address: /192.168.1.42

IP Version: 4 Protocol Type: TCP

IP header length: 20 bytes

Total IP length: 52

Time to live: 64

Flag: 010

Fragment Offset: 0

TCP Segment:

Source Port: 4938 Destination Port: 21

Sequence Number: 709020622 Acknowledgment number: 4221101712

TCP Header Length: 32 bytes

Window Size: 5792

Flag: ACK

Urgent Pointer: 0

Option Field: 12

TCP Payload size: 0 bytes

TCP Payload type: FTP

Data: No payload

Ethernet Frame 157:

Source MAC Address: 00-60-97-B9-58-7D Destination MAC Address: 00-C0-4F-49-D8-25 Ether Type field: IPv4

Frame length : 72 Padding:

IP Packet:

Source IP Address: /192.168.1.62 Destination IP Address: /192.168.1.42

IP Version: 4 Protocol Type: TCP

IP header length: 20 bytes

Total IP length: 58

Time to live: 64

Flag: 010

Fragment Offset: 0

TCP Segment:

Source Port: 4938 Destination Port: 21

Sequence Number: 708153472 Acknowledgment number: 4221341538

TCP Header Length: 32 bytes

Window Size: 5840

Flag: (PSH, ACK)

Urgent Pointer: 0

Option Field: 12

TCP Payload size: 6 bytes

TCP Payload type: FTP

Data: 51 55 49 54 0D 0A QUIT..

Ethernet Frame 155:

Source MAC Address: 00-60-97-B9-58-7D Destination MAC Address: 00-C0-4F-49-D8-25 Ether Type field: IPv4

Frame length : 66 Padding:

IP Packet:

Source IP Address: /192.168.1.62 Destination IP Address: /192.168.1.42

IP Version: 4 Protocol Type: TCP

IP header length: 20 bytes

Total IP length: 52

Time to live: 64

Flag: 010

Fragment Offset: 0

TCP Segment:

Source Port: 4938 Destination Port: 21

Sequence Number: 708153479 Acknowledgment number: 4221341553

TCP Header Length: 32 bytes

Window Size: 5840

Flag: ACK

Urgent Pointer: 0

Option Field: 12

TCP Payload size: 0 bytes

TCP Payload type: FTP

Data: No payload

Ethernet Frame 154:

Source MAC Address: 00-C0-4F-49-D8-25 Destination MAC Address: 00-60-97-B9-58-7D Ether Type field: IPv4

Frame length : 66 Padding:

IP Packet:

Source IP Address: /192.168.1.42 Destination IP Address: /192.168.1.62

IP Version: 4 Protocol Type: TCP

IP header length: 20 bytes

Total IP length: 52

Time to live: 64

Flag: 010

Fragment Offset: 0

TCP Segment:

Source Port: 4938 Destination Port: 21

Sequence Number: 4221341552 Acknowledgment number: 708153479

TCP Header Length: 32 bytes

Window Size: 5792

Flag: (FIN, ACK)

Urgent Pointer: 0

Option Field: 12

TCP Payload size: 0 bytes

TCP Payload type: FTP

Data: No payload

Ethernet Frame 153:

Source MAC Address: 00-60-97-B9-58-7D Destination MAC Address: 00-C0-4F-49-D8-25 Ether Type field: IPv4

Frame length : 66 Padding:

IP Packet:

Source IP Address: /192.168.1.62 Destination IP Address: /192.168.1.42

IP Version: 4 Protocol Type: TCP

IP header length: 20 bytes

Total IP length: 52

Time to live: 64

Flag: 010

Fragment Offset: 0

TCP Segment:

Source Port: 4938 Destination Port: 21

Sequence Number: 708153478 Acknowledgment number: 4221341552

TCP Header Length: 32 bytes

Window Size: 5840

Flag: (FIN, ACK)

Urgent Pointer: 0

Option Field: 12

TCP Payload size: 0 bytes

TCP Payload type: FTP

Data: No payload

Ethernet Frame 152:

Source MAC Address: 00-C0-4F-49-D8-25 Destination MAC Address: 00-60-97-B9-58-7D Ether Type field: IPv4

Frame length : 80 Padding:

IP Packet:

Source IP Address: /192.168.1.42 Destination IP Address: /192.168.1.62

IP Version: 4 Protocol Type: TCP

IP header length: 20 bytes

Total IP length: 66

Time to live: 64

Flag: 010

Fragment Offset: 0

TCP Segment:

Source Port: 21 Destination Port: 4938

Sequence Number: 4221341538 Acknowledgment number: 708153478

TCP Header Length: 32 bytes

Window Size: 5792

Flag: (PSH, ACK)

Urgent Pointer: 0

Option Field: 12

TCP Payload size: 14 bytes

TCP Payload type: FTP

Data: 32 32 31 20 47 6F 6F 64 62 79 65 2E 0D 0A 221 Goodbye...

Ethernet Frame 151:

Source MAC Address: 00-C0-4F-49-D8-25 Destination MAC Address: 00-60-97-B9-58-7D Ether Type field: IPv4

Frame length : 66 Padding:

IP Packet:

Source IP Address: /192.168.1.42 Destination IP Address: /192.168.1.62

IP Version: 4 Protocol Type: TCP

IP header length: 20 bytes

Total IP length: 52

Time to live: 64

Flag: 010

Fragment Offset: 0

TCP Segment:

Source Port: 20 Destination Port: 4940

Sequence Number: 4221101711 Acknowledgment number: 709020622

TCP Header Length: 32 bytes

Window Size: 6435

Flag: (FIN, ACK)

Urgent Pointer: 0

Option Field: 12

TCP Payload size: 0 bytes

TCP Payload type: other

Data: No payload

Ethernet Frame 150:

Source MAC Address: 00-60-97-B9-58-7D Destination MAC Address: 00-C0-4F-49-D8-25 Ether Type field: IPv4

Frame length : 651 Padding:

IP Packet:

Source IP Address: /192.168.1.62 Destination IP Address: /192.168.1.42

IP Version: 4 Protocol Type: TCP

IP header length: 20 bytes

Total IP length: 637

Time to live: 64

Flag: 010

Fragment Offset: 0

TCP Segment:

Source Port: 20 Destination Port: 4940

Sequence Number: 709020036 Acknowledgment number: 4221101711

TCP Header Length: 32 bytes

Window Size: 5792

Flag: (PSH, ACK)

Urgent Pointer: 0

Option Field: 12

TCP Payload size: 585 bytes

TCP Payload type: other

Data: 20 20 20 20 20 20 20 20 20 20 20 20 20 20 20 20

20 20 20 20 20 20 20 20 20 20 20 20 20 20 20 20

20 20 20 20 20 20 20 20 20 20 20 2E 0D 0A 20 20 ...

20 20 20 2E 76 69 72 2E 20 20 20 20 20 20 20 20 .vir.

20 20 20 20 20 20 20 20 20 20 20 20 20 20 20 20

20 20 20 20 20 20 20 20 64 24 62 0D 0A 20 20 2E d$b.. .

64 24 24 24 24 24 24 62 2E 20 20 20 20 2E 63 64 d$$$$$$b. .cd

24 24 62 2E 20 20 20 20 20 2E 64 24 24 62 2E 20 $$b. .d$$b.

20 20 64 24 24 24 24 24 24 24 24 24 24 24 62 20 d$$$$$$$$$$$b

20 2E 64 24 24 62 2E 20 20 20 20 20 20 2E 64 24 .d$$b. .d$

24 62 2E 0D 0A 20 20 24 24 24 24 28 20 29 24 24 $b... $$$$( )$$

24 62 20 64 24 24 24 28 29 24 24 24 2E 20 20 20 $b d$$$()$$$.

64 24 24 24 24 24 24 24 62 20 51 24 24 24 24 24 d$$$$$$$b Q$$$$$

24 24 50 24 24 24 50 2E 24 24 24 24 24 24 24 62 $$P$$$P.$$$$$$$b

2E 20 20 2E 24 24 24 24 24 24 24 62 2E 0D 0A 20 . .$$$$$$$b...

20 51 24 24 24 24 24 24 24 24 24 24 42 24 24 24 Q$$$$$$$$$$B$$$

24 24 24 24 24 50 22 20 20 64 24 24 24 50 51 24 $$$$$P" d$$$PQ$

24 24 24 62 2E 20 20 20 24 24 24 24 2E 20 20 20 $$$b. $$$$.

2E 24 24 24 50 27 20 60 24 24 24 20 2E 24 24 24 .$$$P' `$$$ .$$$

50 27 20 60 24 24 24 0D 0A 20 20 20 20 22 24 24 P' `$$$.. "$$

24 24 24 24 24 50 20 51 24 24 24 24 24 24 24 62 $$$$$P Q$$$$$$$b

20 20 64 24 24 24 50 20 20 20 51 24 24 24 24 62 d$$$P Q$$$$b

20 20 24 24 24 24 62 20 20 20 24 24 24 24 62 2E $$$$b $$$$b.

2E 64 24 24 24 20 24 24 24 24 62 2E 2E 64 24 24 .d$$$ $$$$b..d$$

24 0D 0A 20 20 20 64 24 24 24 24 24 24 50 22 20 $.. d$$$$$$P"

20 20 22 24 24 24 24 24 24 24 24 20 51 24 24 24 "$$$$$$$$ Q$$$

20 20 20 20 20 51 24 24 24 24 20 20 24 24 24 24 Q$$$$ $$$$

24 20 20 20 60 51 24 24 24 24 24 24 24 50 20 20 $ `Q$$$$$$$P

60 51 24 24 24 24 24 24 24 50 0D 0A 20 20 24 24 `Q$$$$$$$P.. $$

24 24 24 24 24 50 20 20 20 20 20 20 20 60 22 22 $$$$$P `""

22 22 22 20 20 20 22 22 20 20 20 20 20 20 20 20 """ ""

22 22 20 20 20 51 24 24 24 50 20 20 20 20 20 22 "" Q$$$P "

51 24 24 24 50 22 20 20 20 20 20 22 51 24 24 24 Q$$$P" "Q$$$

50 22 0D 0A 20 20 60 51 24 24 50 22 20 20 20 20 P".. `Q$$P"

20 20 20 20 20 20 20 20 20 20 20 20 20 20 20 20

20 20 20 20 20 20 20 20 20 20 20 20 20 20 22 22 ""

22 0D 0A 0D 0A 0D 0A 0D 0A "........

Ethernet Frame 158:

Source MAC Address: 00-60-97-B9-58-7D Destination MAC Address: 00-C0-4F-8D-93-F2 Ether Type field: IPv4

Frame length : 74 Padding:

IP Packet:

Source IP Address: /192.168.1.62 Destination IP Address: /192.168.1.66

IP Version: 4 Protocol Type: TCP

IP header length: 20 bytes

Total IP length: 60

Time to live: 64

Flag: 010

Fragment Offset: 0

TCP Segment:

Source Port: 21 Destination Port: 21

Sequence Number: 701566255 Acknowledgment number: 0

TCP Header Length: 40 bytes

Window Size: 5840

Flag: SYN

Urgent Pointer: 0

Option Field: 20

TCP Payload size: 0 bytes

TCP Payload type: FTP

Data: No payload

Ethernet Frame 159:

Source MAC Address: 00-C0-4F-8D-93-F2 Destination MAC Address: 00-60-97-B9-58-7D Ether Type field: IPv4

Frame length : 74 Padding:

IP Packet:

Source IP Address: /192.168.1.66 Destination IP Address: /192.168.1.62

IP Version: 4 Protocol Type: TCP

IP header length: 20 bytes

Total IP length: 60

Time to live: 64

Flag: 010

Fragment Offset: 0

TCP Segment:

Source Port: 21 Destination Port: 21

Sequence Number: 2706227480 Acknowledgment number: 701566256

TCP Header Length: 40 bytes

Window Size: 5792

Flag: (SYN, ACK)

Urgent Pointer: 0

Option Field: 20

TCP Payload size: 0 bytes

TCP Payload type: FTP

Data: No payload

Ethernet Frame 159:

Source MAC Address: 00-60-97-B9-58-7D Destination MAC Address: 00-C0-4F-8D-93-F2 Ether Type field: IPv4

Frame length : 66 Padding:

IP Packet:

Source IP Address: /192.168.1.62 Destination IP Address: /192.168.1.66

IP Version: 4 Protocol Type: TCP

IP header length: 20 bytes

Total IP length: 52

Time to live: 64

Flag: 010

Fragment Offset: 0

TCP Segment:

Source Port: 21 Destination Port: 21

Sequence Number: 701566256 Acknowledgment number: 2706227481

TCP Header Length: 32 bytes

Window Size: 5840

Flag: ACK

Urgent Pointer: 0

Option Field: 12

TCP Payload size: 0 bytes

TCP Payload type: FTP

Data: No payload

Ethernet Frame 160:

Source MAC Address: 00-60-97-B9-58-7D Destination MAC Address: 00-C0-4F-8D-93-F2 Ether Type field: IPv4

Frame length : 66 Padding:

IP Packet:

Source IP Address: /192.168.1.62 Destination IP Address: /192.168.1.66

IP Version: 4 Protocol Type: TCP

IP header length: 20 bytes

Total IP length: 52

Time to live: 64

Flag: 010

Fragment Offset: 0

TCP Segment:

Source Port: 4936 Destination Port: 21

Sequence Number: 701566256 Acknowledgment number: 2706227577

TCP Header Length: 32 bytes

Window Size: 5840

Flag: ACK

Urgent Pointer: 0

Option Field: 12

TCP Payload size: 0 bytes

TCP Payload type: FTP

Data: No payload

Ethernet Frame 162:

Source MAC Address: 00-60-97-B9-58-7D Destination MAC Address: 00-C0-4F-8D-93-F2 Ether Type field: IPv4

Frame length : 76 Padding:

IP Packet:

Source IP Address: /192.168.1.62 Destination IP Address: /192.168.1.66

IP Version: 4 Protocol Type: TCP

IP header length: 20 bytes

Total IP length: 62

Time to live: 64

Flag: 010

Fragment Offset: 0

TCP Segment:

Source Port: 21 Destination Port: 4936

Sequence Number: 701566256 Acknowledgment number: 2706227577

TCP Header Length: 32 bytes

Window Size: 5840

Flag: (PSH, ACK)

Urgent Pointer: 0

Option Field: 12

TCP Payload size: 10 bytes

TCP Payload type: FTP

Data: 41 55 54 48 20 53 53 4C 0D 0A AUTH SSL..

Ethernet Frame 170:

Source MAC Address: 00-C0-4F-8D-93-F2 Destination MAC Address: 00-60-97-B9-58-7D Ether Type field: IPv4

Frame length : 66 Padding:

IP Packet:

Source IP Address: /192.168.1.66 Destination IP Address: /192.168.1.62

IP Version: 4 Protocol Type: TCP

IP header length: 20 bytes

Total IP length: 52

Time to live: 64

Flag: 010

Fragment Offset: 0

TCP Segment:

Source Port: 21 Destination Port: 4936

Sequence Number: 2706227693 Acknowledgment number: 701566312

TCP Header Length: 32 bytes

Window Size: 5792

Flag: (FIN, ACK)

Urgent Pointer: 0

Option Field: 12

TCP Payload size: 0 bytes

TCP Payload type: FTP

Data: No payload

Ethernet Frame 163:

Source MAC Address: 00-C0-4F-8D-93-F2 Destination MAC Address: 00-60-97-B9-58-7D Ether Type field: IPv4

Frame length : 91 Padding:

IP Packet:

Source IP Address: /192.168.1.66 Destination IP Address: /192.168.1.62

IP Version: 4 Protocol Type: TCP

IP header length: 20 bytes

Total IP length: 77

Time to live: 64

Flag: 010

Fragment Offset: 0

TCP Segment:

Source Port: 21 Destination Port: 4936

Sequence Number: 2706227577 Acknowledgment number: 701566266

TCP Header Length: 32 bytes

Window Size: 5792

Flag: (PSH, ACK)

Urgent Pointer: 0

Option Field: 12

TCP Payload size: 25 bytes

TCP Payload type: FTP

Data: 35 30 30 20 41 55 54 48 20 6E 6F 74 20 75 6E 64 500 AUTH not und

65 72 73 74 6F 6F 64 0D 0A erstood..

Ethernet Frame 161:

Source MAC Address: 00-C0-4F-8D-93-F2 Destination MAC Address: 00-60-97-B9-58-7D Ether Type field: IPv4

Frame length : 66 Padding:

IP Packet:

Source IP Address: /192.168.1.66 Destination IP Address: /192.168.1.62

IP Version: 4 Protocol Type: TCP

IP header length: 20 bytes

Total IP length: 52

Time to live: 64

Flag: 010

Fragment Offset: 0

TCP Segment:

Source Port: 21 Destination Port: 4936

Sequence Number: 2706227577 Acknowledgment number: 701566266

TCP Header Length: 32 bytes

Window Size: 5792

Flag: ACK

Urgent Pointer: 0

Option Field: 12

TCP Payload size: 0 bytes

TCP Payload type: FTP

Data: No payload

Ethernet Frame 174:

Source MAC Address: 00-C0-4F-8D-93-F2 Destination MAC Address: 00-60-97-B9-58-7D Ether Type field: IPv4

Frame length : 85 Padding:

IP Packet:

Source IP Address: /192.168.1.66 Destination IP Address: /192.168.1.62

IP Version: 4 Protocol Type: TCP

IP header length: 20 bytes

Total IP length: 71

Time to live: 64

Flag: 010

Fragment Offset: 0

TCP Segment:

Source Port: 21 Destination Port: 4936

Sequence Number: 2706227660 Acknowledgment number: 701566305

TCP Header Length: 32 bytes

Window Size: 5792

Flag: (PSH, ACK)

Urgent Pointer: 0

Option Field: 12

TCP Payload size: 19 bytes

TCP Payload type: FTP

Data: 32 31 35 20 55 4E 49 58 20 54 79 70 65 3A 20 4C 215 UNIX Type: L

38 0D 0A 8..

Ethernet Frame 173:

Source MAC Address: 00-60-97-B9-58-7D Destination MAC Address: 00-C0-4F-8D-93-F2 Ether Type field: IPv4

Frame length : 72 Padding:

IP Packet:

Source IP Address: /192.168.1.62 Destination IP Address: /192.168.1.66

IP Version: 4 Protocol Type: TCP

IP header length: 20 bytes

Total IP length: 58

Time to live: 64

Flag: 010

Fragment Offset: 0

TCP Segment:

Source Port: 21 Destination Port: 4936

Sequence Number: 701566305 Acknowledgment number: 2706227679

TCP Header Length: 32 bytes

Window Size: 5840

Flag: (PSH, ACK)

Urgent Pointer: 0

Option Field: 12

TCP Payload size: 6 bytes

TCP Payload type: FTP

Data: 51 55 49 54 0D 0A QUIT..

Ethernet Frame 172:

Source MAC Address: 00-60-97-B9-58-7D Destination MAC Address: 00-C0-4F-8D-93-F2 Ether Type field: IPv4

Frame length : 66 Padding:

IP Packet:

Source IP Address: /192.168.1.62 Destination IP Address: /192.168.1.66

IP Version: 4 Protocol Type: TCP

IP header length: 20 bytes

Total IP length: 52

Time to live: 64

Flag: 010

Fragment Offset: 0

TCP Segment:

Source Port: 21 Destination Port: 4936

Sequence Number: 701566311 Acknowledgment number: 2706227693

TCP Header Length: 32 bytes

Window Size: 5840

Flag: (FIN, ACK)

Urgent Pointer: 0

Option Field: 12

TCP Payload size: 0 bytes

TCP Payload type: FTP

Data: No payload

Ethernet Frame 170:

Source MAC Address: 00-60-97-B9-58-7D Destination MAC Address: 00-C0-4F-8D-93-F2 Ether Type field: IPv4

Frame length : 66 Padding:

IP Packet:

Source IP Address: /192.168.1.62 Destination IP Address: /192.168.1.66

IP Version: 4 Protocol Type: TCP

IP header length: 20 bytes

Total IP length: 52

Time to live: 64

Flag: 010

Fragment Offset: 0

TCP Segment:

Source Port: 21 Destination Port: 4936

Sequence Number: 701566312 Acknowledgment number: 2706227694

TCP Header Length: 32 bytes

Window Size: 5840

Flag: ACK

Urgent Pointer: 0

Option Field: 12

TCP Payload size: 0 bytes

TCP Payload type: FTP

Data: No payload

Ethernet Frame 171:

Source MAC Address: 00-C0-4F-8D-93-F2 Destination MAC Address: 00-60-97-B9-58-7D Ether Type field: IPv4

Frame length : 80 Padding:

IP Packet:

Source IP Address: /192.168.1.66 Destination IP Address: /192.168.1.62

IP Version: 4 Protocol Type: TCP

IP header length: 20 bytes

Total IP length: 66

Time to live: 64

Flag: 010

Fragment Offset: 0

TCP Segment:

Source Port: 21 Destination Port: 4936

Sequence Number: 2706227679 Acknowledgment number: 701566311

TCP Header Length: 32 bytes

Window Size: 5792

Flag: (PSH, ACK)

Urgent Pointer: 0

Option Field: 12

TCP Payload size: 14 bytes

TCP Payload type: FTP

Data: 32 32 31 20 47 6F 6F 64 62 79 65 2E 0D 0A 221 Goodbye...

Ethernet Frame 169:

Source MAC Address: 00-C0-4F-8D-93-F2 Destination MAC Address: 00-60-97-B9-58-7D Ether Type field: IPv4

Frame length : 162 Padding:

IP Packet:

Source IP Address: /192.168.1.66 Destination IP Address: /192.168.1.62

IP Version: 4 Protocol Type: TCP

IP header length: 20 bytes

Total IP length: 148

Time to live: 64

Flag: 010

Fragment Offset: 0

TCP Segment:

Source Port: 4936 Destination Port: 21

Sequence Number: 2706227481 Acknowledgment number: 701566256

TCP Header Length: 32 bytes

Window Size: 5792

Flag: (PSH, ACK)

Urgent Pointer: 0

Option Field: 12

TCP Payload size: 96 bytes

TCP Payload type: FTP

Data: 32 32 30 20 50 72 6F 46 54 50 44 20 31 2E 32 2E 220 ProFTPD 1.2.

39 20 53 65 72 76 65 72 20 28 4C 61 6E 74 68 61 9 Server (Lantha

6E 75 6D 20 46 54 50 20 53 65 72 76 65 72 20 28 num FTP Server (

47 72 6F 75 70 20 31 35 29 29 20 5B 6C 61 6E 74 Group 15)) [lant

68 61 6E 75 6D 2E 67 72 6F 75 70 31 35 2E 73 73 hanum.group15.ss

61 63 2E 75 74 75 6C 73 61 2E 65 64 75 5D 0D 0A ac.utulsa.edu]..

Ethernet Frame 168:

Source MAC Address: 00-60-97-B9-58-7D Destination MAC Address: 00-C0-4F-8D-93-F2 Ether Type field: IPv4

Frame length : 72 Padding:

IP Packet:

Source IP Address: /192.168.1.62 Destination IP Address: /192.168.1.66

IP Version: 4 Protocol Type: TCP

IP header length: 20 bytes

Total IP length: 58

Time to live: 64

Flag: 010

Fragment Offset: 0

TCP Segment:

Source Port: 4936 Destination Port: 21

Sequence Number: 701566299 Acknowledgment number: 2706227660

TCP Header Length: 32 bytes

Window Size: 5840

Flag: (PSH, ACK)

Urgent Pointer: 0

Option Field: 12

TCP Payload size: 6 bytes

TCP Payload type: FTP

Data: 53 59 53 54 0D 0A SYST..

Ethernet Frame 166:

Source MAC Address: 00-60-97-B9-58-7D Destination MAC Address: 00-C0-4F-8D-93-F2 Ether Type field: IPv4

Frame length : 85 Padding:

IP Packet:

Source IP Address: /192.168.1.62 Destination IP Address: /192.168.1.66

IP Version: 4 Protocol Type: TCP

IP header length: 20 bytes

Total IP length: 71

Time to live: 64

Flag: 010

Fragment Offset: 0

TCP Segment:

Source Port: 4936 Destination Port: 21

Sequence Number: 701566280 Acknowledgment number: 2706227638

TCP Header Length: 32 bytes

Window Size: 5840

Flag: (PSH, ACK)

Urgent Pointer: 0

Option Field: 12

TCP Payload size: 19 bytes

TCP Payload type: FTP

Data: 50 41 53 53 20 31 39 32 2E 31 36 38 2E 31 2E 36 PASS 192.168.1.6

32 0D 0A 2..

Ethernet Frame 167:

Source MAC Address: 00-C0-4F-8D-93-F2 Destination MAC Address: 00-60-97-B9-58-7D Ether Type field: IPv4

Frame length : 88 Padding:

IP Packet:

Source IP Address: /192.168.1.66 Destination IP Address: /192.168.1.62

IP Version: 4 Protocol Type: TCP

IP header length: 20 bytes

Total IP length: 74

Time to live: 64

Flag: 010

Fragment Offset: 0

TCP Segment:

Source Port: 4936 Destination Port: 21

Sequence Number: 2706227638 Acknowledgment number: 701566299

TCP Header Length: 32 bytes

Window Size: 5792

Flag: (PSH, ACK)

Urgent Pointer: 0

Option Field: 12

TCP Payload size: 22 bytes

TCP Payload type: FTP

Data: 35 33 30 20 4C 6F 67 69 6E 20 69 6E 63 6F 72 72 530 Login incorr

65 63 74 2E 0D 0A ect...

Ethernet Frame 165:

Source MAC Address: 00-C0-4F-8D-93-F2 Destination MAC Address: 00-60-97-B9-58-7D Ether Type field: IPv4

Frame length : 102 Padding:

IP Packet:

Source IP Address: /192.168.1.66 Destination IP Address: /192.168.1.62

IP Version: 4 Protocol Type: TCP

IP header length: 20 bytes

Total IP length: 88

Time to live: 64

Flag: 010

Fragment Offset: 0

TCP Segment:

Source Port: 4936 Destination Port: 4936

Sequence Number: 2706227602 Acknowledgment number: 701566280

TCP Header Length: 32 bytes

Window Size: 5792

Flag: (PSH, ACK)

Urgent Pointer: 0

Option Field: 12

TCP Payload size: 36 bytes

TCP Payload type: FTP

Data: 33 33 31 20 50 61 73 73 77 6F 72 64 20 72 65 71 331 Password req

75 69 72 65 64 20 66 6F 72 20 67 72 6F 75 70 31 uired for group1

34 2E 0D 0A 4...

Ethernet Frame 164:

Source MAC Address: 00-60-97-B9-58-7D Destination MAC Address: 00-C0-4F-8D-93-F2 Ether Type field: IPv4

Frame length : 80 Padding:

IP Packet:

Source IP Address: /192.168.1.62 Destination IP Address: /192.168.1.66

IP Version: 4 Protocol Type: TCP

IP header length: 20 bytes

Total IP length: 66

Time to live: 64

Flag: 010

Fragment Offset: 0

TCP Segment:

Source Port: 4936 Destination Port: 4936

Sequence Number: 701566266 Acknowledgment number: 2706227602

TCP Header Length: 32 bytes

Window Size: 5840

Flag: (PSH, ACK)

Urgent Pointer: 0

Option Field: 12

TCP Payload size: 14 bytes

TCP Payload type: other

Data: 55 53 45 52 20 67 72 6F 75 70 31 34 0D 0A USER group14..

Ethernet Frame 175:

Source MAC Address: 08-00-20-AB-D4-A4 Destination MAC Address: 00-C0-4F-8D-99-37 Ether Type field: IPv4

Frame length : 62 Padding:

IP Packet:

Source IP Address: /192.168.1.22 Destination IP Address: /192.168.1.10

IP Version: 4 Protocol Type: TCP

IP header length: 20 bytes

Total IP length: 48

Time to live: 64

Flag: 010

Fragment Offset: 0

TCP Segment:

Source Port: 43999 Destination Port: 80

Sequence Number: 2388860656 Acknowledgment number: 0

TCP Header Length: 28 bytes

Window Size: 49640

Flag: SYN

Urgent Pointer: 0

Option Field: 8

TCP Payload size: 0 bytes

TCP Payload type: other

Data: No payload

Ethernet Frame 177:

Source MAC Address: 08-00-20-AB-D4-A4 Destination MAC Address: 00-C0-4F-8D-99-37 Ether Type field: IPv4

Frame length : 60 Padding: 555555555555

IP Packet:

Source IP Address: /192.168.1.22 Destination IP Address: /192.168.1.10

IP Version: 4 Protocol Type: TCP

IP header length: 20 bytes

Total IP length: 40

Time to live: 64

Flag: 010

Fragment Offset: 0

TCP Segment:

Source Port: 43999 Destination Port: 43999

Sequence Number: 2388860657 Acknowledgment number: 3896578493

TCP Header Length: 20 bytes

Window Size: 49640

Flag: ACK

Urgent Pointer: 0

Option Field: 0

TCP Payload size: 0 bytes

TCP Payload type: other

Data: No payload

Ethernet Frame 176:

Source MAC Address: 00-C0-4F-8D-99-37 Destination MAC Address: 08-00-20-AB-D4-A4 Ether Type field: IPv4

Frame length : 62 Padding:

IP Packet:

Source IP Address: /192.168.1.10 Destination IP Address: /192.168.1.22

IP Version: 4 Protocol Type: TCP

IP header length: 20 bytes

Total IP length: 48

Time to live: 64

Flag: 010

Fragment Offset: 0

TCP Segment:

Source Port: 43999 Destination Port: 43999

Sequence Number: 3896578492 Acknowledgment number: 2388860657

TCP Header Length: 28 bytes

Window Size: 16384

Flag: (SYN, ACK)

Urgent Pointer: 0

Option Field: 8

TCP Payload size: 0 bytes

TCP Payload type: other

Data: No payload

Ethernet Frame 178:

Source MAC Address: 08-00-20-AB-D4-A4 Destination MAC Address: 00-C0-4F-8D-99-37 Ether Type field: IPv4

Frame length : 77 Padding:

IP Packet:

Source IP Address: /192.168.1.22 Destination IP Address: /192.168.1.10

IP Version: 4 Protocol Type: TCP

IP header length: 20 bytes

Total IP length: 63

Time to live: 64

Flag: 010

Fragment Offset: 0

TCP Segment:

Source Port: 43999 Destination Port: 80

Sequence Number: 2388860657 Acknowledgment number: 3896578493

TCP Header Length: 20 bytes

Window Size: 49640

Flag: (PSH, ACK)

Urgent Pointer: 0

Option Field: 0

TCP Payload size: 23 bytes

TCP Payload type: other

Data: 47 45 54 20 2F 63 73 37 34 39 33 2F 20 48 54 54 GET /cs7493/ HTT

50 2F 31 2E 30 0D 0A P/1.0..

Ethernet Frame 179:

Source MAC Address: 00-C0-4F-8D-99-37 Destination MAC Address: 08-00-20-AB-D4-A4 Ether Type field: IPv4

Frame length : 60 Padding: 000000000000

IP Packet:

Source IP Address: /192.168.1.10 Destination IP Address: /192.168.1.22

IP Version: 4 Protocol Type: TCP

IP header length: 20 bytes

Total IP length: 40

Time to live: 64

Flag: 010

Fragment Offset: 0

TCP Segment:

Source Port: 80 Destination Port: 43999

Sequence Number: 3896578493 Acknowledgment number: 2388860680

TCP Header Length: 20 bytes

Window Size: 17520

Flag: ACK

Urgent Pointer: 0

Option Field: 0

TCP Payload size: 0 bytes

TCP Payload type: other

Data: No payload

Ethernet Frame 180:

Source MAC Address: 08-00-20-AB-D4-A4 Destination MAC Address: 00-C0-4F-8D-99-37 Ether Type field: IPv4

Frame length : 60 Padding: 555555555555

IP Packet:

Source IP Address: /192.168.1.22 Destination IP Address: /192.168.1.10

IP Version: 4 Protocol Type: TCP

IP header length: 20 bytes

Total IP length: 40

Time to live: 64

Flag: 010

Fragment Offset: 0

TCP Segment:

Source Port: 80 Destination Port: 43999

Sequence Number: 2388860686 Acknowledgment number: 3896578860

TCP Header Length: 20 bytes

Window Size: 49273

Flag: ACK

Urgent Pointer: 0

Option Field: 0

TCP Payload size: 0 bytes

TCP Payload type: other

Data: No payload

Ethernet Frame 186:

Source MAC Address: 08-00-20-AB-D4-A4 Destination MAC Address: 00-C0-4F-8D-99-37 Ether Type field: IPv4

Frame length : 60 Padding: 555555555555

IP Packet:

Source IP Address: /192.168.1.22 Destination IP Address: /192.168.1.10

IP Version: 4 Protocol Type: TCP

IP header length: 20 bytes

Total IP length: 40

Time to live: 64

Flag: 010

Fragment Offset: 0

TCP Segment:

Source Port: 43999 Destination Port: 80

Sequence Number: 2388860686 Acknowledgment number: 3896578861

TCP Header Length: 20 bytes

Window Size: 49273

Flag: (FIN, ACK)

Urgent Pointer: 0

Option Field: 0

TCP Payload size: 0 bytes

TCP Payload type: other

Data: No payload

Ethernet Frame 185:

Source MAC Address: 08-00-20-AB-D4-A4 Destination MAC Address: 00-C0-4F-8D-99-37 Ether Type field: IPv4

Frame length : 60 Padding: 0D0A0D0A0D0A

IP Packet:

Source IP Address: /192.168.1.22 Destination IP Address: /192.168.1.10

IP Version: 4 Protocol Type: TCP

IP header length: 20 bytes

Total IP length: 46

Time to live: 64

Flag: 010

Fragment Offset: 0

TCP Segment:

Source Port: 43999 Destination Port: 80

Sequence Number: 2388860680 Acknowledgment number: 3896578493

TCP Header Length: 20 bytes

Window Size: 49640

Flag: (PSH, ACK)

Urgent Pointer: 0

Option Field: 0

TCP Payload size: 6 bytes

TCP Payload type: other

Data: 0D 0A 0D 0A 0D 0A ......

Ethernet Frame 184:

Source MAC Address: 08-00-20-AB-D4-A4 Destination MAC Address: 00-C0-4F-8D-99-37 Ether Type field: IPv4

Frame length : 60 Padding: 555555555555

IP Packet:

Source IP Address: /192.168.1.22 Destination IP Address: /192.168.1.10

IP Version: 4 Protocol Type: TCP

IP header length: 20 bytes

Total IP length: 40

Time to live: 64

Flag: 010

Fragment Offset: 0

TCP Segment:

Source Port: 43999 Destination Port: 80

Sequence Number: 2388860686 Acknowledgment number: 3896578861

TCP Header Length: 20 bytes

Window Size: 49273

Flag: ACK

Urgent Pointer: 0

Option Field: 0

TCP Payload size: 0 bytes

TCP Payload type: other

Data: No payload

Ethernet Frame 183:

Source MAC Address: 00-C0-4F-8D-99-37 Destination MAC Address: 08-00-20-AB-D4-A4 Ether Type field: IPv4

Frame length : 421 Padding:

IP Packet:

Source IP Address: /192.168.1.10 Destination IP Address: /192.168.1.22

IP Version: 4 Protocol Type: TCP

IP header length: 20 bytes

Total IP length: 407

Time to live: 64

Flag: 010

Fragment Offset: 0

TCP Segment:

Source Port: 80 Destination Port: 43999

Sequence Number: 3896578493 Acknowledgment number: 2388860686

TCP Header Length: 20 bytes

Window Size: 17520

Flag: (PSH, ACK)

Urgent Pointer: 0

Option Field: 0

TCP Payload size: 367 bytes

TCP Payload type: other

Data: 48 54 54 50 2F 31 2E 31 20 32 30 30 20 4F 4B 0D HTTP/1.1 200 OK.

0A 44 61 74 65 3A 20 57 65 64 2C 20 31 39 20 4A .Date: Wed, 19 J

61 6E 20 32 30 30 35 20 31 31 3A 35 32 3A 35 36 an 2005 11:52:56

20 47 4D 54 0D 0A 53 65 72 76 65 72 3A 20 41 70 GMT..Server: Ap

61 63 68 65 2F 31 2E 33 2E 32 39 20 28 55 6E 69 ache/1.3.29 (Uni

78 29 20 6D 6F 64 5F 73 73 6C 2F 32 2E 38 2E 31 x) mod\_ssl/2.8.1

36 20 4F 70 65 6E 53 53 4C 2F 30 2E 39 2E 37 63 6 OpenSSL/0.9.7c

0D 0A 4C 61 73 74 2D 4D 6F 64 69 66 69 65 64 3A ..Last-Modified:

20 57 65 64 2C 20 32 37 20 4F 63 74 20 32 30 30 Wed, 27 Oct 200

34 20 31 34 3A 31 34 3A 34 34 20 47 4D 54 0D 0A 4 14:14:44 GMT..

45 54 61 67 3A 20 22 33 30 35 39 34 35 35 66 36 ETag: "3059455f6

64 32 32 36 36 38 62 36 38 62 64 37 33 33 35 38 d22668b68bd73358

39 66 31 65 66 64 30 39 37 38 65 36 63 38 30 22 9f1efd0978e6c80"

0D 0A 41 63 63 65 70 74 2D 52 61 6E 67 65 73 3A ..Accept-Ranges:

20 62 79 74 65 73 0D 0A 43 6F 6E 74 65 6E 74 2D bytes..Content-

4C 65 6E 67 74 68 3A 20 36 39 0D 0A 43 6F 6E 6E Length: 69..Conn

65 63 74 69 6F 6E 3A 20 63 6C 6F 73 65 0D 0A 43 ection: close..C

6F 6E 74 65 6E 74 2D 54 79 70 65 3A 20 74 65 78 ontent-Type: tex

74 2F 68 74 6D 6C 0D 0A 0D 0A 3C 68 74 6D 6C 3E t/html....<html>

0A 3C 62 6F 64 79 3E 68 65 79 2C 20 43 6F 6E 67 .<body>hey, Cong

72 61 74 73 2C 20 79 6F 75 27 76 65 20 66 6F 75 rats, you've fou

6E 64 20 6F 75 72 20 77 65 62 20 70 61 67 65 21 nd our web page!

3C 2F 62 6F 64 79 3E 3C 2F 68 74 6D 6C 3E 0A </body></html>.

Ethernet Frame 182:

Source MAC Address: 00-C0-4F-8D-99-37 Destination MAC Address: 08-00-20-AB-D4-A4 Ether Type field: IPv4

Frame length : 60 Padding: 000000000000

IP Packet:

Source IP Address: /192.168.1.10 Destination IP Address: /192.168.1.22

IP Version: 4 Protocol Type: TCP

IP header length: 20 bytes

Total IP length: 40

Time to live: 64

Flag: 010

Fragment Offset: 0

TCP Segment:

Source Port: 80 Destination Port: 43999

Sequence Number: 3896578860 Acknowledgment number: 2388860686

TCP Header Length: 20 bytes

Window Size: 17520

Flag: (FIN, ACK)

Urgent Pointer: 0

Option Field: 0

TCP Payload size: 0 bytes

TCP Payload type: other

Data: No payload

Ethernet Frame 181:

Source MAC Address: 00-C0-4F-8D-99-37 Destination MAC Address: 08-00-20-AB-D4-A4 Ether Type field: IPv4

Frame length : 60 Padding: 000000000000

IP Packet:

Source IP Address: /192.168.1.10 Destination IP Address: /192.168.1.22

IP Version: 4 Protocol Type: TCP

IP header length: 20 bytes

Total IP length: 40

Time to live: 64

Flag: 010

Fragment Offset: 0

TCP Segment:

Source Port: 80 Destination Port: 43999

Sequence Number: 3896578861 Acknowledgment number: 2388860687

TCP Header Length: 20 bytes

Window Size: 17520

Flag: ACK

Urgent Pointer: 0

Option Field: 0

TCP Payload size: 0 bytes

TCP Payload type: other

Data: No payload

Ethernet Frame 187:

Source MAC Address: 00-C0-4F-8D-93-F2 Destination MAC Address: 08-00-20-AB-D4-A4 Ether Type field: IPv4

Frame length : 74 Padding:

IP Packet:

Source IP Address: /192.168.1.66 Destination IP Address: /192.168.1.22

IP Version: 4 Protocol Type: TCP

IP header length: 20 bytes

Total IP length: 60

Time to live: 64

Flag: 010

Fragment Offset: 0

TCP Segment:

Source Port: 56788 Destination Port: 23

Sequence Number: 3108926015 Acknowledgment number: 0

TCP Header Length: 40 bytes

Window Size: 5840

Flag: SYN

Urgent Pointer: 0

Option Field: 20

TCP Payload size: 0 bytes

TCP Payload type: Telnet

Data: No payload

Ethernet Frame 189:

Source MAC Address: 00-C0-4F-8D-93-F2 Destination MAC Address: 08-00-20-AB-D4-A4 Ether Type field: IPv4

Frame length : 66 Padding:

IP Packet:

Source IP Address: /192.168.1.66 Destination IP Address: /192.168.1.22

IP Version: 4 Protocol Type: TCP

IP header length: 20 bytes

Total IP length: 52

Time to live: 64

Flag: 010

Fragment Offset: 0

TCP Segment:

Source Port: 56788 Destination Port: 23

Sequence Number: 3108926016 Acknowledgment number: 2424181815

TCP Header Length: 32 bytes

Window Size: 5840

Flag: ACK

Urgent Pointer: 0

Option Field: 12

TCP Payload size: 0 bytes

TCP Payload type: Telnet

Data: No payload

Ethernet Frame 188:

Source MAC Address: 08-00-20-AB-D4-A4 Destination MAC Address: 00-C0-4F-8D-93-F2 Ether Type field: IPv4

Frame length : 78 Padding:

IP Packet:

Source IP Address: /192.168.1.22 Destination IP Address: /192.168.1.66

IP Version: 4 Protocol Type: TCP

IP header length: 20 bytes

Total IP length: 64

Time to live: 60

Flag: 010

Fragment Offset: 0

TCP Segment:

Source Port: 56788 Destination Port: 23

Sequence Number: 2424181814 Acknowledgment number: 3108926016

TCP Header Length: 44 bytes

Window Size: 49232

Flag: (SYN, ACK)

Urgent Pointer: 0

Option Field: 24

TCP Payload size: 0 bytes

TCP Payload type: Telnet

Data: No payload

Ethernet Frame 191:

Source MAC Address: 00-C0-4F-8D-93-F2 Destination MAC Address: 08-00-20-AB-D4-A4 Ether Type field: IPv4

Frame length : 66 Padding:

IP Packet:

Source IP Address: /192.168.1.66 Destination IP Address: /192.168.1.22

IP Version: 4 Protocol Type: TCP

IP header length: 20 bytes

Total IP length: 52

Time to live: 64

Flag: 010

Fragment Offset: 0

TCP Segment:

Source Port: 56788 Destination Port: 23

Sequence Number: 3108926016 Acknowledgment number: 2424181830

TCP Header Length: 32 bytes

Window Size: 5840

Flag: ACK

Urgent Pointer: 0

Option Field: 12

TCP Payload size: 0 bytes

TCP Payload type: Telnet

Data: No payload

Ethernet Frame 190:

Source MAC Address: 08-00-20-AB-D4-A4 Destination MAC Address: 00-C0-4F-8D-93-F2 Ether Type field: IPv4

Frame length : 81 Padding:

IP Packet:

Source IP Address: /192.168.1.22 Destination IP Address: /192.168.1.66

IP Version: 4 Protocol Type: TCP

IP header length: 20 bytes

Total IP length: 67

Time to live: 60

Flag: 010

Fragment Offset: 0

TCP Segment:

Source Port: 56788 Destination Port: 23

Sequence Number: 2424181815 Acknowledgment number: 3108926016

TCP Header Length: 32 bytes

Window Size: 49232

Flag: (PSH, ACK)

Urgent Pointer: 0

Option Field: 12

TCP Payload size: 15 bytes

TCP Payload type: Telnet

Data: FF FD 18 FF FD 1F FF FD 23 FF FD 27 FF FD 24 ........#..'..$

Ethernet Frame 192:

Source MAC Address: 00-C0-4F-8D-93-F2 Destination MAC Address: 08-00-20-AB-D4-A4 Ether Type field: IPv4

Frame length : 81 Padding:

IP Packet:

Source IP Address: /192.168.1.66 Destination IP Address: /192.168.1.22

IP Version: 4 Protocol Type: TCP

IP header length: 20 bytes

Total IP length: 67

Time to live: 64

Flag: 010

Fragment Offset: 0

TCP Segment:

Source Port: 56788 Destination Port: 23

Sequence Number: 3108926016 Acknowledgment number: 2424181830

TCP Header Length: 32 bytes

Window Size: 5840

Flag: (PSH, ACK)

Urgent Pointer: 0

Option Field: 12

TCP Payload size: 15 bytes

TCP Payload type: Telnet

Data: FF FB 18 FF FB 1F FF FC 23 FF FB 27 FF FC 24 ........#..'..$

Ethernet Frame 193:

Source MAC Address: 08-00-20-AB-D4-A4 Destination MAC Address: 00-C0-4F-8D-93-F2 Ether Type field: IPv4

Frame length : 66 Padding:

IP Packet:

Source IP Address: /192.168.1.22 Destination IP Address: /192.168.1.66

IP Version: 4 Protocol Type: TCP

IP header length: 20 bytes

Total IP length: 52

Time to live: 60

Flag: 010

Fragment Offset: 0

TCP Segment:

Source Port: 23 Destination Port: 56788

Sequence Number: 2424181830 Acknowledgment number: 3108926031

TCP Header Length: 32 bytes

Window Size: 49232

Flag: ACK

Urgent Pointer: 0

Option Field: 12

TCP Payload size: 0 bytes

TCP Payload type: Telnet

Data: No payload

Ethernet Frame 194:

Source MAC Address: 08-00-20-AB-D4-A4 Destination MAC Address: 00-C0-4F-8D-93-F2 Ether Type field: IPv4

Frame length : 84 Padding:

IP Packet:

Source IP Address: /192.168.1.22 Destination IP Address: /192.168.1.66

IP Version: 4 Protocol Type: TCP

IP header length: 20 bytes

Total IP length: 70

Time to live: 60

Flag: 010

Fragment Offset: 0

TCP Segment:

Source Port: 23 Destination Port: 56788

Sequence Number: 2424181830 Acknowledgment number: 3108926031

TCP Header Length: 32 bytes

Window Size: 49232

Flag: (PSH, ACK)

Urgent Pointer: 0

Option Field: 12

TCP Payload size: 18 bytes

TCP Payload type: Telnet

Data: FF FE 23 FF FE 24 FF FA 18 01 FF F0 FF FA 27 01 ..#..$........'.

FF F0 ..

Ethernet Frame 195:

Source MAC Address: 08-00-20-AB-D4-A4 Destination MAC Address: 00-C0-4F-8D-93-F2 Ether Type field: IPv4

Frame length : 66 Padding:

IP Packet:

Source IP Address: /192.168.1.22 Destination IP Address: /192.168.1.66

IP Version: 4 Protocol Type: TCP

IP header length: 20 bytes

Total IP length: 52

Time to live: 60

Flag: 010

Fragment Offset: 0

TCP Segment:

Source Port: 23 Destination Port: 56788

Sequence Number: 2424181848 Acknowledgment number: 3108926048

TCP Header Length: 32 bytes

Window Size: 49232

Flag: ACK

Urgent Pointer: 0

Option Field: 12

TCP Payload size: 0 bytes

TCP Payload type: Telnet

Data: No payload

Ethernet Frame 196:

Source MAC Address: 00-C0-4F-8D-93-F2 Destination MAC Address: 08-00-20-AB-D4-A4 Ether Type field: IPv4

Frame length : 83 Padding:

IP Packet:

Source IP Address: /192.168.1.66 Destination IP Address: /192.168.1.22

IP Version: 4 Protocol Type: TCP

IP header length: 20 bytes

Total IP length: 69

Time to live: 64

Flag: 010

Fragment Offset: 0

TCP Segment:

Source Port: 23 Destination Port: 56788

Sequence Number: 3108926031 Acknowledgment number: 2424181848

TCP Header Length: 32 bytes

Window Size: 5840

Flag: (PSH, ACK)

Urgent Pointer: 0

Option Field: 12

TCP Payload size: 17 bytes

TCP Payload type: Telnet

Data: FF FA 18 00 4C 49 4E 55 58 FF F0 FF FA 27 00 FF ....LINUX....'..

F0 .

Ethernet Frame 197:

Source MAC Address: 08-00-20-AB-D4-A4 Destination MAC Address: 00-C0-4F-8D-93-F2 Ether Type field: IPv4

Frame length : 87 Padding:

IP Packet:

Source IP Address: /192.168.1.22 Destination IP Address: /192.168.1.66

IP Version: 4 Protocol Type: TCP

IP header length: 20 bytes

Total IP length: 73

Time to live: 60

Flag: 010

Fragment Offset: 0

TCP Segment:

Source Port: 23 Destination Port: 56788

Sequence Number: 2424181848 Acknowledgment number: 3108926048

TCP Header Length: 32 bytes

Window Size: 49232

Flag: (PSH, ACK)

Urgent Pointer: 0

Option Field: 12

TCP Payload size: 21 bytes

TCP Payload type: Telnet

Data: 0D 0A 0D 0A 53 75 6E 4F 53 20 35 2E 39 0D 0A 0D ....SunOS 5.9...

00 0D 0A 0D 00 .....

Ethernet Frame 200:

Source MAC Address: 00-C0-4F-8D-93-F2 Destination MAC Address: 08-00-20-AB-D4-A4 Ether Type field: IPv4

Frame length : 66 Padding:

IP Packet:

Source IP Address: /192.168.1.66 Destination IP Address: /192.168.1.22

IP Version: 4 Protocol Type: TCP

IP header length: 20 bytes

Total IP length: 52

Time to live: 64

Flag: 010

Fragment Offset: 0

TCP Segment:

Source Port: 56788 Destination Port: 23

Sequence Number: 3108926048 Acknowledgment number: 2424181878

TCP Header Length: 32 bytes

Window Size: 5840

Flag: ACK

Urgent Pointer: 0

Option Field: 12

TCP Payload size: 0 bytes

TCP Payload type: Telnet

Data: No payload

Ethernet Frame 199:

Source MAC Address: 08-00-20-AB-D4-A4 Destination MAC Address: 00-C0-4F-8D-93-F2 Ether Type field: IPv4

Frame length : 75 Padding:

IP Packet:

Source IP Address: /192.168.1.22 Destination IP Address: /192.168.1.66

IP Version: 4 Protocol Type: TCP

IP header length: 20 bytes

Total IP length: 61

Time to live: 60

Flag: 010

Fragment Offset: 0

TCP Segment:

Source Port: 56788 Destination Port: 23

Sequence Number: 2424181869 Acknowledgment number: 3108926048

TCP Header Length: 32 bytes

Window Size: 49232

Flag: (PSH, ACK)

Urgent Pointer: 0

Option Field: 12

TCP Payload size: 9 bytes

TCP Payload type: Telnet

Data: FF FB 01 FF FB 03 FF FD 01 .........

Ethernet Frame 198:

Source MAC Address: 00-C0-4F-8D-93-F2 Destination MAC Address: 08-00-20-AB-D4-A4 Ether Type field: IPv4

Frame length : 66 Padding:

IP Packet:

Source IP Address: /192.168.1.66 Destination IP Address: /192.168.1.22

IP Version: 4 Protocol Type: TCP

IP header length: 20 bytes

Total IP length: 52

Time to live: 64

Flag: 010

Fragment Offset: 0

TCP Segment:

Source Port: 56788 Destination Port: 23

Sequence Number: 3108926048 Acknowledgment number: 2424181869

TCP Header Length: 32 bytes

Window Size: 5840

Flag: ACK

Urgent Pointer: 0

Option Field: 12

TCP Payload size: 0 bytes

TCP Payload type: other

Data: No payload

Ethernet Frame 201:

Source MAC Address: 00-C0-4F-8D-93-F2 Destination MAC Address: 08-00-20-AB-D4-A4 Ether Type field: IPv4

Frame length : 75 Padding:

IP Packet:

Source IP Address: /192.168.1.66 Destination IP Address: /192.168.1.22

IP Version: 4 Protocol Type: TCP

IP header length: 20 bytes

Total IP length: 61

Time to live: 64

Flag: 010

Fragment Offset: 0

TCP Segment:

Source Port: 56788 Destination Port: 23

Sequence Number: 3108926048 Acknowledgment number: 2424181878

TCP Header Length: 32 bytes

Window Size: 5840

Flag: (PSH, ACK)

Urgent Pointer: 0

Option Field: 12

TCP Payload size: 9 bytes

TCP Payload type: Telnet

Data: FF FD 01 FF FD 03 FF FC 01 .........

Ethernet Frame 202:

Source MAC Address: 08-00-20-AB-D4-A4 Destination MAC Address: 00-C0-4F-8D-93-F2 Ether Type field: IPv4

Frame length : 69 Padding:

IP Packet:

Source IP Address: /192.168.1.22 Destination IP Address: /192.168.1.66

IP Version: 4 Protocol Type: TCP

IP header length: 20 bytes

Total IP length: 55

Time to live: 60

Flag: 010

Fragment Offset: 0

TCP Segment:

Source Port: 23 Destination Port: 56788

Sequence Number: 2424181878 Acknowledgment number: 3108926057

TCP Header Length: 32 bytes

Window Size: 49232

Flag: (PSH, ACK)

Urgent Pointer: 0

Option Field: 12

TCP Payload size: 3 bytes

TCP Payload type: Telnet

Data: FF FE 01 ...

Ethernet Frame 206:

Source MAC Address: 00-C0-4F-8D-93-F2 Destination MAC Address: 08-00-20-AB-D4-A4 Ether Type field: IPv4

Frame length : 66 Padding:

IP Packet:

Source IP Address: /192.168.1.66 Destination IP Address: /192.168.1.22

IP Version: 4 Protocol Type: TCP

IP header length: 20 bytes

Total IP length: 52

Time to live: 64

Flag: 010

Fragment Offset: 0

TCP Segment:

Source Port: 56788 Destination Port: 23

Sequence Number: 3108926057 Acknowledgment number: 2424181881

TCP Header Length: 32 bytes

Window Size: 5840

Flag: ACK

Urgent Pointer: 0

Option Field: 12

TCP Payload size: 0 bytes

TCP Payload type: Telnet

Data: No payload

Ethernet Frame 205:

Source MAC Address: 08-00-20-AB-D4-A4 Destination MAC Address: 00-C0-4F-8D-93-F2 Ether Type field: IPv4

Frame length : 73 Padding:

IP Packet:

Source IP Address: /192.168.1.22 Destination IP Address: /192.168.1.66

IP Version: 4 Protocol Type: TCP

IP header length: 20 bytes

Total IP length: 59

Time to live: 60

Flag: 010

Fragment Offset: 0

TCP Segment:

Source Port: 23 Destination Port: 56788

Sequence Number: 2424181881 Acknowledgment number: 3108926057

TCP Header Length: 32 bytes

Window Size: 49232

Flag: (PSH, ACK)

Urgent Pointer: 0

Option Field: 12

TCP Payload size: 7 bytes

TCP Payload type: Telnet

Data: 6C 6F 67 69 6E 3A 20 login:

Ethernet Frame 203:

Source MAC Address: 00-C0-4F-8D-93-F2 Destination MAC Address: 08-00-20-AB-D4-A4 Ether Type field: IPv4

Frame length : 66 Padding:

IP Packet:

Source IP Address: /192.168.1.66 Destination IP Address: /192.168.1.22

IP Version: 4 Protocol Type: TCP

IP header length: 20 bytes

Total IP length: 52

Time to live: 64

Flag: 010

Fragment Offset: 0

TCP Segment:

Source Port: 23 Destination Port: 56788

Sequence Number: 3108926057 Acknowledgment number: 2424181888

TCP Header Length: 32 bytes

Window Size: 5840

Flag: ACK

Urgent Pointer: 0

Option Field: 12

TCP Payload size: 0 bytes

TCP Payload type: Telnet

Data: No payload

Ethernet Frame 204:

Source MAC Address: 00-C0-4F-8D-93-F2 Destination MAC Address: 08-00-20-AB-D4-A4 Ether Type field: IPv4

Frame length : 74 Padding:

IP Packet:

Source IP Address: /192.168.1.66 Destination IP Address: /192.168.1.22

IP Version: 4 Protocol Type: TCP

IP header length: 20 bytes

Total IP length: 60

Time to live: 64

Flag: 010

Fragment Offset: 0

TCP Segment:

Source Port: 23 Destination Port: 56788

Sequence Number: 3108926057 Acknowledgment number: 2424181888

TCP Header Length: 32 bytes

Window Size: 5840

Flag: (PSH, ACK)

Urgent Pointer: 0

Option Field: 12

TCP Payload size: 8 bytes

TCP Payload type: Telnet

Data: 67 72 6F 75 70 31 35 0A group15.

Ethernet Frame 207:

Source MAC Address: 00-C0-4F-8D-93-F2 Destination MAC Address: 08-00-20-AB-D4-A4 Ether Type field: IPv4

Frame length : 66 Padding:

IP Packet:

Source IP Address: /192.168.1.66 Destination IP Address: /192.168.1.22

IP Version: 4 Protocol Type: TCP

IP header length: 20 bytes

Total IP length: 52

Time to live: 64

Flag: 010

Fragment Offset: 0

TCP Segment:

Source Port: 56788 Destination Port: 56788

Sequence Number: 3108926065 Acknowledgment number: 2424181897

TCP Header Length: 32 bytes

Window Size: 5840

Flag: ACK

Urgent Pointer: 0

Option Field: 12

TCP Payload size: 0 bytes

TCP Payload type: Telnet

Data: No payload

Ethernet Frame 208:

Source MAC Address: 08-00-20-AB-D4-A4 Destination MAC Address: 00-C0-4F-8D-93-F2 Ether Type field: IPv4

Frame length : 75 Padding:

IP Packet:

Source IP Address: /192.168.1.22 Destination IP Address: /192.168.1.66

IP Version: 4 Protocol Type: TCP

IP header length: 20 bytes

Total IP length: 61

Time to live: 60

Flag: 010

Fragment Offset: 0

TCP Segment:

Source Port: 23 Destination Port: 56788

Sequence Number: 2424181888 Acknowledgment number: 3108926065

TCP Header Length: 32 bytes

Window Size: 49232

Flag: (PSH, ACK)

Urgent Pointer: 0

Option Field: 12

TCP Payload size: 9 bytes

TCP Payload type: Telnet

Data: 67 72 6F 75 70 31 35 0D 0A group15..

Ethernet Frame 210:

Source MAC Address: 08-00-20-AB-D4-A4 Destination MAC Address: 00-C0-4F-8D-93-F2 Ether Type field: IPv4

Frame length : 76 Padding:

IP Packet:

Source IP Address: /192.168.1.22 Destination IP Address: /192.168.1.66

IP Version: 4 Protocol Type: TCP

IP header length: 20 bytes

Total IP length: 62

Time to live: 60

Flag: 010

Fragment Offset: 0

TCP Segment:

Source Port: 56788 Destination Port: 23

Sequence Number: 2424181897 Acknowledgment number: 3108926065

TCP Header Length: 32 bytes

Window Size: 49232

Flag: (PSH, ACK)

Urgent Pointer: 0

Option Field: 12

TCP Payload size: 10 bytes

TCP Payload type: Telnet

Data: 50 61 73 73 77 6F 72 64 3A 20 Password:

Ethernet Frame 211:

Source MAC Address: 00-C0-4F-8D-93-F2 Destination MAC Address: 08-00-20-AB-D4-A4 Ether Type field: IPv4

Frame length : 79 Padding:

IP Packet:

Source IP Address: /192.168.1.66 Destination IP Address: /192.168.1.22

IP Version: 4 Protocol Type: TCP

IP header length: 20 bytes

Total IP length: 65

Time to live: 64

Flag: 010

Fragment Offset: 0

TCP Segment:

Source Port: 56788 Destination Port: 23

Sequence Number: 3108926065 Acknowledgment number: 2424181907

TCP Header Length: 32 bytes

Window Size: 5840

Flag: (PSH, ACK)

Urgent Pointer: 0

Option Field: 12

TCP Payload size: 13 bytes

TCP Payload type: Telnet

Data: 31 39 32 2E 31 36 38 2E 31 2E 36 36 0A 192.168.1.66.

Ethernet Frame 209:

Source MAC Address: 00-C0-4F-8D-93-F2 Destination MAC Address: 08-00-20-AB-D4-A4 Ether Type field: IPv4

Frame length : 66 Padding:

IP Packet:

Source IP Address: /192.168.1.66 Destination IP Address: /192.168.1.22

IP Version: 4 Protocol Type: TCP

IP header length: 20 bytes

Total IP length: 52

Time to live: 64

Flag: 010

Fragment Offset: 0

TCP Segment:

Source Port: 56788 Destination Port: 23

Sequence Number: 3108926065 Acknowledgment number: 2424181907

TCP Header Length: 32 bytes

Window Size: 5840

Flag: ACK

Urgent Pointer: 0

Option Field: 12

TCP Payload size: 0 bytes

TCP Payload type: Telnet

Data: No payload

Ethernet Frame 212:

Source MAC Address: 08-00-20-AB-D4-A4 Destination MAC Address: 00-C0-4F-8D-93-F2 Ether Type field: IPv4

Frame length : 68 Padding:

IP Packet:

Source IP Address: /192.168.1.22 Destination IP Address: /192.168.1.66

IP Version: 4 Protocol Type: TCP

IP header length: 20 bytes

Total IP length: 54

Time to live: 60

Flag: 010

Fragment Offset: 0

TCP Segment:

Source Port: 23 Destination Port: 56788

Sequence Number: 2424181907 Acknowledgment number: 3108926078

TCP Header Length: 32 bytes

Window Size: 49232

Flag: (PSH, ACK)

Urgent Pointer: 0

Option Field: 12

TCP Payload size: 2 bytes

TCP Payload type: Telnet

Data: 0D 0A ..

Ethernet Frame 214:

Source MAC Address: 08-00-20-AB-D4-A4 Destination MAC Address: 00-C0-4F-8D-93-F2 Ether Type field: IPv4

Frame length : 120 Padding:

IP Packet:

Source IP Address: /192.168.1.22 Destination IP Address: /192.168.1.66

IP Version: 4 Protocol Type: TCP

IP header length: 20 bytes

Total IP length: 106

Time to live: 60

Flag: 010

Fragment Offset: 0

TCP Segment:

Source Port: 56788 Destination Port: 23

Sequence Number: 2424181909 Acknowledgment number: 3108926078

TCP Header Length: 32 bytes

Window Size: 49232

Flag: (PSH, ACK)

Urgent Pointer: 0

Option Field: 12

TCP Payload size: 54 bytes

TCP Payload type: Telnet

Data: 4C 61 73 74 20 6C 6F 67 69 6E 3A 20 57 65 64 20 Last login: Wed

4A 61 6E 20 31 39 20 31 30 3A 31 31 3A 32 31 20 Jan 19 10:11:21

66 72 6F 6D 20 6C 61 6E 74 68 61 6E 75 6D 2E 67 from lanthanum.g

72 6F 75 70 0D 0A roup..

Ethernet Frame 213:

Source MAC Address: 00-C0-4F-8D-93-F2 Destination MAC Address: 08-00-20-AB-D4-A4 Ether Type field: IPv4

Frame length : 66 Padding:

IP Packet:

Source IP Address: /192.168.1.66 Destination IP Address: /192.168.1.22

IP Version: 4 Protocol Type: TCP

IP header length: 20 bytes

Total IP length: 52

Time to live: 64

Flag: 010

Fragment Offset: 0

TCP Segment:

Source Port: 56788 Destination Port: 23

Sequence Number: 3108926078 Acknowledgment number: 2424181909

TCP Header Length: 32 bytes

Window Size: 5840

Flag: ACK

Urgent Pointer: 0

Option Field: 12

TCP Payload size: 0 bytes

TCP Payload type: Telnet

Data: No payload

Ethernet Frame 215:

Source MAC Address: 00-C0-4F-8D-93-F2 Destination MAC Address: 08-00-20-AB-D4-A4 Ether Type field: IPv4

Frame length : 66 Padding:

IP Packet:

Source IP Address: /192.168.1.66 Destination IP Address: /192.168.1.22

IP Version: 4 Protocol Type: TCP

IP header length: 20 bytes

Total IP length: 52

Time to live: 64

Flag: 010

Fragment Offset: 0

TCP Segment:

Source Port: 56788 Destination Port: 23

Sequence Number: 3108926078 Acknowledgment number: 2424181963

TCP Header Length: 32 bytes

Window Size: 5840

Flag: ACK

Urgent Pointer: 0

Option Field: 12

TCP Payload size: 0 bytes

TCP Payload type: Telnet

Data: No payload

Ethernet Frame 217:

Source MAC Address: 00-C0-4F-8D-93-F2 Destination MAC Address: 08-00-20-AB-D4-A4 Ether Type field: IPv4

Frame length : 74 Padding:

IP Packet:

Source IP Address: /192.168.1.66 Destination IP Address: /192.168.1.22

IP Version: 4 Protocol Type: TCP

IP header length: 20 bytes

Total IP length: 60

Time to live: 64

Flag: 010

Fragment Offset: 0

TCP Segment:

Source Port: 56788 Destination Port: 23

Sequence Number: 3108926078 Acknowledgment number: 2424181965

TCP Header Length: 32 bytes

Window Size: 5840

Flag: (PSH, ACK)

Urgent Pointer: 0

Option Field: 12

TCP Payload size: 8 bytes

TCP Payload type: Telnet

Data: 6C 73 20 2F 74 6D 70 0A ls /tmp.

Ethernet Frame 216:

Source MAC Address: 00-C0-4F-8D-93-F2 Destination MAC Address: 08-00-20-AB-D4-A4 Ether Type field: IPv4

Frame length : 66 Padding:

IP Packet:

Source IP Address: /192.168.1.66 Destination IP Address: /192.168.1.22

IP Version: 4 Protocol Type: TCP

IP header length: 20 bytes

Total IP length: 52

Time to live: 64

Flag: 010

Fragment Offset: 0

TCP Segment:

Source Port: 56788 Destination Port: 23

Sequence Number: 3108926078 Acknowledgment number: 2424181965

TCP Header Length: 32 bytes

Window Size: 5840

Flag: ACK

Urgent Pointer: 0

Option Field: 12

TCP Payload size: 0 bytes

TCP Payload type: Telnet

Data: No payload

Ethernet Frame 218:

Source MAC Address: 08-00-20-AB-D4-A4 Destination MAC Address: 00-C0-4F-8D-93-F2 Ether Type field: IPv4

Frame length : 68 Padding:

IP Packet:

Source IP Address: /192.168.1.22 Destination IP Address: /192.168.1.66

IP Version: 4 Protocol Type: TCP

IP header length: 20 bytes

Total IP length: 54

Time to live: 60

Flag: 010

Fragment Offset: 0

TCP Segment:

Source Port: 56788 Destination Port: 23

Sequence Number: 2424181963 Acknowledgment number: 3108926078

TCP Header Length: 32 bytes

Window Size: 49232

Flag: (PSH, ACK)

Urgent Pointer: 0

Option Field: 12

TCP Payload size: 2 bytes

TCP Payload type: Telnet

Data: 24 20 $

Ethernet Frame 219:

Source MAC Address: 08-00-20-AB-D4-A4 Destination MAC Address: 00-C0-4F-8D-93-F2 Ether Type field: IPv4

Frame length : 75 Padding:

IP Packet:

Source IP Address: /192.168.1.22 Destination IP Address: /192.168.1.66

IP Version: 4 Protocol Type: TCP

IP header length: 20 bytes

Total IP length: 61

Time to live: 60

Flag: 010

Fragment Offset: 0

TCP Segment:

Source Port: 23 Destination Port: 56788

Sequence Number: 2424181965 Acknowledgment number: 3108926086

TCP Header Length: 32 bytes

Window Size: 49232

Flag: (PSH, ACK)

Urgent Pointer: 0

Option Field: 12

TCP Payload size: 9 bytes

TCP Payload type: Telnet

Data: 6C 73 20 2F 74 6D 70 0D 0A ls /tmp..

Ethernet Frame 220:

Source MAC Address: 00-C0-4F-8D-93-F2 Destination MAC Address: 08-00-20-AB-D4-A4 Ether Type field: IPv4

Frame length : 66 Padding:

IP Packet:

Source IP Address: /192.168.1.66 Destination IP Address: /192.168.1.22

IP Version: 4 Protocol Type: TCP

IP header length: 20 bytes

Total IP length: 52

Time to live: 64

Flag: 010

Fragment Offset: 0

TCP Segment:

Source Port: 56788 Destination Port: 23

Sequence Number: 3108926086 Acknowledgment number: 2424181974

TCP Header Length: 32 bytes

Window Size: 5840

Flag: ACK

Urgent Pointer: 0

Option Field: 12

TCP Payload size: 0 bytes

TCP Payload type: Telnet

Data: No payload

Ethernet Frame 222:

Source MAC Address: 08-00-20-AB-D4-A4 Destination MAC Address: 00-C0-4F-8D-93-F2 Ether Type field: IPv4

Frame length : 112 Padding:

IP Packet:

Source IP Address: /192.168.1.22 Destination IP Address: /192.168.1.66

IP Version: 4 Protocol Type: TCP

IP header length: 20 bytes

Total IP length: 98

Time to live: 60

Flag: 010

Fragment Offset: 0

TCP Segment:

Source Port: 56788 Destination Port: 23

Sequence Number: 2424181974 Acknowledgment number: 3108926086

TCP Header Length: 32 bytes

Window Size: 49232

Flag: (PSH, ACK)

Urgent Pointer: 0

Option Field: 12

TCP Payload size: 46 bytes

TCP Payload type: Telnet

Data: 68 73 70 65 72 66 64 61 74 61 5F 72 6F 6F 74 20 hsperfdata\_root

20 73 70 65 63 6B 65 79 73 64 2E 6C 6F 63 6B 20 speckeysd.lock

20 20 77 67 30 30 30 30 30 30 30 34 0D 0A wg00000004..

Ethernet Frame 221:

Source MAC Address: 00-C0-4F-8D-93-F2 Destination MAC Address: 08-00-20-AB-D4-A4 Ether Type field: IPv4

Frame length : 66 Padding:

IP Packet:

Source IP Address: /192.168.1.66 Destination IP Address: /192.168.1.22

IP Version: 4 Protocol Type: TCP

IP header length: 20 bytes

Total IP length: 52

Time to live: 64

Flag: 010

Fragment Offset: 0

TCP Segment:

Source Port: 56788 Destination Port: 23

Sequence Number: 3108926086 Acknowledgment number: 2424182020

TCP Header Length: 32 bytes

Window Size: 5840

Flag: ACK

Urgent Pointer: 0

Option Field: 12

TCP Payload size: 0 bytes

TCP Payload type: Telnet

Data: No payload

Ethernet Frame 223:

Source MAC Address: 00-C0-4F-8D-93-F2 Destination MAC Address: 08-00-20-AB-D4-A4 Ether Type field: IPv4

Frame length : 66 Padding:

IP Packet:

Source IP Address: /192.168.1.66 Destination IP Address: /192.168.1.22

IP Version: 4 Protocol Type: TCP

IP header length: 20 bytes

Total IP length: 52

Time to live: 64

Flag: 010

Fragment Offset: 0

TCP Segment:

Source Port: 56788 Destination Port: 23

Sequence Number: 3108926086 Acknowledgment number: 2424182066

TCP Header Length: 32 bytes

Window Size: 5840

Flag: ACK

Urgent Pointer: 0

Option Field: 12

TCP Payload size: 0 bytes

TCP Payload type: Telnet

Data: No payload

Ethernet Frame 224:

Source MAC Address: 08-00-20-AB-D4-A4 Destination MAC Address: 00-C0-4F-8D-93-F2 Ether Type field: IPv4

Frame length : 112 Padding:

IP Packet:

Source IP Address: /192.168.1.22 Destination IP Address: /192.168.1.66

IP Version: 4 Protocol Type: TCP

IP header length: 20 bytes

Total IP length: 98

Time to live: 60

Flag: 010

Fragment Offset: 0

TCP Segment:

Source Port: 56788 Destination Port: 23

Sequence Number: 2424182020 Acknowledgment number: 3108926086

TCP Header Length: 32 bytes

Window Size: 49232

Flag: (PSH, ACK)

Urgent Pointer: 0

Option Field: 12

TCP Payload size: 46 bytes

TCP Payload type: Telnet

Data: 6F 72 62 69 74 2D 72 6F 6F 74 20 20 20 20 20 20 orbit-root

20 77 67 30 30 30 30 30 30 30 33 20 20 20 20 20 wg00000003

20 20 77 67 30 30 30 30 30 30 30 35 0D 0A wg00000005..

Ethernet Frame 225:

Source MAC Address: 08-00-20-AB-D4-A4 Destination MAC Address: 00-C0-4F-8D-93-F2 Ether Type field: IPv4

Frame length : 68 Padding:

IP Packet:

Source IP Address: /192.168.1.22 Destination IP Address: /192.168.1.66

IP Version: 4 Protocol Type: TCP

IP header length: 20 bytes

Total IP length: 54

Time to live: 60

Flag: 010

Fragment Offset: 0

TCP Segment:

Source Port: 23 Destination Port: 56788

Sequence Number: 2424182066 Acknowledgment number: 3108926086

TCP Header Length: 32 bytes

Window Size: 49232

Flag: (PSH, ACK)

Urgent Pointer: 0

Option Field: 12

TCP Payload size: 2 bytes

TCP Payload type: Telnet

Data: 24 20 $

Ethernet Frame 226:

Source MAC Address: 00-C0-4F-8D-93-F2 Destination MAC Address: 08-00-20-AB-D4-A4 Ether Type field: IPv4

Frame length : 66 Padding:

IP Packet:

Source IP Address: /192.168.1.66 Destination IP Address: /192.168.1.22

IP Version: 4 Protocol Type: TCP

IP header length: 20 bytes

Total IP length: 52

Time to live: 64

Flag: 010

Fragment Offset: 0

TCP Segment:

Source Port: 56788 Destination Port: 23

Sequence Number: 3108926086 Acknowledgment number: 2424182068

TCP Header Length: 32 bytes

Window Size: 5840

Flag: ACK

Urgent Pointer: 0

Option Field: 12

TCP Payload size: 0 bytes

TCP Payload type: Telnet

Data: No payload

Ethernet Frame 227:

Source MAC Address: 00-C0-4F-8D-93-F2 Destination MAC Address: 08-00-20-AB-D4-A4 Ether Type field: IPv4

Frame length : 66 Padding:

IP Packet:

Source IP Address: /192.168.1.66 Destination IP Address: /192.168.1.22

IP Version: 4 Protocol Type: TCP

IP header length: 20 bytes

Total IP length: 52

Time to live: 64

Flag: 010

Fragment Offset: 0

TCP Segment:

Source Port: 56788 Destination Port: 23

Sequence Number: 3108926086 Acknowledgment number: 2424182068

TCP Header Length: 32 bytes

Window Size: 5840

Flag: (FIN, ACK)

Urgent Pointer: 0

Option Field: 12

TCP Payload size: 0 bytes

TCP Payload type: Telnet

Data: No payload

Ethernet Frame 228:

Source MAC Address: 08-00-20-AB-D4-A4 Destination MAC Address: 00-C0-4F-8D-93-F2 Ether Type field: IPv4

Frame length : 66 Padding:

IP Packet:

Source IP Address: /192.168.1.22 Destination IP Address: /192.168.1.66

IP Version: 4 Protocol Type: TCP

IP header length: 20 bytes

Total IP length: 52

Time to live: 60

Flag: 010

Fragment Offset: 0

TCP Segment:

Source Port: 23 Destination Port: 56788

Sequence Number: 2424182068 Acknowledgment number: 3108926087

TCP Header Length: 32 bytes

Window Size: 49232

Flag: ACK

Urgent Pointer: 0

Option Field: 12

TCP Payload size: 0 bytes

TCP Payload type: Telnet

Data: No payload

Ethernet Frame 229:

Source MAC Address: 08-00-20-AB-D4-A4 Destination MAC Address: 00-C0-4F-8D-93-F2 Ether Type field: IPv4

Frame length : 66 Padding:

IP Packet:

Source IP Address: /192.168.1.22 Destination IP Address: /192.168.1.66

IP Version: 4 Protocol Type: TCP

IP header length: 20 bytes

Total IP length: 52

Time to live: 60

Flag: 010

Fragment Offset: 0

TCP Segment:

Source Port: 23 Destination Port: 56788

Sequence Number: 2424182068 Acknowledgment number: 3108926087

TCP Header Length: 32 bytes

Window Size: 49232

Flag: (FIN, ACK)

Urgent Pointer: 0

Option Field: 12

TCP Payload size: 0 bytes

TCP Payload type: Telnet

Data: No payload

Ethernet Frame 230:

Source MAC Address: 00-C0-4F-8D-93-F2 Destination MAC Address: 08-00-20-AB-D4-A4 Ether Type field: IPv4

Frame length : 66 Padding:

IP Packet:

Source IP Address: /192.168.1.66 Destination IP Address: /192.168.1.22

IP Version: 4 Protocol Type: TCP

IP header length: 20 bytes

Total IP length: 52

Time to live: 64

Flag: 010

Fragment Offset: 0

TCP Segment:

Source Port: 56788 Destination Port: 23

Sequence Number: 3108926087 Acknowledgment number: 2424182069

TCP Header Length: 32 bytes

Window Size: 5840

Flag: ACK

Urgent Pointer: 0

Option Field: 12

TCP Payload size: 0 bytes

TCP Payload type: Telnet

Data: No payload

Ethernet Frame 231:

Source MAC Address: 00-C0-4F-8D-93-F2 Destination MAC Address: 08-00-20-AB-D4-A4 Ether Type field: IPv4

Frame length : 74 Padding:

IP Packet:

Source IP Address: /192.168.1.66 Destination IP Address: /192.168.1.22

IP Version: 4 Protocol Type: TCP

IP header length: 20 bytes

Total IP length: 60

Time to live: 64

Flag: 000

Fragment Offset: 0

TCP Segment:

Source Port: 56788 Destination Port: 23

Sequence Number: 3108926015 Acknowledgment number: 0

TCP Header Length: 40 bytes

Window Size: 5840

Flag: SYN

Urgent Pointer: 0

Option Field: 20

TCP Payload size: 0 bytes

TCP Payload type: Telnet

Data: No payload

Ethernet Frame 232:

Source MAC Address: 08-00-20-AB-D4-A4 Destination MAC Address: 00-C0-4F-8D-93-F2 Ether Type field: IPv4

Frame length : 78 Padding:

IP Packet:

Source IP Address: /192.168.1.22 Destination IP Address: /192.168.1.66

IP Version: 4 Protocol Type: TCP

IP header length: 20 bytes

Total IP length: 64

Time to live: 60

Flag: 010

Fragment Offset: 0

TCP Segment:

Source Port: 23 Destination Port: 56788

Sequence Number: 2424181814 Acknowledgment number: 3108926016

TCP Header Length: 44 bytes

Window Size: 49232

Flag: (SYN, ACK)

Urgent Pointer: 0

Option Field: 24

TCP Payload size: 0 bytes

TCP Payload type: Telnet

Data: No payload

Ethernet Frame 233:

Source MAC Address: 00-C0-4F-8D-93-F2 Destination MAC Address: 08-00-20-AB-D4-A4 Ether Type field: IPv4

Frame length : 66 Padding:

IP Packet:

Source IP Address: /192.168.1.66 Destination IP Address: /192.168.1.22

IP Version: 4 Protocol Type: TCP

IP header length: 20 bytes

Total IP length: 52

Time to live: 64

Flag: 000

Fragment Offset: 0

TCP Segment:

Source Port: 23 Destination Port: 56788

Sequence Number: 3108926016 Acknowledgment number: 2424181815

TCP Header Length: 32 bytes

Window Size: 5840

Flag: ACK

Urgent Pointer: 0

Option Field: 12

TCP Payload size: 0 bytes

TCP Payload type: other

Data: No payload

Ethernet Frame 234:

Source MAC Address: 08-00-20-AB-D4-A4 Destination MAC Address: 00-C0-4F-8D-93-F2 Ether Type field: IPv4

Frame length : 66 Padding:

IP Packet:

Source IP Address: /192.168.1.22 Destination IP Address: /192.168.1.66

IP Version: 4 Protocol Type: TCP

IP header length: 20 bytes

Total IP length: 52

Time to live: 60

Flag: 001

Fragment Offset: 0

TCP Segment:

Source Port: 23 Destination Port: 56788

Sequence Number: 2424181815 Acknowledgment number: 3108926016

TCP Header Length: 32 bytes

Window Size: 49232

Flag: (PSH, ACK)

Urgent Pointer: 0

Option Field: 12

TCP Payload size: 0 bytes

TCP Payload type: Telnet

Data: No payload

Ethernet Frame 235:

Source MAC Address: 00-C0-4F-8D-93-F2 Destination MAC Address: 08-00-20-AB-D4-A4 Ether Type field: IPv4

Frame length : 66 Padding:

IP Packet:

Source IP Address: /192.168.1.66 Destination IP Address: /192.168.1.22

IP Version: 4 Protocol Type: TCP

IP header length: 20 bytes

Total IP length: 52

Time to live: 64

Flag: 000

Fragment Offset: 0

TCP Segment:

Source Port: 56788 Destination Port: 23

Sequence Number: 3108926016 Acknowledgment number: 2424181830

TCP Header Length: 32 bytes

Window Size: 5840

Flag: ACK

Urgent Pointer: 0

Option Field: 12

TCP Payload size: 0 bytes

TCP Payload type: Telnet

Data: No payload

Ethernet Frame 236:

Source MAC Address: 08-00-20-AB-D4-A4 Destination MAC Address: 00-C0-4F-8D-93-F2 Ether Type field: IPv4

Frame length : 60 Padding: 000000000000

IP Packet:

Source IP Address: /192.168.1.22 Destination IP Address: /192.168.1.66

IP Version: 4 Protocol Type: TCP

IP header length: 20 bytes

Total IP length: 27

Time to live: 60

Flag: 000

Fragment Offset: 5

TCP Segment:

Source Port: 9215 Destination Port: 64807

Sequence Number: 4294779904 Acknowledgment number: 0

TCP Header Length: 0 bytes

Window Size: 0

Flag: other

Urgent Pointer: 0

Option Field: 0

TCP Payload size: 0 bytes

TCP Payload type: other

Data: No payload

Ethernet Frame 237:

Source MAC Address: 08-00-20-AB-D4-A4 Destination MAC Address: 00-C0-4F-8D-93-F2 Ether Type field: IPv4

Frame length : 60 Padding: 000000000000

IP Packet:

Source IP Address: /192.168.1.22 Destination IP Address: /192.168.1.66

IP Version: 4 Protocol Type: TCP

IP header length: 20 bytes

Total IP length: 28

Time to live: 60

Flag: 001

Fragment Offset: 4

TCP Segment:

Source Port: 65533 Destination Port: 6399

Sequence Number: 4246732797 Acknowledgment number: 0

TCP Header Length: 0 bytes

Window Size: 0

Flag: other

Urgent Pointer: 0

Option Field: 0

TCP Payload size: 0 bytes

TCP Payload type: other

Data: No payload

Ethernet Frame 238:

Source MAC Address: 00-C0-4F-8D-93-F2 Destination MAC Address: 08-00-20-AB-D4-A4 Ether Type field: IPv4

Frame length : 66 Padding:

IP Packet:

Source IP Address: /192.168.1.66 Destination IP Address: /192.168.1.22

IP Version: 4 Protocol Type: TCP

IP header length: 20 bytes

Total IP length: 52

Time to live: 64

Flag: 001

Fragment Offset: 0

TCP Segment:

Source Port: 65531 Destination Port: 65520

Sequence Number: 3108926016 Acknowledgment number: 2424181830

TCP Header Length: 32 bytes

Window Size: 5840

Flag: (PSH, ACK)

Urgent Pointer: 0

Option Field: 12

TCP Payload size: 0 bytes

TCP Payload type: Telnet

Data: No payload

Ethernet Frame 242:

Source MAC Address: 08-00-20-AB-D4-A4 Destination MAC Address: 00-C0-4F-8D-93-F2 Ether Type field: IPv4

Frame length : 60 Padding: 000000000000

IP Packet:

Source IP Address: /192.168.1.22 Destination IP Address: /192.168.1.66

IP Version: 4 Protocol Type: TCP

IP header length: 20 bytes

Total IP length: 28

Time to live: 60

Flag: 001

Fragment Offset: 4

TCP Segment:

Source Port: 65534 Destination Port: 9215

Sequence Number: 4263837690 Acknowledgment number: 0

TCP Header Length: 0 bytes

Window Size: 0

Flag: other

Urgent Pointer: 0

Option Field: 0

TCP Payload size: 0 bytes

TCP Payload type: other

Data: No payload

Ethernet Frame 241:

Source MAC Address: 00-C0-4F-8D-93-F2 Destination MAC Address: 08-00-20-AB-D4-A4 Ether Type field: IPv4

Frame length : 60 Padding: 000000000000

IP Packet:

Source IP Address: /192.168.1.66 Destination IP Address: /192.168.1.22

IP Version: 4 Protocol Type: TCP

IP header length: 20 bytes

Total IP length: 27

Time to live: 64

Flag: 000

Fragment Offset: 5

TCP Segment:

Source Port: 9215 Destination Port: 64295

Sequence Number: 4294714368 Acknowledgment number: 0

TCP Header Length: 0 bytes

Window Size: 0

Flag: other

Urgent Pointer: 0

Option Field: 0

TCP Payload size: 0 bytes

TCP Payload type: other

Data: No payload

Ethernet Frame 240:

Source MAC Address: 08-00-20-AB-D4-A4 Destination MAC Address: 00-C0-4F-8D-93-F2 Ether Type field: IPv4

Frame length : 60 Padding: 000000000000

IP Packet:

Source IP Address: /192.168.1.22 Destination IP Address: /192.168.1.66

IP Version: 4 Protocol Type: TCP

IP header length: 20 bytes

Total IP length: 28

Time to live: 60

Flag: 001

Fragment Offset: 5

TCP Segment:

Source Port: 6145 Destination Port: 65520

Sequence Number: 4294584065 Acknowledgment number: 0

TCP Header Length: 0 bytes

Window Size: 0

Flag: other

Urgent Pointer: 0

Option Field: 0

TCP Payload size: 0 bytes

TCP Payload type: other

Data: No payload

Ethernet Frame 239:

Source MAC Address: 00-C0-4F-8D-93-F2 Destination MAC Address: 08-00-20-AB-D4-A4 Ether Type field: IPv4

Frame length : 60 Padding: 000000000000

IP Packet:

Source IP Address: /192.168.1.66 Destination IP Address: /192.168.1.22

IP Version: 4 Protocol Type: TCP

IP header length: 20 bytes

Total IP length: 28

Time to live: 64

Flag: 001

Fragment Offset: 4

TCP Segment:

Source Port: 6145 Destination Port: 65520

Sequence Number: 4213178364 Acknowledgment number: 0

TCP Header Length: 0 bytes

Window Size: 0

Flag: other

Urgent Pointer: 0

Option Field: 0

TCP Payload size: 0 bytes

TCP Payload type: other

Data: No payload

Ethernet Frame 244:

Source MAC Address: 08-00-20-AB-D4-A4 Destination MAC Address: 00-C0-4F-8D-93-F2 Ether Type field: IPv4

Frame length : 66 Padding:

IP Packet:

Source IP Address: /192.168.1.22 Destination IP Address: /192.168.1.66

IP Version: 4 Protocol Type: TCP

IP header length: 20 bytes

Total IP length: 52

Time to live: 60

Flag: 001

Fragment Offset: 0

TCP Segment:

Source Port: 23 Destination Port: 56788

Sequence Number: 2424181830 Acknowledgment number: 3108926031

TCP Header Length: 32 bytes

Window Size: 49232

Flag: (PSH, ACK)

Urgent Pointer: 0

Option Field: 12

TCP Payload size: 0 bytes

TCP Payload type: Telnet

Data: No payload

Ethernet Frame 243:

Source MAC Address: 08-00-20-AB-D4-A4 Destination MAC Address: 00-C0-4F-8D-93-F2 Ether Type field: IPv4

Frame length : 66 Padding:

IP Packet:

Source IP Address: /192.168.1.22 Destination IP Address: /192.168.1.66

IP Version: 4 Protocol Type: TCP

IP header length: 20 bytes

Total IP length: 52

Time to live: 60

Flag: 000

Fragment Offset: 0

TCP Segment:

Source Port: 23 Destination Port: 56788

Sequence Number: 2424181830 Acknowledgment number: 3108926031

TCP Header Length: 32 bytes

Window Size: 49232

Flag: ACK

Urgent Pointer: 0

Option Field: 12

TCP Payload size: 0 bytes

TCP Payload type: Telnet

Data: No payload

Ethernet Frame 245:

Source MAC Address: 08-00-20-AB-D4-A4 Destination MAC Address: 00-C0-4F-8D-93-F2 Ether Type field: IPv4

Frame length : 60 Padding: 000000000000

IP Packet:

Source IP Address: /192.168.1.22 Destination IP Address: /192.168.1.66

IP Version: 4 Protocol Type: TCP

IP header length: 20 bytes

Total IP length: 22

Time to live: 60

Flag: 000

Fragment Offset: 6

TCP Segment:

Source Port: 65520 Destination Port: 0

Sequence Number: 0 Acknowledgment number: 0

TCP Header Length: 0 bytes

Window Size: 0

Flag: other

Urgent Pointer: 0

Option Field: 0

TCP Payload size: 0 bytes

TCP Payload type: other

Data: No payload

Ethernet Frame 249:

Source MAC Address: 00-C0-4F-8D-93-F2 Destination MAC Address: 08-00-20-AB-D4-A4 Ether Type field: IPv4

Frame length : 60 Padding: 000000000000

IP Packet:

Source IP Address: /192.168.1.66 Destination IP Address: /192.168.1.22

IP Version: 4 Protocol Type: TCP

IP header length: 20 bytes

Total IP length: 28

Time to live: 64

Flag: 001

Fragment Offset: 5

TCP Segment:

Source Port: 22783 Destination Port: 61695

Sequence Number: 4196860159 Acknowledgment number: 0

TCP Header Length: 0 bytes

Window Size: 0

Flag: other

Urgent Pointer: 0

Option Field: 0

TCP Payload size: 0 bytes

TCP Payload type: other

Data: No payload

Ethernet Frame 248:

Source MAC Address: 00-C0-4F-8D-93-F2 Destination MAC Address: 08-00-20-AB-D4-A4 Ether Type field: IPv4

Frame length : 60 Padding: 000000000000

IP Packet:

Source IP Address: /192.168.1.66 Destination IP Address: /192.168.1.22

IP Version: 4 Protocol Type: TCP

IP header length: 20 bytes

Total IP length: 28

Time to live: 64

Flag: 001

Fragment Offset: 4

TCP Segment:

Source Port: 22783 Destination Port: 61695

Sequence Number: 1279872597 Acknowledgment number: 0

TCP Header Length: 0 bytes

Window Size: 0

Flag: other

Urgent Pointer: 0

Option Field: 0

TCP Payload size: 0 bytes

TCP Payload type: other

Data: No payload

Ethernet Frame 247:

Source MAC Address: 00-C0-4F-8D-93-F2 Destination MAC Address: 08-00-20-AB-D4-A4 Ether Type field: IPv4

Frame length : 66 Padding:

IP Packet:

Source IP Address: /192.168.1.66 Destination IP Address: /192.168.1.22

IP Version: 4 Protocol Type: TCP

IP header length: 20 bytes

Total IP length: 52

Time to live: 64

Flag: 001

Fragment Offset: 0

TCP Segment:

Source Port: 56788 Destination Port: 23

Sequence Number: 3108926031 Acknowledgment number: 2424181848

TCP Header Length: 32 bytes

Window Size: 5840

Flag: (PSH, ACK)

Urgent Pointer: 0

Option Field: 12

TCP Payload size: 0 bytes

TCP Payload type: Telnet

Data: No payload

Ethernet Frame 246:

Source MAC Address: 00-C0-4F-8D-93-F2 Destination MAC Address: 08-00-20-AB-D4-A4 Ether Type field: IPv4

Frame length : 60 Padding: 000000000000

IP Packet:

Source IP Address: /192.168.1.66 Destination IP Address: /192.168.1.22

IP Version: 4 Protocol Type: TCP

IP header length: 20 bytes

Total IP length: 21

Time to live: 64

Flag: 000

Fragment Offset: 6

TCP Segment:

Source Port: 61440 Destination Port: 0

Sequence Number: 0 Acknowledgment number: 0

TCP Header Length: 0 bytes

Window Size: 0

Flag: other

Urgent Pointer: 0

Option Field: 0

TCP Payload size: 0 bytes

TCP Payload type: other

Data: No payload

Ethernet Frame 250:

Source MAC Address: 08-00-20-AB-D4-A4 Destination MAC Address: 00-C0-4F-8D-93-F2 Ether Type field: IPv4

Frame length : 66 Padding:

IP Packet:

Source IP Address: /192.168.1.22 Destination IP Address: /192.168.1.66

IP Version: 4 Protocol Type: TCP

IP header length: 20 bytes

Total IP length: 52

Time to live: 60

Flag: 000

Fragment Offset: 0

TCP Segment:

Source Port: 23 Destination Port: 56788

Sequence Number: 2424181848 Acknowledgment number: 3108926048

TCP Header Length: 32 bytes

Window Size: 49232

Flag: ACK

Urgent Pointer: 0

Option Field: 12

TCP Payload size: 0 bytes

TCP Payload type: Telnet

Data: No payload

Ethernet Frame 253:

Source MAC Address: 08-00-20-AB-D4-A4 Destination MAC Address: 00-C0-4F-8D-93-F2 Ether Type field: IPv4

Frame length : 60 Padding: 000000000000

IP Packet:

Source IP Address: /192.168.1.22 Destination IP Address: /192.168.1.66

IP Version: 4 Protocol Type: TCP

IP header length: 20 bytes

Total IP length: 28

Time to live: 60

Flag: 001

Fragment Offset: 4

TCP Segment:

Source Port: 3338 Destination Port: 3338

Sequence Number: 1400204879 Acknowledgment number: 0

TCP Header Length: 0 bytes

Window Size: 0

Flag: other

Urgent Pointer: 0

Option Field: 0

TCP Payload size: 0 bytes

TCP Payload type: other

Data: No payload

Ethernet Frame 255:

Source MAC Address: 00-C0-4F-8D-93-F2 Destination MAC Address: 08-00-20-AB-D4-A4 Ether Type field: IPv4

Frame length : 66 Padding:

IP Packet:

Source IP Address: /192.168.1.66 Destination IP Address: /192.168.1.22

IP Version: 4 Protocol Type: TCP

IP header length: 20 bytes

Total IP length: 52

Time to live: 64

Flag: 000

Fragment Offset: 0

TCP Segment:

Source Port: 13 Destination Port: 2573

Sequence Number: 3108926048 Acknowledgment number: 2424181869

TCP Header Length: 32 bytes

Window Size: 5840

Flag: ACK

Urgent Pointer: 0

Option Field: 12

TCP Payload size: 0 bytes

TCP Payload type: Telnet

Data: No payload

Ethernet Frame 252:

Source MAC Address: 08-00-20-AB-D4-A4 Destination MAC Address: 00-C0-4F-8D-93-F2 Ether Type field: IPv4

Frame length : 66 Padding:

IP Packet:

Source IP Address: /192.168.1.22 Destination IP Address: /192.168.1.66

IP Version: 4 Protocol Type: TCP

IP header length: 20 bytes

Total IP length: 52

Time to live: 60

Flag: 001

Fragment Offset: 0

TCP Segment:

Source Port: 13 Destination Port: 2573

Sequence Number: 2424181848 Acknowledgment number: 3108926048

TCP Header Length: 32 bytes

Window Size: 49232

Flag: (PSH, ACK)

Urgent Pointer: 0

Option Field: 12

TCP Payload size: 0 bytes

TCP Payload type: Telnet

Data: No payload

Ethernet Frame 254:

Source MAC Address: 08-00-20-AB-D4-A4 Destination MAC Address: 00-C0-4F-8D-93-F2 Ether Type field: IPv4

Frame length : 60 Padding: 000000000000

IP Packet:

Source IP Address: /192.168.1.22 Destination IP Address: /192.168.1.66

IP Version: 4 Protocol Type: TCP

IP header length: 20 bytes

Total IP length: 25

Time to live: 60

Flag: 000

Fragment Offset: 6

TCP Segment:

Source Port: 13 Destination Port: 2573

Sequence Number: 0 Acknowledgment number: 0

TCP Header Length: 0 bytes

Window Size: 0

Flag: other

Urgent Pointer: 0

Option Field: 0

TCP Payload size: 0 bytes

TCP Payload type: other

Data: No payload

Ethernet Frame 251:

Source MAC Address: 08-00-20-AB-D4-A4 Destination MAC Address: 00-C0-4F-8D-93-F2 Ether Type field: IPv4

Frame length : 60 Padding: 000000000000

IP Packet:

Source IP Address: /192.168.1.22 Destination IP Address: /192.168.1.66

IP Version: 4 Protocol Type: TCP

IP header length: 20 bytes

Total IP length: 28

Time to live: 60

Flag: 001

Fragment Offset: 5

TCP Segment:

Source Port: 3338 Destination Port: 3338

Sequence Number: 957155853 Acknowledgment number: 0

TCP Header Length: 0 bytes

Window Size: 0

Flag: other

Urgent Pointer: 0

Option Field: 0

TCP Payload size: 0 bytes

TCP Payload type: other

Data: No payload

Ethernet Frame 256:

Source MAC Address: 00-C0-4F-8D-93-F2 Destination MAC Address: 08-00-20-AB-D4-A4 Ether Type field: IPv4

Frame length : 66 Padding:

IP Packet:

Source IP Address: /192.168.1.66 Destination IP Address: /192.168.1.22

IP Version: 4 Protocol Type: TCP

IP header length: 20 bytes

Total IP length: 52

Time to live: 64

Flag: 000

Fragment Offset: 0

TCP Segment:

Source Port: 56788 Destination Port: 23

Sequence Number: 3108926048 Acknowledgment number: 2424181878

TCP Header Length: 32 bytes

Window Size: 5840

Flag: ACK

Urgent Pointer: 0

Option Field: 12

TCP Payload size: 0 bytes

TCP Payload type: Telnet

Data: No payload

Ethernet Frame 259:

Source MAC Address: 00-C0-4F-8D-93-F2 Destination MAC Address: 08-00-20-AB-D4-A4 Ether Type field: IPv4

Frame length : 60 Padding: 000000000000

IP Packet:

Source IP Address: /192.168.1.66 Destination IP Address: /192.168.1.22

IP Version: 4 Protocol Type: TCP

IP header length: 20 bytes

Total IP length: 21

Time to live: 64

Flag: 000

Fragment Offset: 5

TCP Segment:

Source Port: 256 Destination Port: 0

Sequence Number: 0 Acknowledgment number: 0

TCP Header Length: 0 bytes

Window Size: 0

Flag: other

Urgent Pointer: 0

Option Field: 0

TCP Payload size: 0 bytes

TCP Payload type: other

Data: No payload

Ethernet Frame 258:

Source MAC Address: 00-C0-4F-8D-93-F2 Destination MAC Address: 08-00-20-AB-D4-A4 Ether Type field: IPv4

Frame length : 60 Padding: 000000000000

IP Packet:

Source IP Address: /192.168.1.66 Destination IP Address: /192.168.1.22

IP Version: 4 Protocol Type: TCP

IP header length: 20 bytes

Total IP length: 28

Time to live: 64

Flag: 001

Fragment Offset: 4

TCP Segment:

Source Port: 256 Destination Port: 0

Sequence Number: 4244897788 Acknowledgment number: 0

TCP Header Length: 0 bytes

Window Size: 0

Flag: other

Urgent Pointer: 0

Option Field: 0

TCP Payload size: 0 bytes

TCP Payload type: other

Data: No payload

Ethernet Frame 257:

Source MAC Address: 00-C0-4F-8D-93-F2 Destination MAC Address: 08-00-20-AB-D4-A4 Ether Type field: IPv4

Frame length : 66 Padding:

IP Packet:

Source IP Address: /192.168.1.66 Destination IP Address: /192.168.1.22

IP Version: 4 Protocol Type: TCP

IP header length: 20 bytes

Total IP length: 52

Time to live: 64

Flag: 001

Fragment Offset: 0

TCP Segment:

Source Port: 256 Destination Port: 0

Sequence Number: 3108926048 Acknowledgment number: 2424181878

TCP Header Length: 32 bytes

Window Size: 5840

Flag: (PSH, ACK)

Urgent Pointer: 0

Option Field: 12

TCP Payload size: 0 bytes

TCP Payload type: Telnet

Data: No payload

Ethernet Frame 260:

Source MAC Address: 08-00-20-AB-D4-A4 Destination MAC Address: 00-C0-4F-8D-93-F2 Ether Type field: IPv4

Frame length : 60 Padding: 000000000000

IP Packet:

Source IP Address: /192.168.1.22 Destination IP Address: /192.168.1.66

IP Version: 4 Protocol Type: TCP

IP header length: 20 bytes

Total IP length: 28

Time to live: 60

Flag: 001

Fragment Offset: 4

TCP Segment:

Source Port: 23 Destination Port: 56788

Sequence Number: 4211343357 Acknowledgment number: 0

TCP Header Length: 0 bytes

Window Size: 0

Flag: other

Urgent Pointer: 0

Option Field: 0

TCP Payload size: 0 bytes

TCP Payload type: other

Data: No payload

Ethernet Frame 262:

Source MAC Address: 08-00-20-AB-D4-A4 Destination MAC Address: 00-C0-4F-8D-93-F2 Ether Type field: IPv4

Frame length : 60 Padding: 000000000000

IP Packet:

Source IP Address: /192.168.1.22 Destination IP Address: /192.168.1.66

IP Version: 4 Protocol Type: TCP

IP header length: 20 bytes

Total IP length: 21

Time to live: 60

Flag: 000

Fragment Offset: 5

TCP Segment:

Source Port: 256 Destination Port: 0

Sequence Number: 0 Acknowledgment number: 0

TCP Header Length: 0 bytes

Window Size: 0

Flag: other

Urgent Pointer: 0

Option Field: 0

TCP Payload size: 0 bytes

TCP Payload type: other

Data: No payload

Ethernet Frame 261:

Source MAC Address: 08-00-20-AB-D4-A4 Destination MAC Address: 00-C0-4F-8D-93-F2 Ether Type field: IPv4

Frame length : 66 Padding:

IP Packet:

Source IP Address: /192.168.1.22 Destination IP Address: /192.168.1.66

IP Version: 4 Protocol Type: TCP

IP header length: 20 bytes

Total IP length: 52

Time to live: 60

Flag: 001

Fragment Offset: 0

TCP Segment:

Source Port: 256 Destination Port: 0

Sequence Number: 2424181869 Acknowledgment number: 3108926048

TCP Header Length: 32 bytes

Window Size: 49232

Flag: (PSH, ACK)

Urgent Pointer: 0

Option Field: 12

TCP Payload size: 0 bytes

TCP Payload type: Telnet

Data: No payload

Ethernet Frame 265:

Source MAC Address: 08-00-20-AB-D4-A4 Destination MAC Address: 00-C0-4F-8D-93-F2 Ether Type field: IPv4

Frame length : 60 Padding: 000000000000

IP Packet:

Source IP Address: /192.168.1.22 Destination IP Address: /192.168.1.66

IP Version: 4 Protocol Type: TCP

IP header length: 20 bytes

Total IP length: 27

Time to live: 60

Flag: 000

Fragment Offset: 4

TCP Segment:

Source Port: 27759 Destination Port: 26473

Sequence Number: 1849303040 Acknowledgment number: 0

TCP Header Length: 0 bytes

Window Size: 0

Flag: other

Urgent Pointer: 0

Option Field: 0

TCP Payload size: 0 bytes

TCP Payload type: other

Data: No payload

Ethernet Frame 266:

Source MAC Address: 08-00-20-AB-D4-A4 Destination MAC Address: 00-C0-4F-8D-93-F2 Ether Type field: IPv4

Frame length : 60 Padding: 000000000000

IP Packet:

Source IP Address: /192.168.1.22 Destination IP Address: /192.168.1.66

IP Version: 4 Protocol Type: TCP

IP header length: 20 bytes

Total IP length: 23

Time to live: 60

Flag: 000

Fragment Offset: 4

TCP Segment:

Source Port: 65534 Destination Port: 256

Sequence Number: 0 Acknowledgment number: 0

TCP Header Length: 0 bytes

Window Size: 0

Flag: other

Urgent Pointer: 0

Option Field: 0

TCP Payload size: 0 bytes

TCP Payload type: other

Data: No payload

Ethernet Frame 263:

Source MAC Address: 08-00-20-AB-D4-A4 Destination MAC Address: 00-C0-4F-8D-93-F2 Ether Type field: IPv4

Frame length : 66 Padding:

IP Packet:

Source IP Address: /192.168.1.22 Destination IP Address: /192.168.1.66

IP Version: 4 Protocol Type: TCP

IP header length: 20 bytes

Total IP length: 52

Time to live: 60

Flag: 001

Fragment Offset: 0

TCP Segment:

Source Port: 27759 Destination Port: 26473

Sequence Number: 2424181881 Acknowledgment number: 3108926057

TCP Header Length: 32 bytes

Window Size: 49232

Flag: (PSH, ACK)

Urgent Pointer: 0

Option Field: 12

TCP Payload size: 0 bytes

TCP Payload type: Telnet

Data: No payload

Ethernet Frame 264:

Source MAC Address: 00-C0-4F-8D-93-F2 Destination MAC Address: 08-00-20-AB-D4-A4 Ether Type field: IPv4

Frame length : 66 Padding:

IP Packet:

Source IP Address: /192.168.1.66 Destination IP Address: /192.168.1.22

IP Version: 4 Protocol Type: TCP

IP header length: 20 bytes

Total IP length: 52

Time to live: 64

Flag: 000

Fragment Offset: 0

TCP Segment:

Source Port: 27759 Destination Port: 26473

Sequence Number: 3108926057 Acknowledgment number: 2424181881

TCP Header Length: 32 bytes

Window Size: 5840

Flag: ACK

Urgent Pointer: 0

Option Field: 12

TCP Payload size: 0 bytes

TCP Payload type: other

Data: No payload

Ethernet Frame 269:

Source MAC Address: 00-C0-4F-8D-93-F2 Destination MAC Address: 08-00-20-AB-D4-A4 Ether Type field: IPv4

Frame length : 66 Padding:

IP Packet:

Source IP Address: /192.168.1.66 Destination IP Address: /192.168.1.22

IP Version: 4 Protocol Type: TCP

IP header length: 20 bytes

Total IP length: 52

Time to live: 64

Flag: 001

Fragment Offset: 0

TCP Segment:

Source Port: 56788 Destination Port: 23

Sequence Number: 3108926057 Acknowledgment number: 2424181888

TCP Header Length: 32 bytes

Window Size: 5840

Flag: (PSH, ACK)

Urgent Pointer: 0

Option Field: 12

TCP Payload size: 0 bytes

TCP Payload type: Telnet

Data: No payload

Ethernet Frame 268:

Source MAC Address: 00-C0-4F-8D-93-F2 Destination MAC Address: 08-00-20-AB-D4-A4 Ether Type field: IPv4

Frame length : 66 Padding:

IP Packet:

Source IP Address: /192.168.1.66 Destination IP Address: /192.168.1.22

IP Version: 4 Protocol Type: TCP

IP header length: 20 bytes

Total IP length: 52

Time to live: 64

Flag: 000

Fragment Offset: 0

TCP Segment:

Source Port: 56788 Destination Port: 23

Sequence Number: 3108926057 Acknowledgment number: 2424181888

TCP Header Length: 32 bytes

Window Size: 5840

Flag: ACK

Urgent Pointer: 0

Option Field: 12

TCP Payload size: 0 bytes

TCP Payload type: Telnet

Data: No payload

Ethernet Frame 267:

Source MAC Address: 08-00-20-AB-D4-A4 Destination MAC Address: 00-C0-4F-8D-93-F2 Ether Type field: IPv4

Frame length : 66 Padding:

IP Packet:

Source IP Address: /192.168.1.22 Destination IP Address: /192.168.1.66

IP Version: 4 Protocol Type: TCP

IP header length: 20 bytes

Total IP length: 52

Time to live: 60

Flag: 001

Fragment Offset: 0

TCP Segment:

Source Port: 23 Destination Port: 56788

Sequence Number: 2424181878 Acknowledgment number: 3108926057

TCP Header Length: 32 bytes

Window Size: 49232

Flag: (PSH, ACK)

Urgent Pointer: 0

Option Field: 12

TCP Payload size: 0 bytes

TCP Payload type: Telnet

Data: No payload

Ethernet Frame 270:

Source MAC Address: 00-C0-4F-8D-93-F2 Destination MAC Address: 08-00-20-AB-D4-A4 Ether Type field: IPv4

Frame length : 60 Padding: 000000000000

IP Packet:

Source IP Address: /192.168.1.66 Destination IP Address: /192.168.1.22

IP Version: 4 Protocol Type: TCP

IP header length: 20 bytes

Total IP length: 28

Time to live: 64

Flag: 000

Fragment Offset: 4

TCP Segment:

Source Port: 56788 Destination Port: 23

Sequence Number: 1882273034 Acknowledgment number: 0

TCP Header Length: 0 bytes

Window Size: 0

Flag: other

Urgent Pointer: 0

Option Field: 0

TCP Payload size: 0 bytes

TCP Payload type: other

Data: No payload

Ethernet Frame 271:

Source MAC Address: 00-C0-4F-8D-93-F2 Destination MAC Address: 08-00-20-AB-D4-A4 Ether Type field: IPv4

Frame length : 66 Padding:

IP Packet:

Source IP Address: /192.168.1.66 Destination IP Address: /192.168.1.22

IP Version: 4 Protocol Type: TCP

IP header length: 20 bytes

Total IP length: 52

Time to live: 64

Flag: 000

Fragment Offset: 0

TCP Segment:

Source Port: 56788 Destination Port: 23

Sequence Number: 3108926065 Acknowledgment number: 2424181897

TCP Header Length: 32 bytes

Window Size: 5840

Flag: ACK

Urgent Pointer: 0

Option Field: 12

TCP Payload size: 0 bytes

TCP Payload type: Telnet

Data: No payload

Ethernet Frame 272:

Source MAC Address: 08-00-20-AB-D4-A4 Destination MAC Address: 00-C0-4F-8D-93-F2 Ether Type field: IPv4

Frame length : 60 Padding: 000000000000

IP Packet:

Source IP Address: /192.168.1.22 Destination IP Address: /192.168.1.66

IP Version: 4 Protocol Type: TCP

IP header length: 20 bytes

Total IP length: 21

Time to live: 60

Flag: 000

Fragment Offset: 5

TCP Segment:

Source Port: 26482 Destination Port: 28533

Sequence Number: 0 Acknowledgment number: 0

TCP Header Length: 0 bytes

Window Size: 0

Flag: other

Urgent Pointer: 0

Option Field: 0

TCP Payload size: 0 bytes

TCP Payload type: other

Data: No payload

Ethernet Frame 273:

Source MAC Address: 08-00-20-AB-D4-A4 Destination MAC Address: 00-C0-4F-8D-93-F2 Ether Type field: IPv4

Frame length : 60 Padding: 000000000000

IP Packet:

Source IP Address: /192.168.1.22 Destination IP Address: /192.168.1.66

IP Version: 4 Protocol Type: TCP

IP header length: 20 bytes

Total IP length: 28

Time to live: 60

Flag: 001

Fragment Offset: 4

TCP Segment:

Source Port: 26482 Destination Port: 28533

Sequence Number: 1882273037 Acknowledgment number: 0

TCP Header Length: 0 bytes

Window Size: 0

Flag: other

Urgent Pointer: 0

Option Field: 0

TCP Payload size: 0 bytes

TCP Payload type: other

Data: No payload

Ethernet Frame 274:

Source MAC Address: 08-00-20-AB-D4-A4 Destination MAC Address: 00-C0-4F-8D-93-F2 Ether Type field: IPv4

Frame length : 66 Padding:

IP Packet:

Source IP Address: /192.168.1.22 Destination IP Address: /192.168.1.66

IP Version: 4 Protocol Type: TCP

IP header length: 20 bytes

Total IP length: 52

Time to live: 60

Flag: 001

Fragment Offset: 0

TCP Segment:

Source Port: 23 Destination Port: 56788

Sequence Number: 2424181888 Acknowledgment number: 3108926065

TCP Header Length: 32 bytes

Window Size: 49232

Flag: (PSH, ACK)

Urgent Pointer: 0

Option Field: 12

TCP Payload size: 0 bytes

TCP Payload type: Telnet

Data: No payload

Ethernet Frame 276:

Source MAC Address: 08-00-20-AB-D4-A4 Destination MAC Address: 00-C0-4F-8D-93-F2 Ether Type field: IPv4

Frame length : 60 Padding: 000000000000

IP Packet:

Source IP Address: /192.168.1.22 Destination IP Address: /192.168.1.66

IP Version: 4 Protocol Type: TCP

IP header length: 20 bytes

Total IP length: 28

Time to live: 60

Flag: 001

Fragment Offset: 4

TCP Segment:

Source Port: 23 Destination Port: 56788

Sequence Number: 2003792484 Acknowledgment number: 0

TCP Header Length: 0 bytes

Window Size: 0

Flag: other

Urgent Pointer: 0

Option Field: 0

TCP Payload size: 0 bytes

TCP Payload type: other

Data: No payload

Ethernet Frame 277:

Source MAC Address: 08-00-20-AB-D4-A4 Destination MAC Address: 00-C0-4F-8D-93-F2 Ether Type field: IPv4

Frame length : 66 Padding:

IP Packet:

Source IP Address: /192.168.1.22 Destination IP Address: /192.168.1.66

IP Version: 4 Protocol Type: TCP

IP header length: 20 bytes

Total IP length: 52

Time to live: 60

Flag: 001

Fragment Offset: 0

TCP Segment:

Source Port: 23 Destination Port: 56788

Sequence Number: 2424181897 Acknowledgment number: 3108926065

TCP Header Length: 32 bytes

Window Size: 49232

Flag: (PSH, ACK)

Urgent Pointer: 0

Option Field: 12

TCP Payload size: 0 bytes

TCP Payload type: Telnet

Data: No payload

Ethernet Frame 275:

Source MAC Address: 08-00-20-AB-D4-A4 Destination MAC Address: 00-C0-4F-8D-93-F2 Ether Type field: IPv4

Frame length : 60 Padding: 000000000000

IP Packet:

Source IP Address: /192.168.1.22 Destination IP Address: /192.168.1.66

IP Version: 4 Protocol Type: TCP

IP header length: 20 bytes

Total IP length: 22

Time to live: 60

Flag: 000

Fragment Offset: 5

TCP Segment:

Source Port: 23 Destination Port: 56788

Sequence Number: 0 Acknowledgment number: 0

TCP Header Length: 0 bytes

Window Size: 0

Flag: other

Urgent Pointer: 0

Option Field: 0

TCP Payload size: 0 bytes

TCP Payload type: other

Data: No payload

Ethernet Frame 278:

Source MAC Address: 00-C0-4F-8D-93-F2 Destination MAC Address: 08-00-20-AB-D4-A4 Ether Type field: IPv4

Frame length : 66 Padding:

IP Packet:

Source IP Address: /192.168.1.66 Destination IP Address: /192.168.1.22

IP Version: 4 Protocol Type: TCP

IP header length: 20 bytes

Total IP length: 52

Time to live: 64

Flag: 001

Fragment Offset: 0

TCP Segment:

Source Port: 56788 Destination Port: 23

Sequence Number: 3108926065 Acknowledgment number: 2424181907

TCP Header Length: 32 bytes

Window Size: 5840

Flag: (PSH, ACK)

Urgent Pointer: 0

Option Field: 12

TCP Payload size: 0 bytes

TCP Payload type: Telnet

Data: No payload

Ethernet Frame 279:

Source MAC Address: 00-C0-4F-8D-93-F2 Destination MAC Address: 08-00-20-AB-D4-A4 Ether Type field: IPv4

Frame length : 66 Padding:

IP Packet:

Source IP Address: /192.168.1.66 Destination IP Address: /192.168.1.22

IP Version: 4 Protocol Type: TCP

IP header length: 20 bytes

Total IP length: 52

Time to live: 64

Flag: 000

Fragment Offset: 0

TCP Segment:

Source Port: 56788 Destination Port: 23

Sequence Number: 3108926065 Acknowledgment number: 2424181907

TCP Header Length: 32 bytes

Window Size: 5840

Flag: ACK

Urgent Pointer: 0

Option Field: 12

TCP Payload size: 0 bytes

TCP Payload type: Telnet

Data: No payload

Ethernet Frame 280:

Source MAC Address: 00-C0-4F-8D-93-F2 Destination MAC Address: 08-00-20-AB-D4-A4 Ether Type field: IPv4

Frame length : 60 Padding: 000000000000

IP Packet:

Source IP Address: /192.168.1.66 Destination IP Address: /192.168.1.22

IP Version: 4 Protocol Type: TCP

IP header length: 20 bytes

Total IP length: 28

Time to live: 64

Flag: 001

Fragment Offset: 4

TCP Segment:

Source Port: 23 Destination Port: 13878

Sequence Number: 825636910 Acknowledgment number: 0

TCP Header Length: 0 bytes

Window Size: 0

Flag: other

Urgent Pointer: 0

Option Field: 0

TCP Payload size: 0 bytes

TCP Payload type: other

Data: No payload

Ethernet Frame 281:

Source MAC Address: 00-C0-4F-8D-93-F2 Destination MAC Address: 08-00-20-AB-D4-A4 Ether Type field: IPv4

Frame length : 60 Padding: 000000000000

IP Packet:

Source IP Address: /192.168.1.66 Destination IP Address: /192.168.1.22

IP Version: 4 Protocol Type: TCP

IP header length: 20 bytes

Total IP length: 25

Time to live: 64

Flag: 000

Fragment Offset: 5

TCP Segment:

Source Port: 23 Destination Port: 13878

Sequence Number: 167772160 Acknowledgment number: 0

TCP Header Length: 0 bytes

Window Size: 0

Flag: other

Urgent Pointer: 0

Option Field: 0

TCP Payload size: 0 bytes

TCP Payload type: other

Data: No payload

Ethernet Frame 282:

Source MAC Address: 08-00-20-AB-D4-A4 Destination MAC Address: 00-C0-4F-8D-93-F2 Ether Type field: IPv4

Frame length : 66 Padding:

IP Packet:

Source IP Address: /192.168.1.22 Destination IP Address: /192.168.1.66

IP Version: 4 Protocol Type: TCP

IP header length: 20 bytes

Total IP length: 52

Time to live: 60

Flag: 001

Fragment Offset: 0

TCP Segment:

Source Port: 23 Destination Port: 13878

Sequence Number: 2424181907 Acknowledgment number: 3108926078

TCP Header Length: 32 bytes

Window Size: 49232

Flag: (PSH, ACK)

Urgent Pointer: 0

Option Field: 12

TCP Payload size: 0 bytes

TCP Payload type: Telnet

Data: No payload

Ethernet Frame 283:

Source MAC Address: 00-C0-4F-8D-93-F2 Destination MAC Address: 08-00-20-AB-D4-A4 Ether Type field: IPv4

Frame length : 66 Padding:

IP Packet:

Source IP Address: /192.168.1.66 Destination IP Address: /192.168.1.22

IP Version: 4 Protocol Type: TCP

IP header length: 20 bytes

Total IP length: 52

Time to live: 64

Flag: 000

Fragment Offset: 0

TCP Segment:

Source Port: 56788 Destination Port: 23

Sequence Number: 3108926078 Acknowledgment number: 2424181909

TCP Header Length: 32 bytes

Window Size: 5840

Flag: ACK

Urgent Pointer: 0

Option Field: 12

TCP Payload size: 0 bytes

TCP Payload type: Telnet

Data: No payload

Ethernet Frame 284:

Source MAC Address: 08-00-20-AB-D4-A4 Destination MAC Address: 00-C0-4F-8D-93-F2 Ether Type field: IPv4

Frame length : 60 Padding: 000000000000

IP Packet:

Source IP Address: /192.168.1.22 Destination IP Address: /192.168.1.66

IP Version: 4 Protocol Type: TCP

IP header length: 20 bytes

Total IP length: 28

Time to live: 60

Flag: 001

Fragment Offset: 4

TCP Segment:

Source Port: 3338 Destination Port: 0

Sequence Number: 543977319 Acknowledgment number: 0

TCP Header Length: 0 bytes

Window Size: 0

Flag: other

Urgent Pointer: 0

Option Field: 0

TCP Payload size: 0 bytes

TCP Payload type: other

Data: No payload

Ethernet Frame 285:

Source MAC Address: 08-00-20-AB-D4-A4 Destination MAC Address: 00-C0-4F-8D-93-F2 Ether Type field: IPv4

Frame length : 60 Padding: 000000000000

IP Packet:

Source IP Address: /192.168.1.22 Destination IP Address: /192.168.1.66

IP Version: 4 Protocol Type: TCP

IP header length: 20 bytes

Total IP length: 22

Time to live: 60

Flag: 000

Fragment Offset: 4

TCP Segment:

Source Port: 3338 Destination Port: 0

Sequence Number: 0 Acknowledgment number: 0

TCP Header Length: 0 bytes

Window Size: 0

Flag: other

Urgent Pointer: 0

Option Field: 0

TCP Payload size: 0 bytes

TCP Payload type: other

Data: No payload

Ethernet Frame 286:

Source MAC Address: 08-00-20-AB-D4-A4 Destination MAC Address: 00-C0-4F-8D-93-F2 Ether Type field: IPv4

Frame length : 60 Padding: 000000000000

IP Packet:

Source IP Address: /192.168.1.22 Destination IP Address: /192.168.1.66

IP Version: 4 Protocol Type: TCP

IP header length: 20 bytes

Total IP length: 28

Time to live: 60

Flag: 001

Fragment Offset: 6

TCP Segment:

Source Port: 19041 Destination Port: 24942

Sequence Number: 825827377 Acknowledgment number: 0

TCP Header Length: 0 bytes

Window Size: 0

Flag: other

Urgent Pointer: 0

Option Field: 0

TCP Payload size: 0 bytes

TCP Payload type: other

Data: No payload

Ethernet Frame 287:

Source MAC Address: 08-00-20-AB-D4-A4 Destination MAC Address: 00-C0-4F-8D-93-F2 Ether Type field: IPv4

Frame length : 60 Padding: 000000000000

IP Packet:

Source IP Address: /192.168.1.22 Destination IP Address: /192.168.1.66

IP Version: 4 Protocol Type: TCP

IP header length: 20 bytes

Total IP length: 28

Time to live: 60

Flag: 001

Fragment Offset: 9

TCP Segment:

Source Port: 29800 Destination Port: 24942

Sequence Number: 1970089575 Acknowledgment number: 0

TCP Header Length: 0 bytes

Window Size: 0

Flag: other

Urgent Pointer: 0

Option Field: 0

TCP Payload size: 0 bytes

TCP Payload type: other

Data: No payload

Ethernet Frame 289:

Source MAC Address: 08-00-20-AB-D4-A4 Destination MAC Address: 00-C0-4F-8D-93-F2 Ether Type field: IPv4

Frame length : 60 Padding: 000000000000

IP Packet:

Source IP Address: /192.168.1.22 Destination IP Address: /192.168.1.66

IP Version: 4 Protocol Type: TCP

IP header length: 20 bytes

Total IP length: 28

Time to live: 60

Flag: 001

Fragment Offset: 7

TCP Segment:

Source Port: 12346 Destination Port: 30064

Sequence Number: 976367904 Acknowledgment number: 0

TCP Header Length: 0 bytes

Window Size: 0

Flag: other

Urgent Pointer: 0

Option Field: 0

TCP Payload size: 0 bytes

TCP Payload type: other

Data: No payload

Ethernet Frame 288:

Source MAC Address: 08-00-20-AB-D4-A4 Destination MAC Address: 00-C0-4F-8D-93-F2 Ether Type field: IPv4

Frame length : 60 Padding: 000000000000

IP Packet:

Source IP Address: /192.168.1.22 Destination IP Address: /192.168.1.66

IP Version: 4 Protocol Type: TCP

IP header length: 20 bytes

Total IP length: 28

Time to live: 60

Flag: 001

Fragment Offset: 8

TCP Segment:

Source Port: 12346 Destination Port: 30064

Sequence Number: 543973742 Acknowledgment number: 0

TCP Header Length: 0 bytes

Window Size: 0

Flag: other

Urgent Pointer: 0

Option Field: 0

TCP Payload size: 0 bytes

TCP Payload type: other

Data: No payload

Ethernet Frame 292:

Source MAC Address: 08-00-20-AB-D4-A4 Destination MAC Address: 00-C0-4F-8D-93-F2 Ether Type field: IPv4

Frame length : 60 Padding: 000000000000

IP Packet:

Source IP Address: /192.168.1.22 Destination IP Address: /192.168.1.66

IP Version: 4 Protocol Type: TCP

IP header length: 20 bytes

Total IP length: 28

Time to live: 60

Flag: 001

Fragment Offset: 5

TCP Segment:

Source Port: 26990 Destination Port: 14880

Sequence Number: 1466262560 Acknowledgment number: 0

TCP Header Length: 0 bytes

Window Size: 0

Flag: other

Urgent Pointer: 0

Option Field: 0

TCP Payload size: 0 bytes

TCP Payload type: other

Data: No payload

Ethernet Frame 291:

Source MAC Address: 08-00-20-AB-D4-A4 Destination MAC Address: 00-C0-4F-8D-93-F2 Ether Type field: IPv4

Frame length : 66 Padding:

IP Packet:

Source IP Address: /192.168.1.22 Destination IP Address: /192.168.1.66

IP Version: 4 Protocol Type: TCP

IP header length: 20 bytes

Total IP length: 52

Time to live: 60

Flag: 001

Fragment Offset: 0

TCP Segment:

Source Port: 23 Destination Port: 56788

Sequence Number: 2424181909 Acknowledgment number: 3108926078

TCP Header Length: 32 bytes

Window Size: 49232

Flag: (PSH, ACK)

Urgent Pointer: 0

Option Field: 12

TCP Payload size: 0 bytes

TCP Payload type: Telnet

Data: No payload

Ethernet Frame 290:

Source MAC Address: 08-00-20-AB-D4-A4 Destination MAC Address: 00-C0-4F-8D-93-F2 Ether Type field: IPv4

Frame length : 60 Padding: 000000000000

IP Packet:

Source IP Address: /192.168.1.22 Destination IP Address: /192.168.1.66

IP Version: 4 Protocol Type: TCP

IP header length: 20 bytes

Total IP length: 26

Time to live: 60

Flag: 000

Fragment Offset: 10

TCP Segment:

Source Port: 23 Destination Port: 56788

Sequence Number: 218759168 Acknowledgment number: 0

TCP Header Length: 0 bytes

Window Size: 0

Flag: other

Urgent Pointer: 0

Option Field: 0

TCP Payload size: 0 bytes

TCP Payload type: other

Data: No payload

Ethernet Frame 293:

Source MAC Address: 08-00-20-AB-D4-A4 Destination MAC Address: 00-C0-4F-8D-93-F2 Ether Type field: IPv4

Frame length : 66 Padding:

IP Packet:

Source IP Address: /192.168.1.22 Destination IP Address: /192.168.1.66

IP Version: 4 Protocol Type: TCP

IP header length: 20 bytes

Total IP length: 52

Time to live: 60

Flag: 001

Fragment Offset: 0

TCP Segment:

Source Port: 56788 Destination Port: 23

Sequence Number: 2424181963 Acknowledgment number: 3108926078

TCP Header Length: 32 bytes

Window Size: 49232

Flag: (PSH, ACK)

Urgent Pointer: 0

Option Field: 12

TCP Payload size: 0 bytes

TCP Payload type: Telnet

Data: No payload

Ethernet Frame 295:

Source MAC Address: 00-C0-4F-8D-93-F2 Destination MAC Address: 08-00-20-AB-D4-A4 Ether Type field: IPv4

Frame length : 66 Padding:

IP Packet:

Source IP Address: /192.168.1.66 Destination IP Address: /192.168.1.22

IP Version: 4 Protocol Type: TCP

IP header length: 20 bytes

Total IP length: 52

Time to live: 64

Flag: 000

Fragment Offset: 0

TCP Segment:

Source Port: 56788 Destination Port: 23

Sequence Number: 3108926078 Acknowledgment number: 2424181963

TCP Header Length: 32 bytes

Window Size: 5840

Flag: ACK

Urgent Pointer: 0

Option Field: 12

TCP Payload size: 0 bytes

TCP Payload type: Telnet

Data: No payload

Ethernet Frame 294:

Source MAC Address: 08-00-20-AB-D4-A4 Destination MAC Address: 00-C0-4F-8D-93-F2 Ether Type field: IPv4

Frame length : 60 Padding: 000000000000

IP Packet:

Source IP Address: /192.168.1.22 Destination IP Address: /192.168.1.66

IP Version: 4 Protocol Type: TCP

IP header length: 20 bytes

Total IP length: 22

Time to live: 60

Flag: 000

Fragment Offset: 4

TCP Segment:

Source Port: 56788 Destination Port: 23

Sequence Number: 0 Acknowledgment number: 0

TCP Header Length: 0 bytes

Window Size: 0

Flag: other

Urgent Pointer: 0

Option Field: 0

TCP Payload size: 0 bytes

TCP Payload type: Telnet

Data: No payload

Ethernet Frame 298:

Source MAC Address: 00-C0-4F-8D-93-F2 Destination MAC Address: 08-00-20-AB-D4-A4 Ether Type field: IPv4

Frame length : 66 Padding:

IP Packet:

Source IP Address: /192.168.1.66 Destination IP Address: /192.168.1.22

IP Version: 4 Protocol Type: TCP

IP header length: 20 bytes

Total IP length: 52

Time to live: 64

Flag: 001

Fragment Offset: 0

TCP Segment:

Source Port: 56788 Destination Port: 23

Sequence Number: 3108926078 Acknowledgment number: 2424181965

TCP Header Length: 32 bytes

Window Size: 5840

Flag: (PSH, ACK)

Urgent Pointer: 0

Option Field: 12

TCP Payload size: 0 bytes

TCP Payload type: Telnet

Data: No payload

Ethernet Frame 297:

Source MAC Address: 00-C0-4F-8D-93-F2 Destination MAC Address: 08-00-20-AB-D4-A4 Ether Type field: IPv4

Frame length : 66 Padding:

IP Packet:

Source IP Address: /192.168.1.66 Destination IP Address: /192.168.1.22

IP Version: 4 Protocol Type: TCP

IP header length: 20 bytes

Total IP length: 52

Time to live: 64

Flag: 000

Fragment Offset: 0

TCP Segment:

Source Port: 56788 Destination Port: 23

Sequence Number: 3108926078 Acknowledgment number: 2424181965

TCP Header Length: 32 bytes

Window Size: 5840

Flag: ACK

Urgent Pointer: 0

Option Field: 12

TCP Payload size: 0 bytes

TCP Payload type: Telnet

Data: No payload

Ethernet Frame 296:

Source MAC Address: 00-C0-4F-8D-93-F2 Destination MAC Address: 08-00-20-AB-D4-A4 Ether Type field: IPv4

Frame length : 60 Padding: 000000000000

IP Packet:

Source IP Address: /192.168.1.66 Destination IP Address: /192.168.1.22

IP Version: 4 Protocol Type: TCP

IP header length: 20 bytes

Total IP length: 28

Time to live: 64

Flag: 000

Fragment Offset: 4

TCP Segment:

Source Port: 56788 Destination Port: 23

Sequence Number: 1953329162 Acknowledgment number: 0

TCP Header Length: 0 bytes

Window Size: 0

Flag: other

Urgent Pointer: 0

Option Field: 0

TCP Payload size: 0 bytes

TCP Payload type: Telnet

Data: No payload

Ethernet Frame 299:

Source MAC Address: 00-C0-4F-8D-93-F2 Destination MAC Address: 08-00-20-AB-D4-A4 Ether Type field: IPv4

Frame length : 66 Padding:

IP Packet:

Source IP Address: /192.168.1.66 Destination IP Address: /192.168.1.22

IP Version: 4 Protocol Type: TCP

IP header length: 20 bytes

Total IP length: 52

Time to live: 64

Flag: 000

Fragment Offset: 0

TCP Segment:

Source Port: 56788 Destination Port: 23

Sequence Number: 3108926086 Acknowledgment number: 2424181974

TCP Header Length: 32 bytes

Window Size: 5840

Flag: ACK

Urgent Pointer: 0

Option Field: 12

TCP Payload size: 0 bytes

TCP Payload type: Telnet

Data: No payload

Ethernet Frame 300:

Source MAC Address: 3C-18-A0-42-CF-27 Destination MAC Address: 01-00-5E-7F-FF-FA Ether Type field: IPv4

Frame length : 216 Padding:

IP Packet:

Source IP Address: /192.168.1.105 Destination IP Address: /239.255.255.250

IP Version: 4 Protocol Type: TCP

IP header length: 20 bytes

Total IP length: 202

Time to live: 1

Flag: 000

Fragment Offset: 0

UDP Datagram.

Source Port: 56538 Destination Port: 1900

UDP Length: 182

UDP Data Length: 174

UDP Data: 4D 2D 53 45 41 52 43 48 20 2A 20 48 54 54 50 2F M-SEARCH \* HTTP/

31 2E 31 0D 0A 48 4F 53 54 3A 20 32 33 39 2E 32 1.1..HOST: 239.2

35 35 2E 32 35 35 2E 32 35 30 3A 31 39 30 30 0D 55.255.250:1900.

0A 4D 41 4E 3A 20 22 73 73 64 70 3A 64 69 73 63 .MAN: "ssdp:disc

6F 76 65 72 22 0D 0A 4D 58 3A 20 31 0D 0A 53 54 over"..MX: 1..ST

3A 20 75 72 6E 3A 64 69 61 6C 2D 6D 75 6C 74 69 : urn:dial-multi

73 63 72 65 65 6E 2D 6F 72 67 3A 73 65 72 76 69 screen-org:servi

63 65 3A 64 69 61 6C 3A 31 0D 0A 55 53 45 52 2D ce:dial:1..USER-

41 47 45 4E 54 3A 20 47 6F 6F 67 6C 65 20 43 68 AGENT: Google Ch

72 6F 6D 65 2F 36 35 2E 30 2E 33 33 32 35 2E 31 rome/65.0.3325.1

38 31 20 57 69 6E 64 6F 77 73 0D 0A 0D 0A 81 Windows....

Ethernet Frame 301:

Source MAC Address: 08-00-20-AB-D4-A4 Destination MAC Address: 00-C0-4F-8D-93-F2 Ether Type field: IPv4

Frame length : 66 Padding:

IP Packet:

Source IP Address: /192.168.1.22 Destination IP Address: /192.168.1.66

IP Version: 4 Protocol Type: TCP

IP header length: 20 bytes

Total IP length: 52

Time to live: 60

Flag: 001

Fragment Offset: 0

TCP Segment:

Source Port: 23 Destination Port: 56788

Sequence Number: 2424181965 Acknowledgment number: 3108926086

TCP Header Length: 32 bytes

Window Size: 49232

Flag: (PSH, ACK)

Urgent Pointer: 0

Option Field: 12

TCP Payload size: 0 bytes

TCP Payload type: Telnet

Data: No payload

Ethernet Frame 304:

Source MAC Address: 08-00-20-AB-D4-A4 Destination MAC Address: 00-C0-4F-8D-93-F2 Ether Type field: IPv4

Frame length : 60 Padding: 000000000000

IP Packet:

Source IP Address: /192.168.1.22 Destination IP Address: /192.168.1.66

IP Version: 4 Protocol Type: TCP

IP header length: 20 bytes

Total IP length: 21

Time to live: 60

Flag: 000

Fragment Offset: 5

TCP Segment:

Source Port: 29793 Destination Port: 30567

Sequence Number: 0 Acknowledgment number: 0

TCP Header Length: 0 bytes

Window Size: 0

Flag: other

Urgent Pointer: 0

Option Field: 0

TCP Payload size: 0 bytes

TCP Payload type: other

Data: No payload

Ethernet Frame 303:

Source MAC Address: 08-00-20-AB-D4-A4 Destination MAC Address: 00-C0-4F-8D-93-F2 Ether Type field: IPv4

Frame length : 60 Padding: 000000000000

IP Packet:

Source IP Address: /192.168.1.22 Destination IP Address: /192.168.1.66

IP Version: 4 Protocol Type: TCP

IP header length: 20 bytes

Total IP length: 28

Time to live: 60

Flag: 001

Fragment Offset: 5

TCP Segment:

Source Port: 29793 Destination Port: 30567

Sequence Number: 1869575200 Acknowledgment number: 0

TCP Header Length: 0 bytes

Window Size: 0

Flag: other

Urgent Pointer: 0

Option Field: 0

TCP Payload size: 0 bytes

TCP Payload type: other

Data: No payload

Ethernet Frame 302:

Source MAC Address: 08-00-20-AB-D4-A4 Destination MAC Address: 00-C0-4F-8D-93-F2 Ether Type field: IPv4

Frame length : 60 Padding: 000000000000

IP Packet:

Source IP Address: /192.168.1.22 Destination IP Address: /192.168.1.66

IP Version: 4 Protocol Type: TCP

IP header length: 20 bytes

Total IP length: 28

Time to live: 60

Flag: 001

Fragment Offset: 8

TCP Segment:

Source Port: 8224 Destination Port: 30567

Sequence Number: 808464432 Acknowledgment number: 0

TCP Header Length: 0 bytes

Window Size: 0

Flag: other

Urgent Pointer: 0

Option Field: 0

TCP Payload size: 0 bytes

TCP Payload type: other

Data: No payload

Ethernet Frame 305:

Source MAC Address: 08-00-20-AB-D4-A4 Destination MAC Address: 00-C0-4F-8D-93-F2 Ether Type field: IPv4

Frame length : 60 Padding: 000000000000

IP Packet:

Source IP Address: /192.168.1.22 Destination IP Address: /192.168.1.66

IP Version: 4 Protocol Type: TCP

IP header length: 20 bytes

Total IP length: 28

Time to live: 60

Flag: 001

Fragment Offset: 4

TCP Segment:

Source Port: 29540 Destination Port: 11884

Sequence Number: 1953329165 Acknowledgment number: 0

TCP Header Length: 0 bytes

Window Size: 0

Flag: other

Urgent Pointer: 0

Option Field: 0

TCP Payload size: 0 bytes

TCP Payload type: other

Data: No payload

Ethernet Frame 306:

Source MAC Address: 08-00-20-AB-D4-A4 Destination MAC Address: 00-C0-4F-8D-93-F2 Ether Type field: IPv4

Frame length : 60 Padding: 000000000000

IP Packet:

Source IP Address: /192.168.1.22 Destination IP Address: /192.168.1.66

IP Version: 4 Protocol Type: TCP

IP header length: 20 bytes

Total IP length: 28

Time to live: 60

Flag: 001

Fragment Offset: 7

TCP Segment:

Source Port: 29540 Destination Port: 11884

Sequence Number: 1868786464 Acknowledgment number: 0

TCP Header Length: 0 bytes

Window Size: 0

Flag: other

Urgent Pointer: 0

Option Field: 0

TCP Payload size: 0 bytes

TCP Payload type: other

Data: No payload

Ethernet Frame 310:

Source MAC Address: 08-00-20-AB-D4-A4 Destination MAC Address: 00-C0-4F-8D-93-F2 Ether Type field: IPv4

Frame length : 60 Padding: 000000000000

IP Packet:

Source IP Address: /192.168.1.22 Destination IP Address: /192.168.1.66

IP Version: 4 Protocol Type: TCP

IP header length: 20 bytes

Total IP length: 28

Time to live: 60

Flag: 001

Fragment Offset: 6

TCP Segment:

Source Port: 8307 Destination Port: 28773

Sequence Number: 1667982713 Acknowledgment number: 0

TCP Header Length: 0 bytes

Window Size: 0

Flag: other

Urgent Pointer: 0

Option Field: 0

TCP Payload size: 0 bytes

TCP Payload type: other

Data: No payload

Ethernet Frame 309:

Source MAC Address: 08-00-20-AB-D4-A4 Destination MAC Address: 00-C0-4F-8D-93-F2 Ether Type field: IPv4

Frame length : 60 Padding: 000000000000

IP Packet:

Source IP Address: /192.168.1.22 Destination IP Address: /192.168.1.66

IP Version: 4 Protocol Type: TCP

IP header length: 20 bytes

Total IP length: 28

Time to live: 60

Flag: 001

Fragment Offset: 4

TCP Segment:

Source Port: 8307 Destination Port: 28773

Sequence Number: 1919312993 Acknowledgment number: 0

TCP Header Length: 0 bytes

Window Size: 0

Flag: other

Urgent Pointer: 0

Option Field: 0

TCP Payload size: 0 bytes

TCP Payload type: other

Data: No payload

Ethernet Frame 308:

Source MAC Address: 08-00-20-AB-D4-A4 Destination MAC Address: 00-C0-4F-8D-93-F2 Ether Type field: IPv4

Frame length : 66 Padding:

IP Packet:

Source IP Address: /192.168.1.22 Destination IP Address: /192.168.1.66

IP Version: 4 Protocol Type: TCP

IP header length: 20 bytes

Total IP length: 52

Time to live: 60

Flag: 001

Fragment Offset: 0

TCP Segment:

Source Port: 23 Destination Port: 56788

Sequence Number: 2424181974 Acknowledgment number: 3108926086

TCP Header Length: 32 bytes

Window Size: 49232

Flag: (PSH, ACK)

Urgent Pointer: 0

Option Field: 12

TCP Payload size: 0 bytes

TCP Payload type: Telnet

Data: No payload

Ethernet Frame 307:

Source MAC Address: 08-00-20-AB-D4-A4 Destination MAC Address: 00-C0-4F-8D-93-F2 Ether Type field: IPv4

Frame length : 60 Padding: 000000000000

IP Packet:

Source IP Address: /192.168.1.22 Destination IP Address: /192.168.1.66

IP Version: 4 Protocol Type: TCP

IP header length: 20 bytes

Total IP length: 26

Time to live: 60

Flag: 000

Fragment Offset: 9

TCP Segment:

Source Port: 12336 Destination Port: 12340

Sequence Number: 218759168 Acknowledgment number: 0

TCP Header Length: 0 bytes

Window Size: 0

Flag: other

Urgent Pointer: 0

Option Field: 0

TCP Payload size: 0 bytes

TCP Payload type: other

Data: No payload

Ethernet Frame 311:

Source MAC Address: 08-00-20-AB-D4-A4 Destination MAC Address: 00-C0-4F-8D-93-F2 Ether Type field: IPv4

Frame length : 66 Padding:

IP Packet:

Source IP Address: /192.168.1.22 Destination IP Address: /192.168.1.66

IP Version: 4 Protocol Type: TCP

IP header length: 20 bytes

Total IP length: 52

Time to live: 60

Flag: 001

Fragment Offset: 0

TCP Segment:

Source Port: 12336 Destination Port: 26416

Sequence Number: 2424182020 Acknowledgment number: 3108926086

TCP Header Length: 32 bytes

Window Size: 49232

Flag: (PSH, ACK)

Urgent Pointer: 0

Option Field: 12

TCP Payload size: 0 bytes

TCP Payload type: Telnet

Data: No payload

Ethernet Frame 312:

Source MAC Address: 08-00-20-AB-D4-A4 Destination MAC Address: 00-C0-4F-8D-93-F2 Ether Type field: IPv4

Frame length : 60 Padding: 000000000000

IP Packet:

Source IP Address: /192.168.1.22 Destination IP Address: /192.168.1.66

IP Version: 4 Protocol Type: TCP

IP header length: 20 bytes

Total IP length: 28

Time to live: 60

Flag: 001

Fragment Offset: 7

TCP Segment:

Source Port: 8311 Destination Port: 26416

Sequence Number: 538976288 Acknowledgment number: 0

TCP Header Length: 0 bytes

Window Size: 0

Flag: other

Urgent Pointer: 0

Option Field: 0

TCP Payload size: 0 bytes

TCP Payload type: other

Data: No payload

Ethernet Frame 313:

Source MAC Address: 08-00-20-AB-D4-A4 Destination MAC Address: 00-C0-4F-8D-93-F2 Ether Type field: IPv4

Frame length : 60 Padding: 000000000000

IP Packet:

Source IP Address: /192.168.1.22 Destination IP Address: /192.168.1.66

IP Version: 4 Protocol Type: TCP

IP header length: 20 bytes

Total IP length: 28

Time to live: 60

Flag: 001

Fragment Offset: 6

TCP Segment:

Source Port: 8311 Destination Port: 26416

Sequence Number: 808464432 Acknowledgment number: 0

TCP Header Length: 0 bytes

Window Size: 0

Flag: other

Urgent Pointer: 0

Option Field: 0

TCP Payload size: 0 bytes

TCP Payload type: other

Data: No payload

Ethernet Frame 314:

Source MAC Address: 08-00-20-AB-D4-A4 Destination MAC Address: 00-C0-4F-8D-93-F2 Ether Type field: IPv4

Frame length : 60 Padding: 000000000000

IP Packet:

Source IP Address: /192.168.1.22 Destination IP Address: /192.168.1.66

IP Version: 4 Protocol Type: TCP

IP header length: 20 bytes

Total IP length: 28

Time to live: 60

Flag: 001

Fragment Offset: 4

TCP Segment:

Source Port: 28530 Destination Port: 25193

Sequence Number: 1949135471 Acknowledgment number: 0

TCP Header Length: 0 bytes

Window Size: 0

Flag: other

Urgent Pointer: 0

Option Field: 0

TCP Payload size: 0 bytes

TCP Payload type: other

Data: No payload

Ethernet Frame 315:

Source MAC Address: 08-00-20-AB-D4-A4 Destination MAC Address: 00-C0-4F-8D-93-F2 Ether Type field: IPv4

Frame length : 60 Padding: 000000000000

IP Packet:

Source IP Address: /192.168.1.22 Destination IP Address: /192.168.1.66

IP Version: 4 Protocol Type: TCP

IP header length: 20 bytes

Total IP length: 28

Time to live: 60

Flag: 001

Fragment Offset: 8

TCP Segment:

Source Port: 8224 Destination Port: 30567

Sequence Number: 808464432 Acknowledgment number: 0

TCP Header Length: 0 bytes

Window Size: 0

Flag: other

Urgent Pointer: 0

Option Field: 0

TCP Payload size: 0 bytes

TCP Payload type: other

Data: No payload

Ethernet Frame 316:

Source MAC Address: 08-00-20-AB-D4-A4 Destination MAC Address: 00-C0-4F-8D-93-F2 Ether Type field: IPv4

Frame length : 60 Padding: 000000000000

IP Packet:

Source IP Address: /192.168.1.22 Destination IP Address: /192.168.1.66

IP Version: 4 Protocol Type: TCP

IP header length: 20 bytes

Total IP length: 28

Time to live: 60

Flag: 001

Fragment Offset: 5

TCP Segment:

Source Port: 28532 Destination Port: 30567

Sequence Number: 538976288 Acknowledgment number: 0

TCP Header Length: 0 bytes

Window Size: 0

Flag: other

Urgent Pointer: 0

Option Field: 0

TCP Payload size: 0 bytes

TCP Payload type: other

Data: No payload

Ethernet Frame 317:

Source MAC Address: 08-00-20-AB-D4-A4 Destination MAC Address: 00-C0-4F-8D-93-F2 Ether Type field: IPv4

Frame length : 60 Padding: 000000000000

IP Packet:

Source IP Address: /192.168.1.22 Destination IP Address: /192.168.1.66

IP Version: 4 Protocol Type: TCP

IP header length: 20 bytes

Total IP length: 26

Time to live: 60

Flag: 000

Fragment Offset: 9

TCP Segment:

Source Port: 12336 Destination Port: 12341

Sequence Number: 218759168 Acknowledgment number: 0

TCP Header Length: 0 bytes

Window Size: 0

Flag: other

Urgent Pointer: 0

Option Field: 0

TCP Payload size: 0 bytes

TCP Payload type: other

Data: No payload

Ethernet Frame 319:

Source MAC Address: 00-C0-4F-8D-93-F2 Destination MAC Address: 08-00-20-AB-D4-A4 Ether Type field: IPv4

Frame length : 66 Padding:

IP Packet:

Source IP Address: /192.168.1.66 Destination IP Address: /192.168.1.22

IP Version: 4 Protocol Type: TCP

IP header length: 20 bytes

Total IP length: 52

Time to live: 64

Flag: 000

Fragment Offset: 0

TCP Segment:

Source Port: 56788 Destination Port: 23

Sequence Number: 3108926086 Acknowledgment number: 2424182066

TCP Header Length: 32 bytes

Window Size: 5840

Flag: ACK

Urgent Pointer: 0

Option Field: 12

TCP Payload size: 0 bytes

TCP Payload type: Telnet

Data: No payload

Ethernet Frame 318:

Source MAC Address: 00-C0-4F-8D-93-F2 Destination MAC Address: 08-00-20-AB-D4-A4 Ether Type field: IPv4

Frame length : 66 Padding:

IP Packet:

Source IP Address: /192.168.1.66 Destination IP Address: /192.168.1.22

IP Version: 4 Protocol Type: TCP

IP header length: 20 bytes

Total IP length: 52

Time to live: 64

Flag: 000

Fragment Offset: 0

TCP Segment:

Source Port: 56788 Destination Port: 23

Sequence Number: 3108926086 Acknowledgment number: 2424182020

TCP Header Length: 32 bytes

Window Size: 5840

Flag: ACK

Urgent Pointer: 0

Option Field: 12

TCP Payload size: 0 bytes

TCP Payload type: Telnet

Data: No payload

Ethernet Frame 320:

Source MAC Address: 08-00-20-AB-D4-A4 Destination MAC Address: 00-C0-4F-8D-93-F2 Ether Type field: IPv4

Frame length : 66 Padding:

IP Packet:

Source IP Address: /192.168.1.22 Destination IP Address: /192.168.1.66

IP Version: 4 Protocol Type: TCP

IP header length: 20 bytes

Total IP length: 52

Time to live: 60

Flag: 001

Fragment Offset: 0

TCP Segment:

Source Port: 23 Destination Port: 56788

Sequence Number: 2424182066 Acknowledgment number: 3108926086

TCP Header Length: 32 bytes

Window Size: 49232

Flag: (PSH, ACK)

Urgent Pointer: 0

Option Field: 12

TCP Payload size: 0 bytes

TCP Payload type: Telnet

Data: No payload

Ethernet Frame 321:

Source MAC Address: 08-00-20-AB-D4-A4 Destination MAC Address: 00-C0-4F-8D-93-F2 Ether Type field: IPv4

Frame length : 60 Padding: 000000000000

IP Packet:

Source IP Address: /192.168.1.22 Destination IP Address: /192.168.1.66

IP Version: 4 Protocol Type: TCP

IP header length: 20 bytes

Total IP length: 22

Time to live: 60

Flag: 000

Fragment Offset: 4

TCP Segment:

Source Port: 9248 Destination Port: 0

Sequence Number: 0 Acknowledgment number: 0

TCP Header Length: 0 bytes

Window Size: 0

Flag: other

Urgent Pointer: 0

Option Field: 0

TCP Payload size: 0 bytes

TCP Payload type: other

Data: No payload

Ethernet Frame 322:

Source MAC Address: 00-C0-4F-8D-93-F2 Destination MAC Address: 08-00-20-AB-D4-A4 Ether Type field: IPv4

Frame length : 66 Padding:

IP Packet:

Source IP Address: /192.168.1.66 Destination IP Address: /192.168.1.22

IP Version: 4 Protocol Type: TCP

IP header length: 20 bytes

Total IP length: 52

Time to live: 64

Flag: 000

Fragment Offset: 0

TCP Segment:

Source Port: 56788 Destination Port: 23

Sequence Number: 3108926086 Acknowledgment number: 2424182068

TCP Header Length: 32 bytes

Window Size: 5840

Flag: ACK

Urgent Pointer: 0

Option Field: 12

TCP Payload size: 0 bytes

TCP Payload type: Telnet

Data: No payload

Ethernet Frame 323:

Source MAC Address: 00-C0-4F-8D-93-F2 Destination MAC Address: 08-00-20-AB-D4-A4 Ether Type field: IPv4

Frame length : 66 Padding:

IP Packet:

Source IP Address: /192.168.1.66 Destination IP Address: /192.168.1.22

IP Version: 4 Protocol Type: TCP

IP header length: 20 bytes

Total IP length: 52

Time to live: 64

Flag: 000

Fragment Offset: 0

TCP Segment:

Source Port: 56788 Destination Port: 23

Sequence Number: 3108926086 Acknowledgment number: 2424182068

TCP Header Length: 32 bytes

Window Size: 5840

Flag: (FIN, ACK)

Urgent Pointer: 0

Option Field: 12

TCP Payload size: 0 bytes

TCP Payload type: Telnet

Data: No payload

Ethernet Frame 324:

Source MAC Address: 08-00-20-AB-D4-A4 Destination MAC Address: 00-C0-4F-8D-93-F2 Ether Type field: IPv4

Frame length : 66 Padding:

IP Packet:

Source IP Address: /192.168.1.22 Destination IP Address: /192.168.1.66

IP Version: 4 Protocol Type: TCP

IP header length: 20 bytes

Total IP length: 52

Time to live: 60

Flag: 000

Fragment Offset: 0

TCP Segment:

Source Port: 23 Destination Port: 56788

Sequence Number: 2424182068 Acknowledgment number: 3108926087

TCP Header Length: 32 bytes

Window Size: 49232

Flag: ACK

Urgent Pointer: 0

Option Field: 12

TCP Payload size: 0 bytes

TCP Payload type: Telnet

Data: No payload

C:\Users\Prakash Thapa\Desktop\Spring 2018\NetworkSecurity\Assignments\Project1>